WebSmart Switch ECS2100-10T/10P/10PE/28T/28P/28PP/28PP

V2/10P-RAI

***Phase 3 Firmware Version 3.1.1.243***

**INTRODUCTION:**

The ECS2100-10T/10P/10PE is a Gigabit Ethernet Layer 2 switch featuring 8 ports 10/100/1000 ports, and 2 Gigabit Ethernet SFP (Small Form Factor Pluggable) uplink ports.

The ECS2100-28T/28P/28PP/28PPv2 is a Gigabit Ethernet Layer 2 switch featuring 24 ports 10/100/1000 ports, and 4 Gigabit Ethernet SFP (Small Form Factor Pluggable) uplink ports.

The ECS2100-10T/10P/10PE/28T/28P/28PP/28PPv2 is ideal for operator to deploy SMB network providing download/upload 10/100/1000Mbps high speed for triple play service.

|  |
| --- |
| **It is recommended that one thoroughly review this release notes prior to the installation or upgrade of this product.** |

**Firmware Specification:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Status** | **Version No.** | **Type** | **Release Date** |
| EIT/NTC test Version | 3.1.1.243 | Git DEV\_ECS4100\_Phase3 (2024/07/01) | 2024/07/01 |
| EIT | 3.1.0.242 | Git DEV\_ECS4100\_Phase3 (2024/05/27)  Add image profile license | 2024/05/27 |
| NTC test version | 1.2.3.45 | Git Master (2024/03/06) | 2024/03/06 |
| EIT test Version | 1.2.3.44 | Git Master (2024/02/22)  uboot进版到V0.2.1.5 | 2024/02/22 |
| EIT/NTC test Version | 1.2.3.43 | Git Master (2023/04/07)  uboot进版到V0.2.1.4 | 2023/06/28 |
| EIT/NTC test Version | 1.2.3.42 | Git Master (2023/02/14) | 2023/02/16 |
| EIT test Version | 1.2.3.41 | Git Master (2023/01/13) | 2023/01/13 |
| NTC test Version | 1.2.3.40 | Git Master (2022/11/17) | 2022/11/11 |
| NTC test Version | 1.2.3.39 | Git Master (2022/7/4) | 2022/7/14 |
| EIT test Version | 1.2.3.38 | Git Master (2022/7/4) | 2022/7/4 |
| NTC test Version | 1.2.3.37 | Git Master (2022/3/31) | 2022/3/31 |
| EIT/NTC test Version | 1.2.3.36 | Git Master (2022/2/17) | 2022/2/17 |
| EIT test Version | 1.2.3.35 | Git Master (2021/12/10) | 2021/12/10 |
| EIT test Version | 1.2.2.34 | Git Master (2021/10/18) | 2021/10/18 |
| EIT/NTC test Version | 1.2.2.33 | Git Master (2021/07/22) | 2021/07/22 |
| EIT/NTC test Version | 1.2.2.32 | Git Master (2021/03/18) | 2021/03/18 |
| EIT/NTC test Version/MP version | 1.2.2.31 | Git Master (2020/10/16 bugfix and enhance smart-pair,cloude management web ui) | 2020/10/16 |
| EIT/NTC test Version/MP version | 1.2.2.30 | Git Master (2020/09/18 5PM) | 2020/09/18 |
| EIT/NTC test Version | 1.2.2.29 | Git Master (2020/09/01 5PM) | 2020/09/01 |
| EIT test Version | 1.2.2.28 | Git Master (2020/08/25 5PM) | 2020/08/25 |
| NTC Test Version | 1.2.2.27 | Patched on V26 | 2020/01/16 |
| TS test Version | 1.2.2.26 | Patched on V25 | 2019/12/31 |
| TS test Version | 1.2.2.25 | Patched on V24 | 2019/07/29 |
| TS test Version | 1.2.2.24 | Git Master (2019/01/30 5PM) | 2019/03/07 |
| TS test Version | 1.2.2.23 | Git Master (2018/12/12 4PM) | 2018/12/19 |
| NTC/TS test Version | 1.2.2.22 | Git Master (2018/11/09 8PM) | 2018/11/12 |
| TS test Version (Cancel) | 1.2.2.21 | Git Master (2018/10/05 3PM) | 2018/10/9 |
| EIT test Version | 1.2.2.20 | CC: EC\_VOB main (2018/9/4 9:30AM) | 2018/9/4 |
| EIT test Version | 1.2.2.19 | CC: EC\_VOB main (2018/8/28 9:30AM) | 2018/8/28 |
| EIT test Version (Cancel) | 1.2.2.18 | CC: EC\_VOB main (2018/8/20 9:30AM) | 2018/8/20 |
| EIT test Version | 1.2.2.17 | CC: EC\_VOB main (2018/6/29 2:00PM) | 2018/6/29 |
| EIT test Version (Cancel) | 1.2.2.16 | CC: EC\_VOB main (2018/6/20 9:30AM) | 2018/6/20 |
| EIT test Version | 1.2.2.15 | CC: EC\_VOB main (2018/3/21 1:30PM) | 2018/3/21 |
| EIT test Version | 1.2.2.14 | CC: EC\_VOB main (2018/3/20 1:30PM) | 2018/3/20 |
| EIT test Version | 1.2.2.13 | CC: EC\_VOB main (2018/3/6 1:30PM) | 2018/3/6 |
| EIT test Version | 1.2.2.12 | CC: EC\_VOB main (2018/1/16 1:30PM) | 2018/1/16 |
| EIT test Version | 1.2.2.11 | CC: EC\_VOB main (2017/12/11 1:30PM) | 2017/12/11 |
| EIT test Version | 1.2.2.10 | CC: EC\_VOB main (2017/10/27) | 2017/10/27 |
| EIT test Version | 1.2.2.9 | CC: EC\_VOB main (2017/8/15 9:30AM) | 2017/8/15 |
| EIT test Version | 1.2.2.8 | CC: EC\_VOB main (2017/7/7 9:30AM) | 2017/7/7 |
| EIT test Version | 1.2.2.7 | Based on 1.2.2.5 + 00699 + 00704 fix only. | 2017/7/5 |
| EIT test Version | 1.2.2.6 | CC: EC\_VOB main (2017/6/23 9:30AM) | 2017/6/23 |
| EIT test Version | 1.2.2.5 | CC: EC\_VOB main (2017/4/11 16:30PM) | 2017/4/11 |
| EIT test Version | 1.2.2.1 | CC: EC\_VOB main (2017/1/12 13:30PM) | 2017/1/12 |
| EIT test Version | 1.2.2.0 | All the same as V1.2.1.7 and just modify the version number | 2016/12/28 |
| EIT test Version | 1.2.1.7 | CC: EC\_VOB main (2016/12/16 9:30AM) | 2016/12/16 |
| EIT Test Version | 1.2.1.6 | CC: EC\_VOB main (2016/11/30 9:30AM) | 2016/11/30 |
| EIT Test Version | 1.2.1.5 | CC: EC\_VOB main (2016/11/24 9:30AM) | 2016/11/24 |
| EIT Test Version | 1.2.1.4 | CC: EC\_VOB main (2016/11/14 1:00PM) | 2016/11/14 |
| EIT Test Version | 1.2.1.3 | CC: EC\_VOB main (2016/11/1 9:30AM) | 2016/11/1 |
| EIT Test Version | 1.2.1.2 | CC: EC\_VOB main (2016/10/7 1:30PM) From this version, change the runtime’s header. | 2016/10/7 |
| EIT Test Version | 1.2.1.1 | CC: EC\_VOB main (2016/10/4 9:30AM) | 2016/10/5 |
| EIT Test Version | 1.2.1.0 | CC: EC\_VOB main (2016/8/25 9:30AM)  Must use the loader version after V0.1.1.8(include) | 2016/8/25 |
| EIT Test Version | 1.2.0.8 | CC: EC\_VOB main (2016/8/5 1:30PM) | 2016/8/5 |
| EIT Test Version | 1.2.0.7 | CC: EC\_VOB main (2016/7/29 9:30AM) | 2016/7/29 |
| EIT Test Version | 1.2.0.6 | CC: EC\_VOB main (2016/7/14 9:30AM) | 2016/7/15 |
| EIT Test Version | 1.2.0.4 | CC: EC\_VOB main (2016/7/5 9:30AM) | 2016/7/6 |
| EIT Test Version | 1.2.0.3 | CC: EC\_VOB main (2016/5/18 3:30PM) | 2016/5/19 |
| EIT Test Version | 1.2.0.2 | CC: EC\_VOB main (2016/5/2 9:30AM) | 2016/5/3 |
| EIT Test Version | 1.1.2.4 | Based on V1.1.2.3 + enhance ECS2000-28PP-00513 only. | 2016/3/30 |
| EIT Test Version | 1.1.2.3 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2016/3/25 3:00PM) | 2016/3/35 |
| EIT Test Version | 1.1.2.2 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2016/3/3 9:30AM) | 2016/3/3 |
| EIT Test Version | 1.1.2.1 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2016/1/22 9:30AM) | 2016/1/22 |
| NTC Test Version / MP version | 1.1.2.0 | The same as 1.1.1.37 and just change the version number. | 2016/1/5 |
| NTC Test Version | 1.1.1.37 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2016/1/4 9:30AM) | 2016/1/4 |
| NTC Test Version | 1.1.1.36 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/12/21 9:30AM) | 2015/12/21 |
| NTC Test Version | 1.1.1.34 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/12/17 9:30AM) | 2015/12/17 |
| NTC Test Version | 1.1.1.33 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/12/10 9:30AM) | 2015/12/10 |
| NTC Test Version | 1.1.1.32 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/12/04 9:30AM) | 2015/12/04 |
| NTC Test Version | 1.1.1.31 | Based on V1.1.1.30 + fix 00390, 00404, 00405 | 2015/11/30 |
| NTC Test Version | 1.1.1.30 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/11/27 9:30AM) | 2015/11/27 |
| NTC Test Version | 1.1.1.28 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/11/12 4:00PM) | 2015/11/12 |
| NTC Test Version | 1.1.1.27 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/11/6 9:30AM) | 2015/11/6 |
| NTC Test Version | 1.1.1.26 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/10/30 11:00PM) | 2015/10/30 |
| NTC Test Version | 1.1.1.25 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/10/21 4:00PM) | 2015/10/25 |
| NTC Test Version | 1.1.1.24 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/10/21 9:30AM) | 2015/10/21 |
| NTC Test Version | 1.1.1.23 | Based on V1.1.1.22 + ECS2000-28PP-00259 fix | 2015/10/20 |
| NTC Test Version | 1.1.1.22 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/10/16 17:00AM) | 2015/10/16 |
| NTC Test Version | 1.1.1.21 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/10/16 10:00AM) | 2015/10/16 |
| NTC Test Version | 1.1.1.20 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/10/13 10:00AM) | 2015/10/13 |
| NTC Test Version | 1.1.1.13 | Based on V1.1.1.12 + ECS2000-28PP-00254 fix | 2015/10/5 |
| NTC Test Version(PilotRun) | 1.1.1.12 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/9/30 10:00AM) | 2015/9/30 |
| NTC Test Version | 1.1.1.10 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/9/22 2:00PM) | 2015/9/22 |
| NTC Test Version | 1.1.1.9 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/9/15 9:30AM) | 2015/9/15 |
| NTC Test Version | 1.1.1.7 | CC: EC\_VOB main(2015/9/7 9:30AM) | 2015/9/7 |
| RD Test Version | 1.1.1.6 | CC: EC\_VOB main(2015/9/1 11:00AM) | 2015/9/1 |
| RD Test Version | 1.1.1.5 | CC: EC\_VOB main(2015/8/25 10:00AM) | 2015/8/25 |
| RD Test Version | 1.1.1.2 | CC: EC\_VOB main(2015/8/19 10:00AM) | 2015/8/19 |
| RD Test Version | 1.1.1.1 | CC: EC\_VOB main(2015/8/11 1:30PM) | 2015/8/11 |
| NTC Test Version | 1.1.1.0 | CC: EC\_VOB main(2015/7/27 9:30PM) | 2015/7/27 |

**LOADER:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Status** | **Version No.** | **Type** | **Release Date** |
| Testing Version | 0.2.1.4 | CC: EC\_VOB main  (2023/08/02 9:30AM) | 2023/08/02 |
| Testing Version | 0.2.1.3 | CC: EC\_VOB main (2023/04/07 9:30AM) | 2023/06/28 |
| Testing Version | 0.2.1.2 | CC: EC\_VOB main (2016/10/4 9:30AM) | 2021/12/10 |
| Testing Version | 0.2.1.1 | CC: EC\_VOB main (2016/10/4 9:30AM) | 2016/10/5 |
| Testing Version | 0.1.1.8 | CC: EC\_VOB main (2016/8/25 9:30AM)  MUST use the runtime version after V1.2.1.0(include) | 2016/8/25 |
| Testing Version | 0.1.1.7 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2016/7/26 9:30AM) | 2016/7/26 |
| Testing Version | 0.1.1.6 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/12/10 9:30AM) | 2015/12/10 |
| Testing Version | 0.1.1.5 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/12/04 9:30AM) | 2015/12/04 |
| Testing Version | 0.1.1.3 | CC: EC\_VOB ES4626F-SW-FLF-38\_ECS2100\_V1.1.1.7\_Ph1\_branch (2015/11/6 9:30AM) | 2015/11/6 |
| Testing Version | 0.1.0.0 | Init  CC: EC\_VOB main(2015/7/27 9:30PM) | 2015/7/27 |

**HARDware compatibility:**

ALL

**BootPROM compatibility:**

ALL

**Network Management Software Support:**

|  |  |  |
| --- | --- | --- |
| **NMS Platform** | **Version No.** | **Module No.** |
| TBD |  |  |

If you install this image, you may not have control of all of the latest features of this product until the next version(s) of network management software. Please review the software release notes for your specific network management platform for details.

**SUPPORTED FUNCTIONALITY:**

Please see the ECS2100-28PP\_Phase1\_FeatureList\_20150701.xlsx

**Installation and Configuration Notes:**

In general, the ECS2100 **Switch** will be shipped to you pre-configured with this version of firmware. If you would like to upgrade an existing ECS2100 **Switch,** please follow the TFTP download instructions that are included with your firmware image upgrade kit.

**Firmware Changes and Enhancements:**

**The following Known Issues have been fixed in this release of firmware.**

**Loader V0.1.0.0**

|  |  |  |
| --- | --- | --- |
| 1 | Init | Init |

**Runtime V1.1.1.0**

|  |  |  |
| --- | --- | --- |
| 1 | None | None |

**modifications:**

**Loader V0.2.1.5**

|  |  |  |
| --- | --- | --- |
| 1 | 1. ECS2100EC-298 | 1. [ECS2100] adjust amplitude value of PHY RTL8218D in uboot to make eye diagram better |

**Loader V0.2.1.4**

|  |  |  |
| --- | --- | --- |
| 1 | 1. [ECS2100EC-227](https://jira.accton.com:8443/browse/ECS2100EC-227) | 1. ECS2100\_28PP will reboot automatically after diag test and then boot from runtime |

**Loader V0.2.1.3**

|  |  |  |
| --- | --- | --- |
| 1 | ECS2100EC-156 | ECS2100 changes PHY from 8218B to 8218D, uboot should be compatible to the two PHYs |

**Loader V0.2.1.2**

|  |  |  |
| --- | --- | --- |
| 1 | 1. [ECS2100EC-47](https://jira.accton.com:8443/browse/ECS2100EC-47) | [enhance] Support 28PPv2(BID 8) |

**Loader V0.2.1.1**

|  |  |  |
| --- | --- | --- |
| 1 | ECS2000-28PP-00621 | [enhance] [uboot] accept the new header of runtime |

**Loader V0.1.1.8**

|  |  |  |
| --- | --- | --- |
| 1 | ECS2000-28PP-00539 | dut autoreboot when setting boot system opcode from 1.2.0.3 after autoupgrade |
| 2 | ECS2000-28PP-00610 | System: Kernel panic - not syncing: Fatal exception in interrupt when "Flash programming started." is running after delete op |

**Loader V0.1.1.7**

|  |  |  |
| --- | --- | --- |
| 1 | ECS2000-28PP-00581 | [enhance][uboot] support new model ECS2100-10P-RAI |

**Loader V0.1.1.6**

|  |  |  |
| --- | --- | --- |
| 1 | ECS2000-28PP-00309 | PoE: (10P) DUT can't bootup success after connect 8 PDs.   * Disable PoE by default on uboot. |
| 2 | ECS2000-28PP-00448 | [loader] correct the display of dram size |

**Loader V0.1.1.5**

|  |  |  |
| --- | --- | --- |
| 1 | ECS2000-28PP-00317 | [uboot] remove the chip info message from uboot |

**Loader V0.1.1.4**

|  |  |  |
| --- | --- | --- |
| 1 | ECS2000-28PP-00403 | [u-boot] internal loopback not working on 10P device |

**Loader V0.1.1.3**

|  |  |  |
| --- | --- | --- |
| 1 | ECS2000-28PP-00317 | [uboot] remove the chip info message from uboot |

**Loader V0.1.1.2**

|  |  |
| --- | --- |
| 1 | Correct the short-key to enter the u-boot backdoor. |

**Loader V0.1.1.1**

|  |  |
| --- | --- |
| 1 | Support 10T/10PE/10P |

**Loader V0.1.0.0**

|  |  |
| --- | --- |
| 1 | Init Version |

**Runtime V3.1.1.243, Loader 0.2.1.5**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-346 | Customer request to support ZTP default enable on ECS2100. |
|  | ECS2100EC-348 | formal license can not work |

**Runtime V3.1.0.242, Loader 0.2.1.5**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-341 | Profile license can not work for ECS2100 phase3 |
|  | ECS2100EC-336 | [ECS2100-10P] SSH public key authentication. |
|  | ECS2100EC-332 | Web\_Help: HTTPS's help page doesn't describe "HTTP/HTTPS Timeout" item. |
|  | ECS2100EC-267 | 2100 & 2110 Phase3 add Function profile license 。 |
|  | ECS2100EC-276 | Fine tune the image-profile behavior on ECS2100\_Phase3 |
|  | ECS2100EC-270 | snmp-server notify-filter not working for phase3 |

**Runtime V1.2.3.45, Loader 0.2.1.5**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-323 | [SNMP-0020, 0030] add the third snmp community failed |

**Runtime V1.2.3.44, Loader 0.2.1.5**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2100EC-28 | DUT can't reply ICMP timestamp request |
| 2 | ECS2100EC-54 | SYSLOG-0090:no wartmstart syslog |
| 3 | ECS2100EC-113 | [2110\_mibx.json] CPU Guard MAX Threshold is not 500 |
| 4 | ECS2100EC-115 | [IPv4-RemotePing-0260] Level1-5261 DUT doesn't reply ICMP TimeStamp Request |
| 5 | ECS2100EC-132 | [IPv4-RemotePing-0260] ECS2110 DUT doesn't reply ICMP TimeStamp Request |
| 6 | ECS2100EC-140 | [SYSLOG-0090] ECS2110, DUT can not send "System warmStart notification" syslog |
| 7 | ECS2100EC-158 | [IPv4-RemotePing-0260] ECS2100, DUT doesn't reply ICMP TimeStamp Request |
| 8 | ECS2100EC-174 | [SYSLOG-0090] ECS2100, DUT doesn't send "System warmStart notification" syslog when reboot |
| 9 | ECS2100EC-208 | Static Route: After we add and delete some static routes, it cannot create maximum 32 routes on DUT. |
| 10 | ECS2100EC-209 | MIB: Failed to get and set the object "netConfigEntry". |
| 11 | ECS2100EC-222 | [CPU-Guard-0010 ~ CPU-Guard-0060] The cpuGuardHighWatermark of mibx.json is incorrect |
| 12 | ECS2100EC-224 | [CPU guard] MIN\_cpuGuardHighWatermark should be 40, not 20 |
| 13 | ECS2100EC-248 | [ECS2100-10P] SSH public key authentication |
| 14 | ECS2100EC-262 | snmp-server notify-filter not working |
| 15 | ECS2100EC-299 | [ECS2100-10P] About HTTPS Timeout(master) yes |
| 16 | ECS2100EC-229 | ECS2100-28PP vulnerability issues yes |
| 17 | ECS2100EC-298 | [ECS2100] adjust amplitude value of PHY RTL8218D in uboot to make eye diagram better yes. |

**Runtime V1.2.3.43, Loader 0.2.1.4**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-156 | ECS2100 changes PHY from 8218B to 8218D, uboot should be compatible to the two PHYs yes |
|  | ECS2100EC-166 | DHCP Relay: DUT accept invalid DHCP relay setting with network\_ID and itself IP. |
|  | ECS2100EC-168 | WEB: Failed to enter into Help page. yes |
|  | ECS2100EC-175 | [SSHv2-8010, 8100, 8110] ECS2100 SSHv2 always generate key if key is empty yes |
|  | ECS2100EC-176 | LLDP: After we reset this lldp notify interval from maximum field value, DUT cannot send out notify trap message. Yes. |
|  | ECS2100EC-177 | LLDP: Save this lldp setting of Trunk; leave port from trunk, it cannot transmit and receiving lldp. yes |
|  | ECS2100EC-178 | Voice VLAN: After we add invalid zero OUI MAC, DUT reject add any OUI MAC. Yes. |
|  | ECS2100EC-180 | WEB: This maximum static route number is incorrect in Help page; include ECS2100-28T and ECS2110-26T. yes |
|  | [ECS2100EC-227](https://jira.accton.com:8443/browse/ECS2100EC-227) | ECS2100\_28PP will reboot automatically after diag test and then boot from runtime yes |

**Runtime V1.2.3.42, Loader 0.2.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS4100EC-343 | ARP packet duplicate issue. |
|  | ECS2100EC-154 | Enhancement: After reboot, SSH host-key will automatically generated if the host-key is not exsit. |
|  | [ECS2100EC-53](https://jira.accton.com:8443/browse/ECS2100EC-53) | UserAuth: The CLI will froze when login the DUT via tacacs+ authentication, but the tacacs+ service does not exist. or key error. |
|  | ECS2100EC-108 | Disable tsl 1.0 because a security breach was detected |
|  | [ECS2100EC-121](https://jira.accton.com:8443/browse/ECS2100EC-121) | [SSHv2-8080] Level1-5261 SSHv2 seem no support 3DES, AES(128, 192 and 256) |
|  | ECS4100EC\_452 | DHCPv6 Relay: DUT does not reject to set dhcpv6 relay setting as ipv6 address of vlan1 not defined. |
|  | ECS4100EC\_453 | DHCPv6 Relay: After we change DHCPv6 relay destination address to multicast-all; DUT cannot send out RelayForw packets. |
|  | ECS4100EC\_454 | DHCPv6 Relay: DUT does not reject to set reserved ipv6 address as relay destination address. |

**Runtime V1.2.3.41, Loader 0.2.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-141 | MGMTD: there will be a lot of logs like "Reject SNMP 127.0.0.1" when enabe mgmtd. |
|  | ECS2100EC-142 | Web\_Help: Help page of DHCP Server is empty. |
|  | ECS2100EC-143 | CLI: CLI shows debug messages when webUI timeout. |
|  | ECS2100EC-145 | DHCP-Server: CLI doesn't show status of DHCP Server and DHCP pool. |
|  | ECS2100EC-146 | DHCP-Server: Client ID can not be set correctly in WebUI. |
|  | ECS2100EC-147 | DHCP-Server: client-identifier is useless. |
|  | ECS2100EC-149 | CLONE - MGMTD: there will be a lot of logs like "Reject SNMP 127.0.0.1" when enabe mgmtd. |

**Runtime V1.2.3.40, Loader 0.2.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS4100EC-319 | HTTP-HTTPS:the idie time will reset automatic, the session can no logout |
|  | ECS4100EC-295 | runtime backdoor and Linux shell can access via telnet and SSH |
|  | ECS4100EC-326 | Disable tsl 1.0 because a security breach was detected |
|  | ECS2100EC-128 | Enhance DHCP server |

**Runtime V1.2.3.39, Loader 0.2.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-96 | There is an error when copy file to running(2100-10T) |

**Runtime V1.2.3.38, Loader 0.2.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-95 | 2100 support "ip dhcp snooping max-number filter-only" like 4100 |
|  | ECS2100EC-92 | 2100 support banner |
|  | ECS2100EC-89 | POE MCU soft version is wrong(28PPv2) |
|  | ECS2100EC-88 | POE Led is still lights when port can not provide power to PD(28PPv2) |
|  | ECS2100EC-87 | Interface can not provide power when return port's maximun allocation to default(28PPv2) |

**Runtime V1.2.3.37, Loader 0.2.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-83 | The port provides power when POE is disable |
|  | ECS2100EC-84 | The time range can not work with POE |
|  | ECS2100EC-85 | DUT provides poer exceeding configured maximux allocation power |

**Runtime V1.2.3.36, Loader 0.2.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | [ECS2100EC-75](https://jira.accton.com:8443/browse/ECS2100EC-47) | Support 28PPv2 TI POE Solution |
|  | ECS2100EC-64 | The command "show power inline status" is lost in show tech-support |

**Runtime V1.2.3.35, Loader 0.2.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | [ECS2100EC-47](https://jira.accton.com:8443/browse/ECS2100EC-47) | Support 28PPv2(RTL8218D phy module) |

**Runtime V1.2.2.34, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-63 | SNTP Server can be set with hostname in WEB but cli mode can't |
|  | ECS4100EC-254 | Mib file,memory unit should be Bytes |
|  | ECS2100EC-62 | ECS2100 support bid for 2100-28PPv2 |
|  | ECS2100EC-61 | Cumulative mgmtd updates and fixes:  19924: remove VLAN membership prior to deletion [All models]  19557: Register switch with static IP cannot finish the synchronization [All models]  18109: add system date retrieval from SNMP [All models] |
|  | 1. [ECS2100EC-60](https://jira.accton.com:8443/browse/ECS2100EC-60) | Show tech-support ：some items are missing |
|  | ECS4100EC-250 | command "ip http authentication aaa exec-authorization" won't be show in running-config |

**Runtime V1.2.2.33, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS4100EC-246 | ARP table no timeout |
|  | ECS4100EC-242 | Switch save configuration during keep sending Syslog trap. the switch will hang and trigger the watchdog |
|  | ECS4100EC-243 | If setting "Authorization exec default" without tacas+/radius server. The user privilege level will be 0 |
|  | ECS2100EC-44 | Disable openssl ssl2/ssl3 function |
|  | ECS4100EC-238 | Huawei and EC switches can not telnet to each other |
|  | ECS2100EC-48 | ecCloud agent (mgmtd) has to write routes into config file and reboot the switch. Switch reboot is not desired, takes long time. |
|  | ECS4100EC-7 | DAI doesn't work after the switch reboot |
|  | ECS4100EC-237 | Optimization "ip arp inspection vlan" search method to prevent trigger Watchdog XFER\_TD and CLI\_GROUP |
|  | ECS4100EC-228 | When switch lost connect with tacacs+ server can setting config without tacas+ server authorizztion |
|  | ECS2100EC-46 | Cumulative mgmtd release to ECS4100 and ECS2100 series |
|  | ECS2100EC-45 | 2100 add backdoor command to CLI, and Tech-Support display |

**Runtime V1.2.2.32, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-39 | Mdns/Smart-pair cause loop |
|  | ECS2100EC-42 | Dhcp-snooping/Smart-pair cause loop |
|  | ECS4100EC-206 | After reload dut, mdns no normal work |
|  | ECS4100EC-178 | 4100mib has wrong word case |
|  | ECS4100EC-94 | 1QVLAN: DUT doesn't delete vlan range as VLAN status is rspan. |
|  | ECS4100EC-193 | Disable mDNS, packet still trap to CPU porting from ECS4100-144 |
|  | ECS2100EC-35 | 2100 not support exclude-vlan,the web interface should be removed |

**Runtime V1.2.2.31, Loader 0.2.1.1**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | EPR | | Headline |  |
|  | | ECS4100EC-160 | Exclude-vlan and cloud-management webhelp has error |  |
|  | | ECS4100EC-159 | WebHelp:Exclude-vlan and cloud-management:some setting ranges are wrong |  |
|  | | ECS4100EC-157 | ECS4100 Exclude-vlan and cloud management no webhelp |  |
|  | ECS4100EC-154 | | Web：cloud management page error |  |
|  | ECS4100EC-128 | | DUT only sends 88 NS when set dad attempts sets to 600. |  |
|  | ECS4100EC-131 | | IPv6-AddrConfig: DUT uses wrong MTU to segment packets. |  |
|  | ECS4100EC-151 | | (Enhancement) Add cloud management page in web GUI |  |
|  | ECS2100EC-32 | | (Enhancement)ECS2100 support SMART-PAIR |  |
|  | ECS4100EC-127 | | 1QVLAN: DUT cannot save ipv6 address setting on non-default vlan. |  |
|  | ECS4100EC-134 | | configure mstp cause console print error message |  |
|  | ECS4100EC-133 | | Ingress packet queue(dev\_nicdrv) is suspend & dhcp snp packet cause tx memory leakage |  |
|  | ECS2100EC-15 | | only 4 snmp-server host can be created |  |

**Runtime V1.2.2.30, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-24 | Syslog: Got "succeeded" when "Failed to create new configuration" |
|  | ECS2100EC-29 | SNMP:It's only allower to create 4 not 5 hosts |
|  | ECS2100EC-31 | fix complie error for lan.c |

**Runtime V1.2.2.29, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS4100EC-88 | RADIUS-Acct:The DUT would hang when process of radius accounting |
|  | ECS4100EC-83 | DUT stuck after delete/recreate ip interface and then show ip interface |
|  | ECS4100EC-86 | save cofigstuck for tens minutes and then reboot auto when save config the second time |
|  | ECS4100EC-81 | SNMP: only three snmp community is allowed |
|  | ECS4100EC-82 | SNMP: snmp-server user add failed when add two private snmp user |

**Runtime V1.2.2.28, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2100EC-14 | update new license and update cloud mgmt file |
|  | ECS2100EC-12 | [Enhancement]Radsec function for TLS over TCP |
|  | ECS4100EC-73 | SW Watchdog Timeout due to thread GVRP\_GROUP(Porting from ECS4100EC-63 to ECS4100\_master) |
|  | ECS4100EC-18 | [MSTP] configure mstp cause console print error message. |
|  | ECS4100EC-2 / ECS2100EC-8 | Add IgniteNet cloud management daemon (mgmtd) on 10 selected models:  ECS4100-12T, ECS4100-28T, ECS4100-28P, ECS2100-10P, ECS2100-28PP, ECS2100-28P, ECS2100-10T, ECS2100-28T, ECS4100-12PH, ECS2100-52T.  To be consistent with current EdgeCore switches line, the Cloud management will be disabled by default. Customers would enable Cloud themselves.  Requires increased BIX file upload buffer (i.e. intermediate firmware for upgrade to Cloud managed one).  It was also decided to merge Called-Station-Id commit into this very ticket. |
|  | ECS4100EC-3 | IP Source Guard is filtering PPPoE |
|  | ECS4100-52T-00677 | Configure logging command failed in provisioning |

**Runtime V1.2.2.27, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | 1. [ECS2100EC-7](https://jira.edge-core.com:8443/browse/ECS2100EC-7) (Jira) | Linux Kernel version display problem with "show version" command. |

**Runtime V1.2.2.26, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  |  | [Enhancement] Support default DHCP mode and Initial IP address. |
|  | ECS4100-52T-00649 | [NTP server] When the switch reboot and check configuration provision will occur "Fail to set NTP server xxxxx”. |
|  | ECS4100-52T-00660 | [IGMP] When the first IGMP query is received, manually remove the IGMP VLAN on the port will trigger an exception. |
|  | ECS2000-28PP-01047 | HTTP-Download Config and get old config. |
|  |  |  |

**Runtime V1.2.2.25, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2000-28PP-01050 | ECS2100-28PP does not provide power to a specific PD (IP phone - SAMSUNG SMT-i2205D w/ old firmware version). |

**Runtime V1.2.2.24, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
|  | ECS2000-28PP-01027 | MIB: fileCopyServerInetAddressType description misses the ‘ipv6(2)’ type.  *=> Modified MIB file only (LAST-UPDATED "201903080000Z")* |
|  | ECS4100-52T-00463 | MIB: new traps for sfpInsertTrap/sfpRemoveTrap, Syslog as well  *=> Modified MIB file only (LAST-UPDATED "201903120000Z")* |
|  | ECS4100-52T-00468 | MIB: new traps for sFlowEnableTrap/sFlowDisableTrap, Syslog as well  *=> Modified MIB file only (LAST-UPDATED "201903120000Z")* |
|  | | |
|  | EPR | Headline |
| 1 | ECS2000-28PP-01025 | Continus pings would suddenly get no responses, however, will automatically recover (in 4.5min) at all times |
| 2 | ECS2000-28PP-01028 | SW\_WDT will be triggered (SNMP\_TD task exception) when SNMP retrieves ARP ACL name having 18 and more chars. |
| 3 | ECS4100-52T-00590 | SNMP coldstart/warmstart traps carry invalid IPv6 Loopback address (::1) in the Source IP address. |
| 4 | ECS4100-52T-00609 | Fails to add/delete static mac address via SNMP, however, works well via CLI. *(Occurs in ECS2100 V1.2.2.21~1.2.2.23)* |
| 5 | ECS4100-52T-00614 | SNMP: DAI mode cannot be changed via SNMP daiVlanArpAclStatus. |
| 6 | ECS4100-52T-00588 | Invalid SSHv2 key type (DSA) can be copied to DUT. |
|  |  |  |
| **V1.2.2.12** | | |
|  | ECS2000-28PP-00955 | Ingress filtering does not work after DHCP snooping is enabled. |
|  | Simba-Common-00226 | Switch still learns the MAC address when a receive port does not join that VLAN and its ingress filtering is enabled. |

**Runtime V1.2.2.23, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00874 | If vlan interface enables dhcp and v6 autoconfig, auto upgrade could not find new image |
| 2 | ECS2000-28PP-00895 | Use vlan 4094, can’t autoupgrade ... Monitoring |
| 3 | ECS2000-28PP-00941 | plug in any device will learn on voice vlan and will not age out |
| 4 | ECS2000-28PP-00971 | Vlan IP is delivering by DHCP. Execute "ip dhcp dynamic-provision",No reaction for a while and the device will reboot by WDT |
| ECS2000-28PP-00984 | Console will freeze while executing "copy startup-config (w/ ‘lldp med-location civic-addr‘ settings) to running-config". |
| 5 | ECS2000-28PP-00989 | IGMPSNP: Statically registered group cannot be saved successfully. |
| 6 | ECS2000-28PP-00994 | Index element `vlanDot1qTunnelPortIndex' must have a range restriction. |
| 7 | ECS4100-52T-00551 | [Enhance] SSH supports CTR cipher - upgrade to OpenSSHv7.8p1. |
| ECS4100-52T-00564 | The SFTP feature does not work with IPv6 |
| ECS2000-28PP-00981 | ECS2100-series SSH key exchange protocol is obsolete |
| 8 | ECS4100-52T-00568 | [Enhance] Configurable mgmt. IPv6 address with prefix length up to 126. |
| 9 | ECS4100-52T-00574 | Dropped is the last one of fragmented UDP packets when DHCP snooping is enabled. |

**Runtime V1.2.2.22, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00939 | ip phone cannot join back to voice vlan when ip changed |
| 2 | ECS2000-28PP-00944 | [ALAXALA] The STP loopback detection fails after port shutdown / no shutdown |
| 3 | ECS2000-28PP-00945 | Customized(Non-Std) LLDP broadcast packets (DA: FFFFFFFFFFFF & EtherType: 88CC) cannot be flooding to other ports |
| 4 | ECS2000-28PP-00956  ECS2000-28PP-00962 | [ALAXALA] If to enable IGMP snooping plus querier , the console will hang after setting the VLAN suspend after 5 minutes  [ALAXALA] console locked issue and suddenly reboot by reconfiguring L3 Interface. |
| 5 | ECS2000-28PP-00980 | Switch will warm-start when repeatedly retrieve/release DHCP IP (lease time: 60s) (WDT issue in V22b) |
| 6 | ECS2000-28PP-00985 | [Enhance] Kernel immediately dumps the exception messages on the console. |
| 7 | ECS4100-52T-00540 | If dynamic-provision configuration include dynamic-provision setting again, it will let the function to loop |
| 8 | ECS4100-52T-00571 | [Enhancement] SW WatchDog monitor GVRP\_GROUP |

**Runtime V1.2.2.21, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00878 | [alaxala]We test oid .1.3.6.1.2.1.4.22 then display error |
| 2 | ECS2000-28PP-00933 | [Enhancement] Support to download exception log and watchdog log. |
| 3 | ECS2000-28PP-00950 | NTP server cannot be deleted if set in WEB, however, CLI works well. |
| 4 | ECS2000-28PP-00957 | (MSTP\_issue)MST configuration of spanning-tree is deleted by device after reboot in v1.2.2.20 |
| 5 | ECS4100-52T-00552 | NTP: support to add or delete NTP IPv4/IPv6/hostname servers in SNMP private MIB |
| 6 | ECS2000-28PP-00886 | The WebGUI over Chrome may be not correctly rendering while logging on the switch repeatedly. (no such WebGUI issue over Firefox) |

**Runtime V1.2.2.20, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00877 | [Alaxala] One of vlans request ip, it will let other vlan request at the same time. |
| 2 | ECS2000-28PP-00907 | [Alaxala]The lifetime of the IPv6 address shows wrong |
| 3 | ECS2000-28PP-00908 | [Alaxala] suspend vlan send dhcp discover |
| 4 | ECS2000-28PP-00913 | [MLDSNP] when added a static mrouter port that the switch will not sent out the report by proxy-reporting. |
| 5 | ECS2000-28PP-00914 | [IGMPSNP] "dynamic" mrouter-forward-mode will forward multicast traffic to the another mrouter port directly. |
| 6 | ECS2000-28PP-00919 | [MLDSNP] switch will removed the MLD entry when it received another MLD Query(lower IP address). |
| 7 | ECS2000-28PP-00922 | [MLDSNP] After switch received the MLDv1 Query then it will start to send abnormal MLD Query |
| 8 | ECS2000-28PP-00923. | port security traffic block |

**Runtime V1.2.2.19, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| ~~1~~ | ~~ECS2000-28PP-00878~~ | ~~[alaxala]We test oid .1.3.6.1.2.1.4.22 then display error~~ |
| 2 | ECS2000-28PP-00887 | ZTP can’t autorun. |
| 3 | ECS2000-28PP-00894 | [Alaxala] MAC ACL with time-range(2rules) could not work well for the counter setting |
| 4 | ECS2000-28PP-00898 | In the source guard function with DHCP snooping linkage, part of the source IP address assigned by DHCP becomes Block |
| 5 | ECS2000-28PP-00902 | [Alaxala]After enable the proxy-reporting of IGMP/MLD,the general query didn't flood to all of ports |
| 6 | ECS2000-28PP-00904 | [Alexala] when the "mrouter-forward-mode" is dynamic, the client bellowing static mrouter port isn't in group table |
| 7 | ECS2000-28PP-00905 | Time-Range configuration could not be deleted. |
| 8 | ECS2000-28PP-00911 | [Alaxala] MAC ACL(3rules) with time-range with counter then bind a port, but counter can’t work |
| 9 | ECS2000-28PP-00912 | [Alaxala] Specific arrangement of MAC ACL binding to port by counter , it will let other MAC ACL counter not to work . |
| 10 | Simba-Common-00270. | ZTP can’t autorun. |
| 11 | Simba-Common-00271. | [alaxala][Alaxala] When the share key is over to 48 , we will face watchdog reboot. |

**Runtime V1.2.2.18, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00880 | [Alaxala] Set the snmp version 3 inform, we will face exception |
| 2 | ECS2000-28PP-00883 | [Alaxala] We receive snmpinform then show run, then freeze |
| 3 | ECS2000-28PP-00884 | [Alaxala] authorization exec didn't work well. |
| 4 | ECS2000-28PP-00885 | [alaxala] When the port 1 is trunking port, the "Statisitcs" in GUI will be crash |
| 5 | ECS2000-28PP-00888 | [Alaxala] When we want to set "clock timezone-predefined" by telnet with tab selective, switch will have exception happened. |
| 6 | ECS2000-28PP-00890 | [alaxala] We can display full ACE in GUI for HW counter |
| 7 | ECS2000-28PP-00891 | [alaxala][Alaxala] When the share key is over to 48 , we will face watchdog reboot. |
| 8 | ECS2000-28PP-00892 | [Alaxala]Static Mac-address-table entry won't work on lacp interface after reboot |
| 9 | ECS2000-28PP-00893 | [Alaxala]we can set the to history command to port-channel , but we can't remove it via port-channel interface. |
| 10 | ECS2000-28PP-00896 | Cannot obtain the statistic from WebUI when ACL name to be TCAM full is set to interface. |
| 11 | ECS2000-28PP-00897 | [Alaxala] Command "Clear ipv6 mld snooping groups dynamic" not work |
| 12 | ECS2000-28PP-00900 | [Alaxala] IPv6 ACL can't work well for the source-port destination-port filter |
| 13 | ECS2000-28PP-00901. | STP state will flapping (non-fwd/fwd) when switch received the SyncE packet. |
| 14 | ECS2000-28PP-00903 | [Alaxala ]If the IGMP entries is full, only one client can join to multicast stream well. |
| 15 | ECS2000-28PP-00906. | Can't trigger the swSmtpConnFailure trap. |
| 16 | ECS2000-28PP-00910. | When we want to set "clock timezone-predefined" by telnet, then switch crash. |
| 17 | Simba-Common-00261. | STP state will flapping (non-fwd/fwd) when switch received the SyncE packet. |
| 18 | Simba-Common-00262. | Can't trigger the swSmtpConnFailure trap. |
| 19 | Simba-Common-00263. | WebUI display white screen when apply ACL counter more than 10 ACE |
| 20 | Simba-Common-00264. | [Alaxala] Set the snmp version 3 inform, we will face exception |
| 21 | Simba-Common-00266. | When we want to set "clock timezone-predefined" by telnet, then switch crash. |
| 22 | ECS4100-52T-00434 | This project did not support stitck mac. But this epr change the port security display. Ignore the port channel. |

**Runtime V1.2.2.17, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00881 | AutoUpgrade-0070: error message will pop-up when set ECS2100\_V1.2.2.16.bix to be boot opcode |
| 2 | Simba-Common-00260 | Building libxslt library will fail in cloud server |

**Runtime V1.2.2.16 (Cancel), Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00646 | 802.1X-DACL: The ACL rule can not binding on the port when re-create the ACL rule. |
| 2 | ECS2000-28PP-00847 | RIP: After disable/enable vlan, the statistic value always display 750251720 on "show ip protocol rip" |
| 3 | ECS2000-28PP-00848 | After reboot LAG not calculate on MSTP (Random) |
| 4 | ECS2000-28PP-00849 | After reboot LAG not calculate on MSTP |
| 5 | ECS2000-28PP-00854. | Default configure each interface will be set to "ethernet cfm port-enable" |
| 6 | ECS2000-28PP-00863 | OSPF can specify to delete route information via WebUI |
| 7 | ECS2000-28PP-00864 | LA instantaneous interruption occurred when copy running-config to startup-config |
| 8 | ECS2000-28PP-00866 | switch send out untagged report when enabled MLD snooping |
| 9 | ECS2000-28PP-00869 | No command to remove time range rule |
| 10 | ECS2000-28PP-00870 | After we create an ACL and binding to port with counter, the counter function will failed with increasing the ace to the ACL |
| 11 | ECS2000-28PP-00871 | In "show running", we should remove partner mode setting if we didn't write this config |
| 12 | ECS2000-28PP-00872. | After kill WTDOG\_PROC, show log ram is incorrect |
| 13 | ECS4100-52T-00176 | system name was changed when configure interface vlan ip address |
| 14 | Simba-Common-00133. | SNTP: Timezone is EU, summer time doesn't end at the last sunday of October every year |
| 15 | Simba-Common-00221. | TACACS+Acct-0080:Interim value and Accounting Stop value not find in Accounting log |
| 16 | Simba-Common-00222. | Fail to telnet EC switch(ECS4120) from Cisco device |
| 17 | Simba-Common-00229. | LLDP web:LLDP remote port/trunk "port id" information display in web is not correct |
| 18 | Simba-Common-00242. | After disable then enable vlan on Web, vlan interface link down |
| 19 | Simba-Common-00249. | STP Alternate port does not discard VLAN tagged BPDU packets |

**Runtime V1.2.2.15, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00795 | WebMultiLanguage: Some WebHelp is different from "English" and "簡體中文" about "系統>時間". |
| 2 | ECS2000-28PP-00852 | incorrect trunk members in web page. |
| 3 | ECS2000-28PP-00840 | Correct simple chinese web page, web help page. (only correct some epr. Others will handle by itself' epr.) this build for ECS2000-28PP-00795. |

**Runtime V1.2.2.14, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00703 | 50 mac-address remained in mac table even if clear all mac table. |
| 2 | ECS2000-28PP-00731 | Web:RIP: No helper Web page for RIP. |
| 3 | ECS2000-28PP-00793 | WebMultiLanguage: "GMRP" information "系統>性能" shall be removed from WebHelp when it's set to "簡體中文" |
| 4 | ECS2000-28PP-00800 | WebHelp: There is no baudrate 57600 on WebHelp description. |
| 5 | ECS2000-28PP-00802 | WebHelp: The value of CPU Guard is wrong. (50-500 => 50-300) |
| 6 | ECS2000-28PP-00806 | WEB: DUT should support L3-Relay chinese description in Help page. |
| 7 | ECS2000-28PP-00808 | WebHelp: Please intergrate WebHelp about History page. |
| 8 | ECS2000-28PP-00818 | PortTrunk: The translation between web page and help are different. |
| 9 | ECS2000-28PP-00819 | Web: Help page of Storm Control is wrong. |
| 10 | ECS2000-28PP-00822 | Web: Help page of time range is blank. |
| 11 | ECS2000-28PP-00827 | IGMP-SNP: The IGMP forwarding priority need to be removed from web help. |
| 12 | ECS2000-28PP-00828 | IGMP-SNP: The default IGMP filter mode in web help is incorrect. |
| 13 | ECS2000-28PP-00840 | Correct simple chinese web page, web help page. (only correct some epr. Need next version.) |
| 14 | ECS2000-28PP-00842 | After delete vlan on Web, ip address loss on this vlan |
| 15 | ECS2000-28PP-00844 | After disable then enable vlan on Web, vlan interface link down |
| 16 | ~~ECS2000-28PP-00852~~ | ~~incorrect trunk members in web page. (verify fail in this version)~~ |
| 17 | Simba-Common-00238. | MVR: MVR-0210 will cause console stop response |
| 18 | Simba-Common-00243. | WEB: DUT should display correct L2/L3 Relay description in WEB page. |
| 19 | Simba-Common-00244. | DHCP Relay: DUT should support to switch this L2/L3 Relay by WEB. |

**Runtime V1.2.2.13, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00747. | Link state of LACP trunk member port changes between up and down repeatedly |
| 2 | ECS2000-28PP-00791 | WebMultiLanguage: "CoS to Queue"&"DSCP to Queue" should be renamed to "CoS到Queue"&"DSCP到Queue" when set it to 簡體中文. |
| 3 | ECS2000-28PP-00794 | WebMultiLanguage: SFTP description is lost on "系統/文件" WebHelp. |
| 4 | ECS2000-28PP-00801 | WebHelp: The value of "靜默時間範圍" shall be "1-65535" not "0-65535" on "簡體中文WebHelp. |
| 5 | ECS2000-28PP-00803 | WebHelp: Please integrate WebHelp about HH:MM:DD for "System>Reset" & "系統>重啟. |
| 6 | ECS2000-28PP-00807 | WebHelp: Suggest to modify "統計/圖表" 可"統計或圖表" on "簡體中文WebHelp. |
| 7 | ECS2000-28PP-00810 | WebHelp: Please remove "(Range: 25-28)" from "Interface > Port > Transceiver" because it's single image |
| 8 | ECS2000-28PP-00814 | WebHelp: RSPAN session range shall be 1-3. |
| 9 | ECS2000-28PP-00820 | PortTrunk: The translation of history mode are different between web page and help. |
| 10 | ECS2000-28PP-00824 | CoS: The default queue mode is incorrect in help page. |
| 11 | ECS2000-28PP-00832. | SNMPWALK but get error about sysResourceMgt |
| 12 | ECS2000-28PP-00839. | [Enhancement]SFP EEPROM/DDM/Measured info no clear after SFP removed. |
| 13 | ECS2000-28PP-00840 | Correct simple chinese web page, web help page. (only correct some epr. Need next version.) |
| 14 | ECS2000-28PP-00841. | MVR: MVR-0210 will cause console stop response (ECS2100 did not have MVR. But this epr modify the igmpsnp code) |
| 15 | ECS2000-28PP-00845 | [Web] Help page do not have guide for "Routing Protocol" |
| 16 | ECS2000-28PP-00846 | [Web] RIP: Network cannot show |
| 17 | ECS2000-28PP-00850 | After reboot static MAC of LAG disappear |
| 18 | ECS2000-28PP-00851 | [enhance] update the web help page (1.2.2.9) |
| 19 | ECS2110-26T-00145 | DHCPV6 Relay: DUT suould support to configure DHCPV6 Relay setting through WEB. |
| 20 | Simba-Common-00235. | switch forward all LLDP packets when dot1q enabled globally |
| 21 | Simba-Common-00236. | [Enhancement]SFP EEPROM/DDM/Measured info no clear after SFP removed. |
| 22 | Simba-Common-00237. | Write "reload in" command in configure file make switch stuck. |
| 23 | Simba-Common-00239. | After reboot static MAC of LAG disappear |
| 24 | Simba-Common-00240. | [enhance] Use HW watchdog to monitor SW watchdog |

**Runtime V1.2.2.12, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00736 | conflict of diffserv and routing |
| 2 | ECS2000-28PP-00768 | Web help page freeze |
| 3 | ECS2000-28PP-00783. | Failed to set the TACACS+ server for aaa accounting dot1x. |
| 4 | ECS2000-28PP-00784. | RateLimit: kbps shall be renamed to Kbps on CLI &WebUI. |
| 5 | ECS2000-28PP-00788. | change spanning-tree mode will make the traffic stop. |
| 6 | ECS2000-28PP-00831 | [Enhancement] CLI dynamic command |
| 7 | ECS4100-52T-00299 | ECS4100 (28T/28P-ITUS) Support for reset button |
| 8 | Simba-Common-00220. | Europe summer time end date is incorrect |
| 9 | Simba-Common-00223. | Failed to set the TACACS+ server for aaa accounting dot1x. |
| 10 | Simba-Common-00225. | change spanning-tree mode will make the traffic stop. |
| 11 | Simba-Common-00228. | sflow sample packet doesn't include IPv4 information. |
| 12 | Simba-Common-00232. | [Enhancement] Support read Total/Dynamic/Static mac count by SNMP |
| 13 | Simba-Common-00233. | [Enhancement] CLI dynamic command |
| 14 | Simba-Common-00234. | SNMPWALK but get error about sysResourceMgt |

**Runtime V1.2.2.11, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ~~ECS2000-28PP-00703~~ | ~~50 mac-address remained in mac table even if clear all mac table.~~ |
| 2 | ECS2000-28PP-00708 | [enhance] support poe chip fw 018818 & 021020 & 021019 |
| 3 | ECS2000-28PP-00709 | [enhance] runtime can upgrade the poe chip fw, and can read poe fw version. |
| 4 | ECS2000-28PP-00756. | CLI-Terminal-show any command about 10 times and set SNMP location will cause system crash. |
| 5 | ECS2000-28PP-00757 | stop routing after flush mac-address table two times |
| 6 | ECS2000-28PP-00759. | OAM should init the semaphore when startup |
| 7 | ECS2000-28PP-00765 | 1QVLAN-1870:DUT cannot save maximum VLAN setting per port |
| 8 | ECS2000-28PP-00766. | [RTK patch] rtk\_l2\_addrEntry\_get() support to get CAM entry (for 9x chip) |
| 9 | ECS2000-28PP-00767 | host route malfunction after applying static mac-address for host route |
| 10 | ECS2000-28PP-00770. | [Enhancement]Let RTK SDK RX thread be realtime with high priority |
| 11 | ECS2000-28PP-00777 | [Enhance] switching B/W L2 DHCP relay and L3 DHCP relay |
| 12 | ECS2000-28PP-00778 | [enhance] support simple chinese web page, web help page. |
| 13 | Simba-Common-00214. | CLI-Terminal-show any command about 10 times and set SNMP location will cause system crash. |
| 14 | Simba-Common-00216. | OAM should init the semaphore when startup |
| 15 | Simba-Common-00219 | RARP ethertype ix 0x8035, but the code is defined as 0x0835 in lan.c |

**Runtime V1.2.2.10, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00695 | loopback detecion detects traffic loop even port is DOWN |
| 2 | ECS2000-28PP-00726 | SNMP:RIP: Can't set MIB OID rip2IfConfDefaultMetric to valid value. |
| 3 | ECS2000-28PP-00732 | Web:RIP: On Routing Protocol>RIP>Distance>Action:Show page, display RIP distance with error subnet mask. |
| 4 | ECS2000-28PP-00733 | Web:RIP: When only create a RIP network per VLAN, can't open Routing Protocol>RIP>Network>Action:Show page. |
| 5 | ECS2000-28PP-00735. | [S900-NE-IT2-011] Can not save all of the vlan settings by comand(switchport allowed vlan) after reload the system |
| 6 | ECS2000-28PP-00737. | Web-1QVLAN-0020:delete all vlan didnot successfully |
| 7 | ECS2000-28PP-00739. | Enhancement: support LACP passive mode |
| 8 | ECS2000-28PP-00741 | RMON2-0190:trapDestOwner cannot be set |
| 9 | ECS2000-28PP-00742. | [IGMP filter] the multicast traffic does not match rule, but it still will be forwarded. |
| 10 | ECS2000-28PP-00743 | [WEB] RIP > Interface > Modify does not work. |
| 11 | ECS2000-28PP-00746 | Static port-channel cause loopback detection enable global failed |
| 12 | ECS2000-28PP-00749. | SNMP: The value of OID "lldpRemManAddrIfId" remove ".0" at the end. |
| 13 | ECS2000-28PP-00751. | IGMPSNP: fail to configure per VLAN settings soon after many VLANs are created |
| 14 | ECS2000-28PP-00752. | PPPoEIA can't work with QinQ tunnel |
| 15 | ECS2000-28PP-00755 | ASIC still learns mac address even disable mac learning on the port |
| 16 | ECS2000-28PP-00760 | [rd cloud] fix the Realtek project(ECS2100, ECS2110, ECS4100) build issue on RD Cloud build server. |
| 17 | Simba-Common-00099. | MLDSNP: Multicast data can not flood to other ports even MLDSNP is disabled. |
| 18 | Simba-Common-00135. | SNMP\_TD crash |
| 19 | Simba-Common-00138. | [Enhance] Modified openSSL/libXML build script to avoid privilege issue |
| 20 | Simba-Common-00145. | NTP: The ntp client of DUT will getting the ntp information after 1024 secs when the DUT reboot. |
| 21 | Simba-Common-00146. | Web-1QVLAN-0020:delete all vlan didnot successfully |
| 22 | Simba-Common-00148. | Enhancement: support LACP passive mode |
| 23 | Simba-Common-00150. | [IGMP filter] the multicast traffic does not match rule, but it still will be forwarded. |
| 24 | Simba-Common-00151. | [S900-S1\_9/E-NEST-056]After execution of copy running-config startup-config, if Startup configuration file name is NULL, no e |
| 25 | Simba-Common-00152. | Link state of LACP trunk member port changes between up and down repeatedly |
| 26 | Simba-Common-00153. | Static port-channel cause loopback detection enable global failed |
| 27 | Simba-Common-00154. | loopback detecion detects traffic loop even port is DOWN |
| 28 | Simba-Common-00155. | SNMP: The value of OID "lldpRemManAddrIfId" remove ".0" at the end. |
| 29 | Simba-Common-00156. | IPv6FTP: When DUT upgrade code with interrupt network connection and reconnect. It would cause upload fail. |
| 30 | Simba-Common-00210. | Web:RIP: On Routing Protocol>RIP>Distance>Action:Show page, display RIP distance with error subnet mask. |
| 31 | Simba-Common-00211. | Web:RIP: When only create a RIP network per VLAN, can't open Routing Protocol>RIP>Network>Action:Show page. |
| 32 | Simba-Common-00212. | IGMPSNP: fail to configure per VLAN settings soon after many VLANs are created |
| 33 | Simba-Common-00213. | PPPoEIA can't work with QinQ tunnel |

**Runtime V1.2.2.9, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00698. | SNMP\_TD crash |
| 2 | ECS2000-28PP-00706 | Web-1QVLAN-0020:delete all vlan didnot successfully |
| 3 | ECS2000-28PP-00710 | RIP: When DUT receive a RIP response with default route, there is no default route on RIP routing table. |
| 4 | ECS2000-28PP-00716 | RIP: No command to show RIP statistics from CLI. |
| 5 | ECS2000-28PP-00717 | RIP: No command to reset all RIP statistics on DUT from CLI. |
| 6 | ECS2000-28PP-00721 | RIP: The secondary IP address can't send periodic response. |
| 7 | ECS2000-28PP-00723 | Web:RIP: DUT doesn't support OSPF, but can configure RIP redistribute as OSPF on Web page for DUT. |
| 8 | ECS2000-28PP-00724 | Web:RIP: Information about sending RIP version and Receiving RIP version from Web page is not same as that from CLI. |
| 9 | ECS2000-28PP-00727 | SNMP:RIP: Inforamtion about sending RIP version and Receiving RIP version from SNMP is not same as that from CLI. |
| 10 | ECS2000-28PP-00730 | RIP: DUT can forward pakets with TTL=1 or TTL=0 by route forwarding. |
| 11 | ECS2000-28PP-00734 | [enhance] remove ERPS |
| 12 | Simba-Common-00141. | Failed to get switchport LACP info. |
| 13 | Simba-Common-00143. | Web:RIP: DUT doesn't support OSPF, but can configure RIP redistribute as OSPF on Web page for DUT. |
| 14 | Simba-Common-00144. | Web:RIP: Information about sending RIP version and Receiving RIP version from Web page is not same as that from CLI. |

**Runtime V1.2.2.8, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00697 | show policy-map cause CLI hang |
| 2 | ECS2000-28PP-00699 | packets send to switch cause routing loop - L3 rule issue |
| 3 | ECS2000-28PP-00704 | the switch doesn't remove host route(arp entry) when mac aging out. |
| 4 | ECS2000-28PP-00715 | SNMP:RIP: There is no private MIB table about RIP. |
| 5 | ECS2000-28PP-00718 | RIP: No command to show information about RIP peer on DUT from CLI. |
| 6 | ECS2000-28PP-00728 | SNMP:RIP: When set MIB OID rip2IfConfSend to 1(doNotSend), getting the value is other value. |
| 7 | ECS2000-28PP-00729 | SNMP:RIP: When set MIB OID rip2IfConfReceive to 4(doNotRecieve), getting the value is other value. |
| 8 | ECS4100-52T-00178 | [enhance] Change kernel memory allocator from SLOB to SLAB to have better performance |

**Runtime V1.2.2.7 (Based on V1.2.2.5), Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00699 | packets send to switch cause routing loop - L3 rule issue |
| 2 | ECS2000-28PP-00704 | the switch doesn't remove host route(arp entry) when mac aging out. |

**Runtime V1.2.2.6, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00691. | ECS4100 high cpu util |
| 2 | ECS2000-28PP-00696 | need remove atc's mib from private mib file. |
| 3 | ECS2000-28PP-00700 | [enhance] support RIP |
| 4 | ECS2000-28PP-00701 | Inject the LLDP packet, then dashboard and show remote device information will empty. |
| 5 | Simba-Common-00134. | NTP-0040:dut didnot handle NTP multiple servers well |
| 6 | Simba-Common-00136. | Inject the LLDP packet, then dashboard and show remote device information will empty. |
| 7 | Simba-Common-00140. | After reload , CPU Utilization incorrect bigger than 800M |

**Runtime V1.2.2.5, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00667 | RMON2 0080:snmpt didnot set probeConfigprobeDownloadTFTPServer successfully |
| 2 | ECS2000-28PP-00668 | RMON20110 0130:snmpt didnot set netConfigIPAddress successfully |
| 3 | ~~ECS2000-28PP-00669~~ | ~~RMON2 0180 0190:snmpt didnot set trapDestIndex-trapDestAddress and rapDestOwner successfully~~ |
| 4 | ECS2000-28PP-00684 | switch drop OSPF/RIP/VRRP packets when IGMPSNP or MVR is enabled |
| 5 | ECS2000-28PP-00690 | massive ip & arp packets may trigger hw watchdog reboot |
| 6 | ECS2100-10P-ACN-00050. | cable diag does not support the port at 10M Full/Half duplex. |
| 7 | Simba-Common-00098. | OSPF: When we clear OSPF interface setting from WEB; DUT show exception, and CLI is halted. |
| 8 | Simba-Common-00103. | The MVR VLAN does not removed automatically when I disable“mvr do 1 type receiver” on port 1. |
| 9 | Simba-Common-00104. | switch linkup slowly after switch reboot |
| 10 | Simba-Common-00106 | LLDP-MED: capabilities TLV transmission shall be enabled first and disabled last relative to other MED TLVs |
| 11 | Simba-Common-00107. | Huawei switch S2300 can't recognize ECS4100's LLDP packet with "dot1-tlv protocol identity" |
| 12 | Simba-Common-00109. | DoS: Use LOIC to attack port 22, CLI has no response and DUT reboot by watchdog. |
| 13 | Simba-Common-00110. | port utilization info is incorrect |
| 14 | Simba-Common-00112. | CPU MAC on slave is not removed when VLAN interface removed |
| 15 | Simba-Common-00113. | (54T)VLAN: IPs on VLAN IDs which are multiple of 32 up to 224 cannot be reachable. |
| 16 | Simba-Common-00114. | snmpEngineTime didn't reset the value even switch reboot |
| 17 | Simba-Common-00121. | [Telnet] After tool "LOIC" TCP:23port attack, modified thread pool for telnetd & tnshd |
| 18 | Simba-Common-00127. | [Stacking] sometimes startup config disappear |
| 19 | Simba-Common-00128. | MSTP: Change the instance priority, the traffic will stop and recover the issue after 6 mins. |
| 20 | Simba-Common-00130. | stacking problem: remove the stacking cable swtich will reload |

**Runtime V1.2.2.1, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00638 | [PoE] Add PoE chip lost-contact event to syslog-flash. |
| 2 | ECS2000-28PP-00657. | DNS: There is no DNS private mib. |
| 3 | ECS2000-28PP-00658. | DNS: There is no "show hosts" command. |
| 4 | ECS2000-28PP-00659. | CLI: Please rename "Excutes" to "Execute" about cable-diagnostics. |
| 5 | Simba-Common-00096. | memory leakage when injecting specific lldp packets |
| 6 | Simba-Common-00097. | loopback detection log messages are incorrect |
| 7 | Simba-Common-00100. | ECS4100-52T sends LLDP packet with no “port description, system name and system description” field after receiving Huawei s |

**Runtime V1.2.1.7, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00644 | [enhance] update the web help page (1.2.1.5) |
| 2 | ECS2000-28PP-00647 | Spanning-tree: We cannot enable the STP mode from WEB. |
| 3 | ECS2000-28PP-00648 | RADIUS-Acct: The console and Web of accounting information that is mismatch |
| 4 | ECS2000-28PP-00649 | Voice VLAN: DUT should not display the trunk member port in voice-vlan status list. |
| 5 | ECS2000-28PP-00651 | Spanning-tree: The default loopback-detection operation is incorrect on WEB. |
| 6 | ECS2000-28PP-00652 | Spanning-tree: We cannot enable loopback-detection on port from WEB. |
| 7 | ECS2000-28PP-00654 | IP-Cluster: The cluster member ID range is incorrect in WEB help page. |
| 8 | ECS2000-28PP-00656 | PoE: The maximum power budget in help page are inconsistent. |
| 9 | ECS2100-10P-ACN-00020 | CableDiag: No cable will show "OK" when run cable-diagnostics after the port is unplugged. |
| 10 | Simba-Common-00088 | [stacking] slave module port fail to set media-type sfp-force |
| 11 | Simba-Common-00093 | tacacs+-0080:dut crash when admin/admin login dut after tacacs-server key removed |
| 12 | Simba-Common-00094 | RADIUS-Acct: The console and Web of accounting information that is mismatch |

**Runtime V1.2.1.6, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00644 | [enhance] update the web help page (1.2.1.5) |
| 2 | Simba-Common-00085 | switch with stack can't display config complete via SSH |
| 3 | Simba-Common-00087 | switch stops sending syslog trap to server |

**Runtime V1.2.1.5, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00635 | [enhance] support QinQ priority mapping |
| 2 | Simba-Common-????? | IGMP-SNP: After remove vlan, an exception occurs. |
| 3 | Simba-Common-????? | IP-Cluster: Commander auto reboots after it logs off member switch. |
| 4 | Simba-Common-00086 | IP-Cluster: IP Cluster Web Management Failed |

**Runtime V1.2.1.4, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00550 | Statistics: The discard counter doesn't counting (Web part) |
| 2 | ECS2000-28PP-00632 | [Enhance] Support IP Cluster |
| 3 | ECS2000-28PP-00633 | Enhancement: add a new library function to replace strcat or strncat |
| 4 | ECS2000-28PP-00636 | PoE Power Consumption and firmware version are not showing on web page |

**Runtime V1.2.1.3, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00591 | [Enhancement] WEB needs to support MLDSNP Filtering |
| 2 | ECS2000-28PP-00619 | spelling/grammar - security > ip source guard > general |
| 3 | ECS2000-28PP-00627 | [enhance] the jump code of doing phase1 to phase2 (SYS\_CPNT\_XFER\_UPGRADE\_UBOOT\_AND\_RUNTIME need enabled, default is disable.) |
| 4 | ECS2000-28PP-00628 | STP : DUT2 console is down when spanning tree mode is stp |
| 5 | ECS2000-28PP-00629 | RSTP-PDU : DUT console is down after receive some PDU |
| 6 | ECS2000-28PP-00630 | MLDSNP: Forwarding rate of some UDP well known packets is very poor. |
| 7 | ECS2000-28PP-00633 | Enhancement: add a new library function to replace strcat or strncat |

**Runtime V1.2.1.2, Loader 0.2.1.1 (From this version, change the runtime’s header)**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00586 | [WEB] Remove/Disable MEP in ERPS |
| 2 | ECS2000-28PP-00620 | [enhance] phase2's new runtime header |

**Runtime V1.2.1.1, Loader 0.2.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00493 | [enhance] support sysTimeZonePredefined and sysSummerTimeMgt on MIB |
| 2 | ECS2000-28PP-00549 | [enhance] display total flash size in CLI 'dir' command for EC products. |
| 3 | ECS2000-28PP-00557 | IPv4-StaticRoute: Packets could not be forwarded after change routes continuously. |
| 4 | ECS2000-28PP-00564 | PoE: The help page need to be modified. |
| 5 | ECS2000-28PP-00565 | CoS: When we change DSCP-Queue mapping before trust mode, the output ratio is incorrect. |
| 6 | ECS2000-28PP-00577 | [WEB] MLDSNP statistic page has no Filter Drop to display. |
| 7 | ECS2000-28PP-00578 | Super password can remote login when set vtp password |
| 8 | ECS2000-28PP-00601 | TCAM: Deny ACE entries would be counted when the diffserv policy is bound to the port. |
| 9 | ECS2000-28PP-00604 | MVR: Group can not be deleted when registered port received leave report in transparent mode. |
| 10 | ECS2000-28PP-00606 | Syslog: restartControl by cold start (SNMP) will send warm start trap. |
| 11 | ECS2000-28PP-00607 | Diffserv: "set phb" command shall be removed from policy map. |
| 12 | ECS2000-28PP-00617 | Diffserv: missing 'no set ip dscp' command |
| 13 | ECS2000-28PP-00618 | [enhance] update the web help page (1.2.1.0) |
| 14 | ECS2000-28PP-00623 | ECS4120-28F media-type sfp-forced 100fx after reboot will linkup as 1000full. |
| 15 | ECS2000-28PP-00625 | DQoS: The default priority is not modifying when the port had once the authenticated. |
| 16 | ECS2000-28PP-00626 | 802.1XDQoS: The DUT will permit the supplicant when the attribute is wrong configure. |
| 17 | ECS2110-26T-00221 | CoS: Change cos-queue mapping, the data receive ratio is not changed. |

**Runtime V1.2.1.0, Loader 0.1.1.8 (Must)**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00430 | mac-authentication & IPSG mac mode can't work together |
| 2 | ECS2000-28PP-00525 | Dynamic Provision: The Dynamic Provision cannot work. |
| 3 | ECS2000-28PP-00539 | dut autoreboot when setting boot system opcode from 1.2.0.3 after autoupgrade |
| 4 | ECS2000-28PP-00547 | DHCPv6-Relay: DUT should support to set Relay address by WEB/SNMP. (web part) |
| 5 | ECS2000-28PP-00598 | dhcp retransmission interval is not right |
| 6 | ECS2000-28PP-00599 | RD-AUTOGRADE-0060 syslog about upgrade success didnot match expection |
| 7 | ECS2000-28PP-00600 | grammar - reload (Global Configuration) |
| 8 | ECS2000-28PP-00602 | 802.1X:802.1X-0120 mac based auth failed |
| 9 | ECS2000-28PP-00605 | grammar - Change "Tool" to "Tools" in folder list and related pages |
| 10 | ECS2000-28PP-00608 | igmpsnooping:DUTPA sent query with ip lower than dut ip,there is no dynamic mrouter port and querier is not the lower ip |
| 11 | ECS2000-28PP-00610 | System: Kernel panic - not syncing: Fatal exception in interrupt when "Flash programming started." is running after delete op |
| 12 | ECS2000-28PP-00611 | IGMP-SNP: When DUT receive IGMP query with lower IP address, the received port can't become mrouter port. |
| 13 | ECS2000-28PP-00614 | [enhance] update the web help page (1.2.0.6) |
| 14 | ECS2000-28PP-00566 | ECS2100 series PoE description maximum allocation power only by model ECS2100-10P/28PP |

**Runtime V1.2.0.8, Loader 0.1.1.7**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00584 | acl490~520,IP-extended ACL setting follow hints is failed |
| 2 | ECS2000-28PP-00587 | cli-termiarl0100,snmp0380 0400:hostname with symbol or length bigger than 54 cannot be set successfully |
| 3 | ECS2000-28PP-00590 | mDNS: Cannot login the DUT by WEB management when user using the IE(11.0) browser and mDNS address. |
| 4 | ECS2000-28PP-00593 | CLI-terminal: We cannot configure this maximum system name on DUT. |
| 5 | ECS2000-28PP-00595 | TACACS+: The DUT will reboot automatically when user logins the DUT by TACACS account, but the TACACS key is mismatch. |
| 6 | ECS2000-28PP-00603 | Correct ACL command tree |
| 7 | ECS2110-26T-00094 | SNMP/MIB and Web miss the "Linux Kernel Version" item. |

**Runtime V1.2.0.7, Loader 0.1.1.7**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00522 | CableDiag(Web): Pop "Data is invalid" when run cable diagnostic on fiber port from WebUI. |
| 2 | ECS2000-28PP-00531 | DHCPV6 Relay: DUT suould support to configure DHCPV6 Relay setting through SNMP. |
| 3 | ECS2000-28PP-00559 | WebAuth: Got "Failed to enable WebAuth" by CLI and "Data is invalid" by WebUI. |
| 4 | ECS2000-28PP-00561 | CoS: The help page of CoS is incorrect. |
| 5 | ECS2000-28PP-00574 | [enhance] support ERPS |
| 6 | ECS2000-28PP-00575 | [enhance] support new model ECS2100-10P-RAI |
| 7 | ECS2000-28PP-00576 | [enhance] set PoE power buget of ECS2100-10P-RAI to 101W |
| 8 | ECS2000-28PP-00582 | SSH: Watchdog reboots after SSH session timeout. |
| 9 | ECS2000-28PP-00583 | MLDSNP: Mrouter port forwarded multicaset data to normal port when normal port sent the same multicast data first. |
| 10 | ECS2000-28PP-00585 | failed to bind more service policy on port |
| 11 | ECS2000-28PP-00589 | RSTP/STP : The spanning tree mode configuration command can NOT be rejected when spanning tree is disabled |
| 12 | ECS2000-28PP-00592 | STP: DUT should reject to change the spanning-tree mode when spanning-tree status is "disable". |
| 13 | ECS2000-28PP-00594 | [web] Disable supporting Simplified Chinese. |

**Runtime V1.2.0.6, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00479 | NTP: The incorrect description of help page |
| 2 | ECS2000-28PP-00520 | MLDSNP: Other Querier Address can not be changed when non-querier received other queries. |
| 3 | ECS2000-28PP-00541 | IPV6-MLD-SNPDUT didnot handle the MLD querier election well to select the Lower IP address. |
| 4 | ECS2000-28PP-00543 | DUT didnot handle the various IPv6 Multicasts well when enables MLD Snooping |
| 5 | ECS2000-28PP-00547 | DHCPv6-Relay: DUT should support to set Relay address by WEB/SNMP. (SNMP part) |
| 6 | ~~ECS2000-28PP-00559~~ | ~~WebAuth: Got "Failed to enable WebAuth" by CLI and "Data is invalid" by WebUI.~~ |
| 7 | ECS2000-28PP-00560 | PoE: The PoE power range in WEB is incorrect. |
| 8 | ECS2000-28PP-00579 | [enhance] support mDNS |
| 9 | ECS2000-28PP-00580 | [enhance] update the web help page (1.2.0.3) |

**Runtime V1.2.0.4, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00492 | [Enhancement] HTTPS certificate should be able to return to default. |
| 2 | ECS2000-28PP-00500 | [enhance] support IPv6AddrTable. (.1.3.6.1.2.1.55.1.8) |
| 3 | ECS2000-28PP-00515 | MLDSNP: Can not show VLAN and Multicast IPv6 Address when show group with VLAN number. |
| 4 | ECS2000-28PP-00517 | MLDSNP: IPv6 well-known multicast can not be flooded. |
| 5 | ECS2000-28PP-00523 | PoE: add new cmd to choose mode for per-port maximum allocation. |
| 6 | ECS2000-28PP-00528 | [enhance] remove dhcp server |
| 7 | ECS2000-28PP-00545 | [enhance] remove phy internal loopback test. |
| 8 | ECS2000-28PP-00546 | [enhance] PoE: add new cmd to choose mode for per-port maximum allocation.(web part) |
| 9 | ECS2000-28PP-00551 | DHCPv6 Relay: DUT does not drop Relay-forw packets as receiving Hop-count large than or equal max-hop "32". |
| 10 | ECS2000-28PP-00555 | IPv4-StaticRoute: Packsets conuld be forwarded to other VLAN When one static route entry is removed. |
| 11 | ECS2000-28PP-00556 | IPv4-StaticRoute: CLI crashed when interface VLAN is down and showing routing table. |
| 12 | ECS2000-28PP-00558 | IPv4-StaticRoute: Static route can not work with trunk. |
| 13 | ECS2000-28PP-00563 | [enhance] support QinQ |
| 14 | ECS2000-28PP-00567 | MLDSNP: When MLDSNP was disabled, Other Querier Address doesn't show None. |
| 15 | ECS2000-28PP-00568 | MLDSNP: Other Querier Expire is 0 when received the query with higher IP address. |
| 16 | ECS2000-28PP-00569 | MLDSNP: Other Querier Address doesn't show None when the DUT received a query with higher IP address. |
| 17 | ECS2000-28PP-00570 | MLDSNP: Self Querier Expire is not 0 when the DUT receives teh query with lower IP address. |
| 18 | ECS2000-28PP-00571 | MLDSNP: DUT can not send the query when enable querier and VLAN's IP is lower. |
| 19 | ECS2000-28PP-00572 | MLDSNP: DUT, which is not querier, sent query when ther querier expired. |
| 20 | ECS2000-28PP-00573 | MLDSNP: IPv6 well-known multicast can not be flooded. |
| 21 | ECS2000-28PP-00550 | Statistics: The discard counter doesn't counting (CLI part) |

**Runtime V1.2.0.3, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00412 | [Enhancement] Support IPv4 static route |
| 2 | ECS2000-28PP-00421 | [enhance] support Web Authentication |
| 3 | ECS2000-28PP-00518 | snmp :dut canot be connected snmp version 1 with community public,after delete a snmp host |
| 4 | ECS2000-28PP-00527 | DHCP-SNP: When we reset the max-binding setting, it isn't matched to default value. |

**Runtime V1.2.0.2, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00264 | StaticRoute:DUT can set invalid s as next hop. |
| 2 | ECS2000-28PP-00274 | [Enhancement] sFlow on the RTL8380\_FAMILY |
| 3 | ECS2000-28PP-00275 | [Enhancement]Support Internal loopback test   * No web page |
| 4 | ECS2000-28PP-00276 | [Enhancement] DHCP server and L3 relay (v4/v6) >> Does not support DHCP Server. Will use ECS2000-28PP-00528 to remove DHCP Server.   * No snmp and web page. |
| 5 | ECS2000-28PP-00295 | [WEB] Support Simplified Chinese. |
| 6 | ECS2000-28PP-00326 | syslog trap contain "SNMP" string |
| 7 | ECS2000-28PP-00375 | SNMP:the warmSrart traps cannot be received when SNMP trap is enabled |
| 8 | ECS2000-28PP-00406 | [Enhancement] Support DoS rate limit |
| 9 | ~~ECS2000-28PP-00412~~ | ~~[Enhancement] Support IPv4 static route~~   * Fail |
| 10 | ECS2000-28PP-00417 | [enhance] support SFTP for file configuration and runtime upgrade. |
| 11 | ECS2000-28PP-00421 | [enhance] support Web Authentication   * fail |
| 12 | ECS2000-28PP-00476 | SNMP: Do not destory the community mapping group after remove notification host. |
| 13 | ECS2000-28PP-00486 | [WEB] Enhancement for sFlow web pages. |
| 14 | ECS2000-28PP-00509 | IP SourceGuard: The display parameters and iterm don't arrange in binding table neatly. |
| 15 | ECS2000-28PP-00510 | SNMP: We got an error message while perform SNMP walk. |
| 16 | ECS2000-28PP-00519 | DHCP: After we delete VLAN interface, DUT does not remove DHCP Client Vendor-class ID. |
| 17 | ECS2000-28PP-00521 | MLDSNP: Some show commands caused DUT to crash and reboot. |
| 18 | ECS2000-28PP-00526 | [Enhance] Exception log messages |

**Runtime V1.1.2.4, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00513 | enlarge overload condition to 34W for PoE class 0 - 3 |

**Runtime V1.1.2.3, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00463 | MLDSNP: DUT doesn't send tagged query including general query and GS query. |
| 2 | ECS2000-28PP-00481 | extended problem of ECS2000-28PP-00300 |
| 3 | ECS2000-28PP-00490 | MAC-VLAN: The information in CLI is different with MIB and Web |
| 4 | ECS2000-28PP-00504 | [Telnet] After tool "LOIC" TCP:23port attack, the DUT would reboot |
| 5 | ECS2000-28PP-00508 | [Enhancement] remove PoE overload disable mechanism from poedrv |
| 6 | ECS2000-28PP-00511 | Memory rising/falling trap reference to "memoryFreeInPercent" |
| 7 | ECS2000-28PP-00512 | [SFP DDM] "TX/RX power: NA", "Not support DDM" at CLI "show interface transceiver" |
| 8 | ~~ECS2000-28PP-00513~~ | ~~enlarge overload condition to 34W for PoE class 0 - 3~~ |
| 9 | ECS2000-28PP-00514 | missing a mib object to enabe/disable dhcp dynamic provision status |

**Runtime V1.1.2.2, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00145 | IPv6-AddrConfig: VLAN1 cann't get IPv6 addres from DHCPv6 server when VLAN1 and other VLAN have static address. |
| 2 | ECS2000-28PP-00308 | DAI: After setting ARP inspection can't get the gateway mac address. |
| 3 | ECS2000-28PP-00344 | CoS/DSCP should not map PHB in ECS2100 project , because of chipset limit. |
| 4 | ECS2000-28PP-00345 | After setting ARP inspection can't get the gateway mac address. |
| 5 | ECS2000-28PP-00447 | Dashboard: Switch event will be overlapped when multiple level are existed. |
| 6 | ECS2000-28PP-00469 | WEB: DUT should support to set the Cable Diag through WEB Page. |
| 7 | ECS2000-28PP-00475 | HTTPs: The https certificate information is incorrect. |
| 8 | ECS2000-28PP-00480 | DHCP client can't obtian IP address. (extended problem of ES3528MV2-FLF-EC-00612) |
| 9 | ECS2000-28PP-00483 | Update the web help page (V1.1.2.0) |
| 10 | ECS2000-28PP-00485 | The model name of ECS2100-10PE is incorrect. |
| 11 | ECS2000-28PP-00487 | [Telnet] watchdog reboot while using TCP 23 port link to DUT but not follow telnet protocol |
| 12 | ECS2000-28PP-00488 | IGMPSNP MIB can not set any port as the static router port |
| 13 | ECS2000-28PP-00489 | DHCP-snooping: Inform ACK dropped from trust port when the DHCP Snooping Binding entry is not existed |
| 14 | ECS2000-28PP-00491 | IP Source Guard: The MAC entry cannot be configured to maximum VLAN 4094. |

**Runtime V1.1.2.1, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00320 | MAC-base VLAN can't work with DHCPSNP |
| 2 | ECS2000-28PP-00341 | command "ip igmp snooping priority"   * Not support this. |
| 3 | ECS2000-28PP-00397 | IGMP-SNP: The static group can't be saved properly. |
| 4 | ECS2000-28PP-00435 | malformed of show ip dhcp snooping |
| 5 | ECS2000-28PP-00437 | DBG [SYS\_CALLBACK\_MGR\_SendMsg(), 13563]: |
| 6 | ECS2000-28PP-00460 | PoE: PoE software version displayed incorrect value. |
| 7 | ECS2000-28PP-00461 | LLDP-MED: (28T)Non-PoE device still sent Power-via-MDI TLV out. |
| 8 | ~~ECS2000-28PP-00463~~ | ~~MLDSNP: DUT doesn't send tagged query including general query and GS query.~~ |
| 9 | ECS2000-28PP-00472 | switch crash because of tacacs authentication, but there is no tacacs setting   * Duplicate with ECS2000-28PP-00470 |
| 10 | ECS2000-28PP-00474 | PoE: Help message should be the correct range of current board, on CLI and WEB. |
| 11 | ECS2000-28PP-00477 | ECViewPro: Got error: ECS2100-Series.mib: "617417", "3389:0", and "6159.9" when compile |
| 12 | ECS2000-28PP-00478 | Modify dhcpsnp default per port limit from code to oem |
| 13 | ECS2000-28PP-00482 | remove 26T/52T in private mib file. |

**Runtime V1.1.1.37, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00300 | MAC-VLAN/MAC-Filter: Can't set MAC: mac-address 001122334455 mask ff0000000000 |
| 2 | ECS2000-28PP-00434 | no info about show bridge-ext |
| 3 | ECS2000-28PP-00464 | Help: Suggest to correct spell from "disable" to disabled". |
| 4 | ~~ECS2000-28PP-00465~~ | ~~DHCP-snooping : The log information "failed to add dhcpsnp binding" is incorrect~~ |
| 5 | ECS2000-28PP-00466 | [NMTR] Discard input increased upon booted |
| 6 | ECS2000-28PP-00467 | [enhance] DAI: The log information of DAI add which type of arp dropped. |
| 7 | ECS2000-28PP-00470 | [Tacacs] Configured "authentication login tacacs" will cause CLI session waiting a long time and watchdog reboot |
| 8 | ECS2000-28PP-00471 | [telnet] Multi-user login with telnet at the same time might cause DUT reboot |

**Runtime V1.1.1.36, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00321 | MAC-base VLAN can't work with IPSG   * It is chip limitation. But use this epr to move the mac/protocol/voice vlan rule to slice 11 |
| 2 | ECS2000-28PP-00431 | enhancement : show policy-map interface |
| 3 | ECS2000-28PP-00456 | [web] Security > IP Source Guard > General. ACL Table Max Binding Entry does not match CLI. |
| 4 | ECS2000-28PP-00458 | IPSG binding table does not get info from DHCPSNP binding table |

**Runtime V1.1.1.34, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00320 | MAC-base VLAN can't work with DHCPSNP   * Fix indirectly in ECS2000-28PP-00323 -> Fix in V1.1.1.28 |
| 2 | ~~ECS2000-28PP-00321~~ | ~~MAC-base VLAN can't work with IPSG~~  ~~Not fixed in V1.1.1.34~~ |
| 3 | ECS2000-28PP-00347 | remove SW limiation : DHCPSNP 200 binding entries per system   * This was not a problem since ECS2000-28PP-00444 changes the entries. |
| 4 | ECS2000-28PP-00371 | LACP : The LACP can NOT be build after the port is removed from port security  Fix indirectly in ECS2000-28PP-00323 -> Fix in V1.1.1.28 |
| 5 | ECS2000-28PP-00372 | LACP : The LACP can NOT be build successfully  Fix indirectly in ECS2000-28PP-00323 -> Fix in V1.1.1.28 |
| 6 | ECS2000-28PP-00376 | Help-page: Storm control shall be changed to be disabled by default |
| 7 | ECS2000-28PP-00419 | DHCP-SNP: The display parameters and iterm don't arrange neatly. |
| 8 | ECS2000-28PP-00426 | web-page - can't configure DHCPSNP max-number |
| 9 | ECS2000-28PP-00429 | PortTrunk: When link partner without trunk setting, CLI print debug message. |
| 10 | ECS2000-28PP-00431 | enhancement : show policy-map interface |
| 11 | ECS2000-28PP-00433 | 2 problems of debug telnet |
| 12 | ECS2000-28PP-00435 | malformed of show ip dhcp snooping |
| 13 | ECS2000-28PP-00436 | traceroute does not support domain name |
| 14 | ECS2000-28PP-00438 | mib problem : does not support upgrade bootRom and loader in runtime. |
| 15 | ECS2000-28PP-00439 | auto-upgrade : it shows complete but it's failed. |
| 16 | ECS2000-28PP-00444 | [enhance] modify the ip dhcp snooping and ip source guard binding entries. |
| 17 | ECS2000-28PP-00450 | DHCP-snooping : The log information of dhcp snooping is ambiguous |
| 18 | ECS2000-28PP-00451 | remove interface vlan 2, the CPU MAC for VLAN 2 is still exist |
| 19 | ECS2000-28PP-00452 | [WEB] Move DHCPSNP and DHCP Option82 pages from IP Service to Security. |
| 20 | ECS2000-28PP-00453 | DHCP Client can't obtain IP address |
| 21 | ECS2000-28PP-00454 | ECS3510-28T DHCPSNP Client can't renew ip address |

**Runtime V1.1.1.33, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00253 | 802.1X: The DUT will send more radius requests to radius server when the dot1x operation-mode is single-host. |
| 2 | ECS2000-28PP-00340 | all of arp packets trapped to cpu and leads high cpu utilization |
| 3 | ECS2000-28PP-00407 | AutoUpgrade: ftp and tftp path should not allowed input @ if there is no username and password before IP |
| 4 | ECS2000-28PP-00423 | Web: "LLDP Remote Device Port List" on Dashboard is always empty |
| 5 | ECS2000-28PP-00427 | Dynamic QoS - should not display egress-rate limit on running-config |
| 6 | ECS2000-28PP-00428 | IPv4 ACL & MAC ACL can't work together |
| 7 | ECS2000-28PP-00440 | [AMTR]When created a trunk but with connection with link partner without setting a trunk, a error message is occured. |
| 8 | ECS2000-28PP-00441 | switch does not clear IPSG binding table when appliying clear DHCPSNP table. |
| 9 | ECS2000-28PP-00446 | update the web help page (1.1.1.31) |

**Runtime V1.1.1.32, Loader 0.1.1.5**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00290 | ACL: Can not bind ACL to a port with counter and time-range on WebUI. |
| 2 | ECS2000-28PP-00332 | PoE: Dut output power more than max allocation on 28PP with external PSU. |
| 3 | ECS2000-28PP-00408 | [Enhancement] Modify dashboard page. |
| 4 | ECS2000-28PP-00409 | AutoUpgrade:dut Abnormal when delete opcode file after autoupgrade several times |
| 5 | ECS2000-28PP-00411 | ImageMgt: The DUT will crash when execute auto upgrade |
| 6 | ECS2000-28PP-00413 | [WEB] ARP Inspection should only show existed VLAN. |

**Runtime V1.1.1.31, Loader 0.1.1.4**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00390 | [Enhancement] Dashboard page for WEB. |
| 2 | ECS2000-28PP-00404 | The file name of auto upgrade should be ECS2100-series.bix |
| 3 | ECS2000-28PP-00405 | Telnet and ping support host name |

**Runtime V1.1.1.30, Loader 0.1.1.4**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00311 | VLAN 1 cannot be removed, it will appear again after save configure and reboot. |
| 2 | ECS2000-28PP-00312 | VLAN 1 cannot be removed, it will appear again after save configure and reboot. |
| 3 | ECS2000-28PP-00329 | error message is not consistent if there is no member on port-channel |
| 4 | ECS2000-28PP-00349 | Enhance : command "show ip igmp profile" |
| 5 | ECS2000-28PP-00367 | LLDP : DUT can NOT handle the lldp pdu with Interface name and chassis ID/port ID with 255 |
| 6 | ECS2000-28PP-00370 | first apr packet cannot be leart to arp table after shutdown-no shutdown port |
| 7 | ECS2000-28PP-00374 | IP Source Guard: DUT should reject to create IPSG entry over maximum binding limit. |
| 8 | ECS2000-28PP-00378 | ACL hardware counter malfunction if add new ACE |
| 9 | ECS2000-28PP-00379 | [Enhancement] DHCP Snooping option82 CID/RID |
| 10 | ECS2000-28PP-00381 | [Enhancement] Adjust order of some WEB pages. |
| 11 | ECS2000-28PP-00388 | StormCtrl: Only broadcast will be displayed on show running-config after enabled and then disable it again. |
| 12 | ECS2000-28PP-00389 | [Enhancement] Add "Save Current Settings" button on index page. |
| 13 | ECS2000-28PP-00390 | [Enhancement] Dashboard page for WEB. |
| 14 | ECS2000-28PP-00393 | ACL-TCAM: When TCAM rule over maximum entry, the entry still can be created. |
| 15 | ECS2000-28PP-00394 | 802.1X-VLAN: The original VLAN does not remove when the port has been assign dynamic vlan. |
| 16 | ECS2000-28PP-00395 | [Enhancement] Dynamic QOS assignment (include egress rate limit) |
| 17 | ECS2000-28PP-00398 | [enhance] support MAC Authentication |
| 18 | ECS2000-28PP-00399 | [enhance] support Firmware Auto upgrade |
| 19 | ECS2000-28PP-00400 | [enhance] support Dynamic Provision (Configuration Auto upgrade(DHCP Option 66/67)) |
| 20 | ECS2000-28PP-00401 | [enhance] support FTP for file configuration and runtime upgrade. |
| 21 | ECS2000-28PP-00402 | [enhance] support DNS Client without DNS proxy |

**Runtime V1.1.1.28, Loader 0.1.1.3**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00289 | IGMP-SNP: The default value of IGMP snooping in help page is incorrect. |
| 2 | ECS2000-28PP-00298 | PortSecurity: The DUT will dump the error message when disable/enable the port security. |
| 3 | ECS2000-28PP-00302 | Help-page: Storm control is 500-262142, and please modify SFP description |
| 4 | ECS2000-28PP-00307 | IP Source Guard: After we enable and disable IPSG with max-binding "1", PC cannot ping to another PC. |
| 5 | ECS2000-28PP-00316 | LBD: should prevent ingress filtering from been changed when LBD operation is working on the port |
| 6 | ECS2000-28PP-00319 | Configuration of ARP ACL is not save properly in running-config/startup-config |
| 7 | ECS2000-28PP-00322 | MAC-base VLAN can't work with DAI |
| 8 | ECS2000-28PP-00323 | MAC-base VLAN can't work with DAI |
| 9 | ECS2000-28PP-00327 | STP LBD(action Block) can’t other detect traffic loops which happened on other ports. |
| 10 | ECS2000-28PP-00328 | Non-STP LBD(action Block) can’t other detect traffic loops which happened on other ports. |
| 11 | ECS2000-28PP-00331 | Ingress-filtering should not be disabled if Non-STP LBD is enabed. |
| 12 | ECS2000-28PP-00334 | should remove telnet "host name" command IF DNS not support. |
| 13 | ECS2000-28PP-00335 | remove command "dir boot-rom:" |
| 14 | ECS2000-28PP-00342 | IGMPSNP does not work with MAC-Base VLAN |
| 15 | ECS2000-28PP-00343 | IPSG max-binding set to 1 will drop the packets exist in binding entry |
| 16 | ECS2000-28PP-00346 | IP standard/extended, MAC ACL applied to port can’t filter packet to CPU |
| 17 | ECS2000-28PP-00348 | Show queue mode and press "other" can't quit |
| 18 | ECS2000-28PP-00352 | IPv6 std & ext ACL info in TCAM is in correct |
| 19 | ECS2000-28PP-00353 | IPv6 std & ext ACL info is incorrect in TCAM table |
| 20 | ECS2000-28PP-00354 | IP ACL can't work with IPSG |
| 21 | ECS2000-28PP-00357 | (10-port) wrong port LEDs behavior. |
| 22 | ECS2000-28PP-00361 | update the web help page (1.1.1.25) |
| 23 | ECS2000-28PP-00373 | [enhance] remove the block action of STP loopback detection and non-stp loopback detection. |

**Runtime V1.1.1.27, Loader 0.1.1.3**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00183 | SNMP: SNMP Engine boot will not reset back to 1 after engine-id reset. |
| 2 | ECS2000-28PP-00208 | SNMP: DUT factory default reboot ,SNMP Engine boots will not be 1 |
| 3 | ECS2000-28PP-00258 | CoS: CLI can't stop display queue mode after press other key. |
| 4 | ECS2000-28PP-00278 | Statistics: UDLD does not been removed |
| 5 | ECS2000-28PP-00282 | Help\_Page: Default vlaue of IP Address Mode, IP Address, and Subnet Mask in help page is wrong. |
| 6 | ECS2000-28PP-00283 | Help\_Page: Default vlaue of all items of DoS Protection is wrong. |
| 7 | ECS2000-28PP-00285 | PortSec: The MAC-address of security can not move between the port security of ports when the network-access aging is enabled |
| 8 | ECS2000-28PP-00286 | DHCP-SNP: When the DHCP-Client move to another port, DUT create wrong binding enrty. |
| 9 | ECS2000-28PP-00287 | Help Page: The default spanning-tree enabling status is wrong. |
| 10 | ECS2000-28PP-00288 | Diffserv: (Web) Please modify description of meter from WEB help. |
| 11 | ~~ECS2000-28PP-00289~~ | ~~IGMP-SNP: The default value of IGMP snooping in help page is incorrect.~~  ~~(not fix in this version)~~ |
| 12 | ECS2000-28PP-00291 | Spanning-tree: When we set the release mode to manual, the loop-detection action cannot work. |
| 13 | ECS2000-28PP-00292 | Help\_Page: Please remove descripton of ACL Mirror on ACL help page. |
| 14 | ECS2000-28PP-00293 | IP Source Guard: When we enable DHCP-SNP and IPSG with MAC mode; DUT should not discard all DHCP-Request packets. |
| 15 | ECS2000-28PP-00294 | DHCP-SNP: DUT should limit the DHCP Snooping maximum binding number; and it should drop unnecessary DHCP-Request packets. |
| 16 | ECS2000-28PP-00296 | SwitchMgmt: EPLD show 0.00, and "Main Power Status" shows "Not present". |
| 17 | ECS2000-28PP-00297 | Help\_Page: It has been modified about web help description because default IP is 192.168.2.10. |
| 18 | ECS2000-28PP-00298 | PortSecurity: The DUT will dump the error message when disable/enable the port security. |
| 19 | ECS2000-28PP-00302 | Help-page: Storm control is 500-262142, and please modify SFP description |
| 20 | ECS2000-28PP-00303 | IGMP-SNP: After diable/enable igmp-snp, multicast traffic can't be forwarded properly. |
| 21 | ECS2000-28PP-00304 | ACL-TCAM: We can create entry over TCAM rules. |
| 22 | ECS2000-28PP-00305 | IGMP-SNP: Change maximum IGMP-SNP group to 511. |
| 23 | ECS2000-28PP-00306 | LoopbackDetection: No help page of LBD information |
| 24 | ECS2000-28PP-00310 | Loopback Detection: A problem of default value that is about LBD and ingress rule. |
| 25 | ECS2000-28PP-00314 | HW change: GPIO RST\_CONFIG reversed to be low-active at 10T model. |
| 26 | ECS2000-28PP-00324 | remove unsupport command "Clear elm, mar, mv6, pope" |
| 27 | ECS2000-28PP-00325 | remove unsupported debug commands "debug mvr6 , show debug mvr6" |
| 28 | ECS2000-28PP-00329 | error message is not consistent if there is no member on port-channel |
| 29 | ECS2000-28PP-00337 | igmp max-group is 511, not 512 |
| 30 | ECS2000-28PP-00350 | memory rising trap appears every switch rebooting |
| 31 | ECS2000-28PP-00361 | update the web help page (1.1.1.25) |
| 32 | ECS2000-28PP-00362 | [enhance] change the default of Broadcast storm control to Disable |
| 33 | ECS2000-28PP-00363 | 802.1x: The Radius host will disappear when sets the key value of radius host is maximum number after save/reboot the DUT. |

**Runtime V1.1.1.26, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00267 | ACL: Untagged/tagged 802.3 filter is useless. |
| 2 | ECS2000-28PP-00281 | [AMTR] Static MAC address can't add when learned 8k dynamic MAC address |
| 3 | ECS2000-28PP-00284 | RSPAN: First session source port setting will be copied to other sessions when show running/startup |
| 4 | ECS2000-28PP-00299 | ACL:tagged packets cannot be denied by ACL |
| 5 | ECS2000-28PP-00301 | CLI: Unexpected message is showed after the DUT rebooted (only 10P). |
| 6 | ECS2000-28PP-00313 | [Enhancement]Remove cable diag time-out error message. |

**Runtime V1.1.1.25, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00279 | [SNMP] while delete trap host by CLI, then it will fail to add trap host table by MIB |

**Runtime V1.1.1.24, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00120 | Trap: This trap host cannot be configured successfully. |

**Runtime V1.1.1.23, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00259 | SYSLOG: Please fix/remove error log when DUT bootup. |

**Runtime V1.1.1.22, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00269 | [enhance] remove EFM OAM, UDLD |

**Runtime V1.1.1.21, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00172 | CPU-Storm-Protection: Can not access DUT when input unicast packets which DA is DUT's MAC to DUT and CPU guard is enabled. |
| 2 | ECS2000-28PP-00203 | RADIUS-Acct: The Accounting name will keep count that doesn't refresh when the port has changed the accounting name. |
| 3 | ECS2000-28PP-00205 | Radius: The traffic will forward when authenticator state is connecting. |
| 4 | ECS2000-28PP-00226 | Web: Please integrate UI(3 sessions allowed) and help(1 session allowed) |
| 5 | ECS2000-28PP-00229 | IPv6: IPv6 ND packets can be trapped to CPU when all IPv6 function is disabled. |
| 6 | ECS2000-28PP-00256 | PoE: (28PP) DUT can't output power when PD request over maximum allocation power. |
| 7 | ECS2000-28PP-00260 | Unsupported commands on CLI and WebUI shall be removed. |
| 8 | ECS2000-28PP-00261 | System: This Average CPU Utilization is 60% in default setting. |
| 9 | ECS2000-28PP-00262 | IP Source-guard: DUT should not create acl/mac dynamic entry over maximum binding. |
| 10 | ECS2000-28PP-00265 | [enhance] support Non-STP loopback Detection |
| 11 | ECS2000-28PP-00268 | MSTP : DUT can NOT save the MSTP config after reload |
| 12 | ECS2000-28PP-00269 | [enhance] remove EFM OAM, UDLD |
| 13 | ECS2000-28PP-00270 | ImageMgmt: The auto upgrade information has display on help page, the product doesn't support. |
| 14 | ECS2000-28PP-00271 | ACL: IPv6 pacekts would be dropped by IPv4 ACL. |
| 15 | ECS2000-28PP-00272 | PortSecurity: The port will shut down when the learning mac-address has no exceed the max-mac-count of port security. |
| 16 | ECS2000-28PP-00273 | IP Source-guard: DUT should not create acl/mac dynamic entry over maximum binding.(Sync to phase1 branch) |

**Runtime V1.1.1.20, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00092 | WEB: time range shoud be under Administration |
| 2 | ECS2000-28PP-00121 | IPv6-TraceRoute: Source IP address on traceroute execution page is wrong. |
| 3 | ECS2000-28PP-00185 | LLDP: Create LLDP CA-Type with maximum length of CA-Value, it will dispaly garbage character on WEB. |
| 4 | ECS2000-28PP-00220 | Help\_Page: Host Name in Ping help page shall be reomved. |
| 5 | ECS2000-28PP-00224 | Diffserv: We can't add police rate-limit via WEB. |
| 6 | ECS2000-28PP-00250 | [AMTR] SDK print Error Code: 0x60009 when disable port security and left security MAC in system. |
| 7 | ECS2000-28PP-00251 | EEE: Suggest to remove power-save setting/description from SFP ports |
| 8 | ECS2000-28PP-00252 | [WEB] Administration > PoE > PSE, Configure Global page shows undefined. |
| 9 | ECS2000-28PP-00255 | Ping: Data size in packets is what we configured when it is configured less than 32 bytes or great than 512 bytes. |
| 10 | ECS2000-28PP-00257 | PortSecurity: The DUT will crash and reboot automatically when enable port security and show the mac-table or running-config. |
| 11 | ECS2000-28PP-00260 | Unsupported commands on CLI and WebUI shall be removed.  (remove loader password, QinQ, VLAN Trunking, EFM OAM, UDLD) |
| 12 | ECS2000-28PP-00263 | Wrong Main Power Status at "show version" command |
| 13 | ECS2000-28PP-00266 | [enhance] change default setting(default static ip, igmpsnp, stp, dos...) due to EC's request. |
| 14 | ES4528BH2-HPoE-0815-EC-00020 | L2\_L4 process might crash while PSEC status changed between enable/disable with continue packets inject. |

**Runtime V1.1.1.13, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00254 | WatchDog: 10port models are always reset affter runtime runs. |

**Runtime V1.1.1.12, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00122 | IPv6-TraceRoute: Description of max-failures on CLI has wrong word. |
| 2 | ECS2000-28PP-00192 | TimeRange: The time range bound to the interface can not be showed when it's name has mixed characters and numbers. |
| 3 | ECS2000-28PP-00200 | IP Source Guard: DUT cannot create dynamic IPSG binding entry under MAC mode. |
| 4 | ECS2000-28PP-00201 | NTP: The DUT doesn't send the request packets of ntp. |
| 5 | ECS2000-28PP-00204 | Protocol-VLAN: The VLAN priority doesn't chang after change priority setting. |
| 6 | ECS2000-28PP-00207 | Voice VLAN: After we enable and disabling security, DUT should not drop non-OUI voice VLAN traffic. |
| 7 | ECS2000-28PP-00213 | Port Security: The DUT will crash and reboot automatically when 802.1x and port security function have work as the same time. |
| 8 | ECS2000-28PP-00234 | TrafficSeg: After enable DAI/DHCP snooping with traffic-segmentation, CLI print error message. |
| 9 | ECS2000-28PP-00237 | 1QVLAN: DUT cannot clear VLAN 4094 MAC address. |
| 10 | ECS2000-28PP-00240 | Statistic: The RMON packets count should not be increased on link-down status; and it cannot be cleared. |
| 11 | ECS2000-28PP-00242 | L2Switch:Flowcontrol function can’t be saved |
| 12 | ECS2000-28PP-00243 | IP Source Guard: DUT cannot create dynamic IPSG binding entry under MAC mode. (Sync to branch) |
| 13 | ECS2000-28PP-00244 | NTP: The DUT doesn't send the request packets of ntp. (Sync to Branch) |
| 14 | ECS2000-28PP-00245 | 1QVLAN:ingress filter will not work correctly after save config and reboot |
| 15 | ECS2000-28PP-00246 | System: DUT lose to send out control packets and rebooting itself in system environment. |
| 16 | ECS2000-28PP-00247 | GPIO: Error message after port security enabled |

**Runtime V1.1.1.10, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00141 | IPv6-AddrConfig: DUT only sends 1 NS packet when DAD attempts is factory default value. |
| 2 | ECS2000-28PP-00151 | DAI: DUT console lock and auto reboot in havy loading. |
| 3 | ECS2000-28PP-00154 | DAI: We can't enable arp inspection validate IP without allow zeros by SNMP. |
| 4 | ECS2000-28PP-00156 | MLDSNP: FCS in MLD GSS query sent from DUT is wrong. |
| 5 | ECS2000-28PP-00166 | IGMP-Filter: After create IGMP profile via SNMP, the range table become mismatch. |
| 6 | ECS2000-28PP-00175 | IPv4-RemotePing: DUT accepts echo reply which source IP address is different from destinaton IP address of echo request. |
| 7 | ECS2000-28PP-00180 | RSTP: After we enable RSTP with LACP, DUT return error and all data flooding. |
| 8 | ECS2000-28PP-00194 | SNMP: CLI print debug message after perform SNMP walk several minutes. |
| 9 | ECS2000-28PP-00195 | L2SW:when configure port flow control ,it will cause print error message to console |
| 10 | ECS2000-28PP-00209 | Help\_Page: Hele page of MAC-Based VLAN is blank. |
| 11 | ECS2000-28PP-00210 | Help\_Page: Please remove RA Guard Mode description. |
| 12 | ECS2000-28PP-00212 | Help\_Page: TCAM description doesn't match current design. |
| 13 | ECS2000-28PP-00216 | Help\_Page: Please remove Echo/Chargen Attack and WinNuke Attack description. |
| 14 | ECS2000-28PP-00218 | IP Source Guard: After PC can new IP address, DUT does not update dynamic IPSG entry. |
| 15 | ECS2000-28PP-00219 | Help\_Page: Help page of IP is blank. |
| 16 | ECS2000-28PP-00220 | Help\_Page: Host Name in Ping help page shall be reomved. |
| 17 | ECS2000-28PP-00221 | PoE: We can't save PoE Maximum Allocation Power value. |
| 18 | ECS2000-28PP-00222 | Rate-Limit: Enable ingress rate-limit on trunk, both ingress and egress are take effect. |
| 19 | ECS2000-28PP-00223 | PortTrunk: CLI print error message after disable auto-negotiation and enable flow control. |
| 20 | ECS2000-28PP-00225 | System: After we get snmp-walk to DUT, it return error. |
| 21 | ECS2000-28PP-00226 | Web: Please integrate UI(3 sessions allowed) and help(1 session allowed) |
| 22 | ECS2000-28PP-00227 | ACL: Can't add any ACE of IP ACL. |
| 23 | ECS2000-28PP-00228 | LLDP: Some typo need to be correct in help page. |
| 24 | ECS2000-28PP-00230 | System: After we save running configuration and rebooting, some data always is flooded. |
| 25 | ECS2000-28PP-00231 | Mirror-PortBased:configure port mirror will fail and does not work |
| 26 | ECS2000-28PP-00232 | [1G fiber port]Let 1G fiber support AutoNeg. |
| 27 | ECS2000-28PP-00233 | Update the web help page to correct some eprs' issue. |
| 28 | ECS2000-28PP-00235 | MVR receiver port will receive 2 query |
| 29 | ECS2000-28PP-00236 | WatchDog: apply different way to kick watch dog, CPU's or RTL3189's GPIO. |
| 30 | ECS2000-28PP-00243 | IP Source Guard: DUT cannot create dynamic IPSG binding entry under MAC mode. (Sync to branch) |
| 31 | ECS2000-28PP-00244 | NTP: The DUT doesn't send the request packets of ntp. (Sync to Branch) |

**Runtime V1.1.1.9, Loader 0.1.1.1**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00096 | Ping: Ping packet size on WebUI can be set out of range. |
| 2 | ECS2000-28PP-00097 | ImageMgmt: Remove the autoUpgrade page of web. |
| 3 | ECS2000-28PP-00169 | TrafficSeg: Sent IGMP join message to downlink port, CLI print error message. |
| 4 | ECS2000-28PP-00176 | LLDP: The value of auto-negotiation capability shows all zero. |
| 5 | ECS2000-28PP-00177 | LLDP: The remote information not aligned after receive maximum length of system name TLV. |
| 6 | ECS2000-28PP-00191 | Remove booting debug/error message on console on 10 port device |
| 7 | ECS2000-28PP-00196 | [MAU MIB]MAU MIB geteway error message is shown |
| 8 | ECS2000-28PP-00206 | [L2Switch] [ECS2000-10T] Porting |
| 9 | ~~ECS2000-28PP-00211~~ | ~~1QVLAN: After we save VLAN tag setting on SFP port and rebooting; this egress packets should be unatgged.~~ |

**Runtime V1.1.1.7, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00076 | Static address cannot set to an inactive trunk |
| 2 | ECS2000-28PP-00098 | Ping6: The DUT doesn't have any response on WebUI when target IP address is multicast address. |
| 3 | ECS2000-28PP-00153 | Syslog: There is no remote warm/cold start log when we create maximum logging host. |
| 4 | ECS2000-28PP-00155 | MLDSNP: Disabled Immediate Leave is useless. |
| 5 | ECS2000-28PP-00164 | DHCP-Relay: This option82 drop mode cannot work. |
| 6 | ECS2000-28PP-00170 | AMTR: DUT cannot save maximum static address, and it return error. |
| 7 | ECS2000-28PP-00171 | IGMP-SNP: Configure IGMP priority, CLI print error message. |
| 8 | ECS2000-28PP-00179 | RSTP: After we enabled and disable loop-detection, DUT is halted and rebooting itself. |
| 9 | ECS2000-28PP-00181 | IGMP-SNP: When immediate leave enable, the IGMPv3 group can't leave after recieve leave message. |
| 10 | ECS2000-28PP-00190 | [new model]10 port board, porting peripherals. |
| 11 | ECS2000-28PP-00193 | [WEB] Modify login page |

**Runtime V1.1.1.6, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00077 | SNMP: CLI print debug message after perform SNMP walk. |
| 2 | ECS2000-28PP-00094 | SNTP: The effect of summer time is incorrect for australia and new zealand region. |
| 3 | ECS2000-28PP-00104 | IGMP-SNP: Create mrouter port by port range, only first port become mrouter port. |
| 4 | ECS2000-28PP-00109 | MLDSNP: Multicast dataMLDSNP: Multicast data can't be forwarded to another static mrouter when change unknown-multicast mode. |
| 5 | ECS2000-28PP-00115 | Port security: Error Code: 0x13 DEV\_SWDRV\_GetPortLinkStatus(): Line = 9099 , error\_id=19 |
| 6 | ECS2000-28PP-00118 | IGMP-SNP: The maximum group value over feature list. |
| 7 | ECS2000-28PP-00123 | IGMP-SNP: There is unnessary IGMP authencation command. |
| 8 | ECS2000-28PP-00126 | L2SW: After we link to SFP port, DUT cannot learn any MAC address. |
| 9 | ECS2000-28PP-00128 | SNMPTrap: Enterprise value in standard SNMP trap is wrong. |
| 10 | ECS2000-28PP-00129 | 802.1x: The ping will time out that is between DUT and PC when the dot1x state is the Authenticated. |
| 11 | ECS2000-28PP-00131 | LACP: LACP display page can't exit by press other key (other than [Space], [Enter] or [A]). |
| 12 | ECS2000-28PP-00134 | Remove SYS\_CPNT\_DHCPSNP\_SYSTEM\_RATELIMIT |
| 13 | ECS2000-28PP-00136 | Statistic: After we connect packet generator and SFP ports, the statistic/RMON count cannot work. |
| 14 | ECS2000-28PP-00140 | IPv6-AddrConfig: IPv6 address got from RA shows "INVALID" |
| 15 | ECS2000-28PP-00142 | [ECS4510-28F] revise design when SFP port type change |
| 16 | ECS2000-28PP-00146 | 1QVLAN: After we set acceptable-frame type to tagged, DUT drop all untag/tag packets. |
| 17 | ECS2000-28PP-00147 | 1QVLAN: After we set acceptable-frame type to tagged, DUT lose control packets. |
| 18 | ECS2000-28PP-00148 | 1QVLAN: After we change VLAN status from suspend to active; DUT return error and drop all packets. |
| 19 | ECS2000-28PP-00150 | Port-Trunk: Connect trunk member with forced 100 full port, CLI print error message. |
| 20 | ECS2000-28PP-00158 | MSTP: The DUT will continuing print the error message when topology change overnight. |
| 21 | ECS2000-28PP-00159 | MSTP: The DUT will continuing print the error message when topology change overnight. |
| 22 | ECS2000-28PP-00161 | DHCP-Relay: After we enable DHCP-Relay-option82, DUT cannot forward DHCP-Reply to client. |
| 23 | ECS2000-28PP-00163 | DoS-Protection: UDP Flooding Attack is useless. |
| 24 | ECS2000-28PP-00165 | RSPAN: Failed to set port monitor when RSPAN is existed. |
| 25 | ECS2000-28PP-00167 | ACL: Behavior of TCP control-flag is wrong. |
| 26 | ECS2000-28PP-00168 | IGMP-Filter: The maximum group range is incorrect. |
| 27 | ECS2000-28PP-00174 | AMTR: The collision-mac-address-table always is empty. |
| 28 | ECS2000-28PP-00182 | [POE] Spec changed. Every poe porst supports 802.3at, all the time. |
| 29 | ECS2000-28PP-00187 | [enhance] change the model name from ECS2000 to ECS2100 |
| 30 | ECS2000-28PP-00188 | Diffserv: Can't set police rate-limit via SNMP. |
| 31 | ECS2000-28PP-00189 | SFP eeprom is failed to read, on some tranceivers. |

**Runtime V1.1.1.5, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00029 | [EEE]Lack of Power Saving web page |
| 2 | ECS2000-28PP-00071 | LLDP : The Operational MAU Type is Unknown (0x0000) |
| 3 | ECS2000-28PP-00078 | [Enhancement] CPU utilization is approach 30% in the default environment |
| 4 | ECS2000-28PP-00088 | CoS: The packet receiving ratio doesn't follow DSCP mutation table. |
| 5 | ECS2000-28PP-00090 | CoS: CLI can't stop display queue mode after press other key. |
| 6 | ECS2000-28PP-00093 | It will make mac-address dynamic learned on trunk 1 be cleared when trunk 1 still have active trunk member. |
| 7 | ECS2000-28PP-00099 | WEB: need remove dynamic VLAN web page from this product. |
| 8 | ECS2000-28PP-00105 | Trunk : DUT would pop error message continously when connect to 10Mhalf hub |
| 9 | ECS2000-28PP-00107 | CLI : DUT would show some debug message after reload |
| 10 | ECS2000-28PP-00108 | MLDSNP: Unexpected message is showed when enable MLD Snooping. |
| 11 | ECS2000-28PP-00110 | Provision: Reload this DUT, it return some error. |
| 12 | ECS2000-28PP-00114 | Configuration: After we save maximum VLAN and ACL setting, DUT lose startup configuration. |
| 13 | ECS2000-28PP-00117 | WEB: The feature list dosen't support the cos-phb, but dut can show the feature on WEB |
| 14 | ECS2000-28PP-00124 | IPv6-TraceRoute: Can't traceroute link-local address on WebUI. |
| 15 | ECS2000-28PP-00125 | Provision: Reload this DUT, it return some error. |
| 16 | ECS2000-28PP-00127 | SNMP: DUT factory default reboot ,SNMP Engine boots will not be 1 |
| 17 | ECS2000-28PP-00130 | SNMP:DUT factory default reboot,SNMP Engine boots will not be 1 |
| 18 | ECS2000-28PP-00132 | CLI: Please remove ACL/MAC/VLAN mirror command. |
| 19 | ECS2000-28PP-00133 | [MAU MIB]Gateway implementation |
| 20 | ECS2000-28PP-00137 | 802.1x: The supplicant information will disappear when enable reauthentication. |
| 21 | ECS2000-28PP-00138 | CPU queue scheduling and weight |
| 22 | ECS2000-28PP-00143 | Cable-Diag does not work on salve units |
| 23 | ECS2000-28PP-00149 | DHCPServer: The host IP shall be display on "Active Pool". |
| 24 | ECS2000-28PP-00152 | Cable Diagnostic: DUT should remove this loopback test command since it isn't supported. |

**Runtime V1.1.1.2, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00084 | DHCP-Snooping: After we remove port member from trunk, DUT show invalid interface ID. |
| 2 | ECS2000-28PP-00085 | CoS: Drop precedence could be configured on WEB. |
| 3 | ECS2000-28PP-00086 | Diffserv: We can configure meter on WEB. |
| 4 | ECS2000-28PP-00087 | CLI command prompt should show 4094. |
| 5 | ECS2000-28PP-00091 | WEB: need support forbidden type on VLAN page. |
| 6 | ECS2000-28PP-00095 | 1QVLAN: After we remove native VLAN and saving configuration, it will appear this VLAN again. |
| 7 | ECS2000-28PP-00102 | Web: Model name in front panel on WebUI is wrong and Site Map is 4040 Not Found. |
| 8 | ECS2000-28PP-00106 | Remove MAC Authentication |
| 9 | ~~ECS2000-28PP-00108~~ | ~~MLDSNP: Unexpected message is showed when enable MLD Snooping.~~  ~~(Not fix yet)~~ |
| 10 | ECS2000-28PP-00111 | IPv4-AddrConfig: DHCP Client Vendor Class ID is wrong. |
| 11 | ECS2000-28PP-00112 | IP Source Guard: After we enable IPSG, client cannot get IP. |
| 12 | ECS2000-28PP-00135 | Update the web help page. (1.1.1.0) |

**Runtime V1.1.1.1, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00007 | [Rule] Porting |
| 2 | ECS2000-28PP-00017 | Bring up peripherals |
| 3 | ECS2000-28PP-00029 | [EEE]Lack of Power Saving web page |
| 4 | ECS2000-28PP-00037 | validate POE function |
| 5 | ECS2000-28PP-00040 | Voice vlan: DUT not change voice vlan packets' vlan priority which match voice vlan oui |
| 6 | ECS2000-28PP-00047 | [CoS] Porting |
| 7 | ECS2000-28PP-00068 | Syslog: to support save logfile in TLV format. |
| 8 | ECS2000-28PP-00070 | [EEE] Revised EEE code by charlie's review |
| 9 | ECS2000-28PP-00071 | LLDP : The Operational MAU Type is Unknown (0x0000) |
| 10 | ECS2000-28PP-00072 | Delete unnecessary files from CC |
| 11 | ECS2000-28PP-00073 | remove mvr6 function |
| 12 | ECS2000-28PP-00074 | SNMP: SNMP Engine boot will not reset back to 1 after engine-id changed. |
| 13 | ECS2000-28PP-00075 | Diffserv: We can't save class-map configuration. |
| 14 | ECS2000-28PP-00079 | [Internal Loopback]Remove this feautre from phase 1. |
| 15 | ECS2000-28PP-00082 | ACL: CLI has IP/IPv6 command on MAC ACL. |
| 16 | ECS2000-28PP-00081 | MAC-VLAN: This MAC VLAN cannot work. |
| 17 | ECS2000-28PP-00083 | CLI: remove garp/gvrp related commands because they are not supported for the project |

**Runtime V1.1.1.0**

|  |  |
| --- | --- |
| 1 | Init Version |

**Work as Designed (wAD) Or Faulty report eprs:**

**Runtime V1.1.2.2, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00355 | ACL can't deny dhcp packet If VLAN interface is static IP. |
| 2 | ECS2000-28PP-00396 | 802.1X-GVLAN: User can configure the Guest-VLAN which is the id number of suspend VLAN or id number of inexistent VLAN . |
| 3 | ECS2000-28PP-00455 | After delete static mac entry, the corresponding arp entry should be deleted, too. |
| 4 | ECS2000-28PP-00484 | IP Source Guard: The default maximum binding number is incorrect. |
| 5 | ECS2000-28PP-00497 | IP Source Guard: We can enable this IP filter with MAC mode, but DUT does not filter this source IP. |

**Runtime V1.1.1.35, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00432 | 802.1x authorized, but 802.1x is disabled.  -> modify spec. |
| 2 | ECS2000-28PP-00443 | 802.1x-GVLAN-0030:Guest VLAN shall NOT take effect if specified VLAN is not activated on DUT  -> modify spec |
| 3 | ECS2000-28PP-00468 | DHCP-SNP: DHCP-SNP maximum binding does not matched to IP Source-guard, and it should be limited.   * Due to EPR: ECS2000-28PP-00444 |

**Runtime V1.1.1.35, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00418 | DHCP-SNP: DUT send out incorrect encoding option 82 information. |

**Runtime V1.1.1.34, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00383 | IPv4-AddrConfig: Default gateway address can set network address and broadcast address. |

**Runtime V1.1.1.33, Loader 0.1.1.6**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00410 | DHCP\_DYNC\_Prov: When destination file name over 32 we got error message. |
| 2 | ECS2000-28PP-00424 | Statistic: When we inject unicast packets with 128 bytes and no CRC error, this undersize and Fragments count should not be i |

**Runtime V1.1.1.30, Loader 0.1.1.4**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00336 | maximum IPSG binding entires is 63 per system |
| 2 | ECS2000-28PP-00368 | LLDP : The LLDP pdu dose NOT include TIATR-41Committee |
| 3 | ECS2000-28PP-00369 | IPv4-AddrConfig:Setting Gateway IP with network address and broadcast address will not appear error. |
| 4 | ECS2000-28PP-00380 | MAC-VALN: MAC-VLAN function can not work. |
| 5 | ECS2000-28PP-00382 | COS : The ratio is wrong when mapping priority queue |
| 6 | ECS2000-28PP-00391 | Statistic: When we inject unicast packets to single port from mutiple ports; the collision count is not increased. |
| 7 | ECS2000-28PP-00392 | CoS: When data forwarded by same queue, the received ratio will become incorrect. |

**Runtime V1.1.1.24, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00248 | Voice Vlan : Voice vlan security mode can NOT drop the packetes' which not match voice vlan oui |

**Runtime V1.1.1.21, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00239 | 802.1X: The dot1x functionally should be work well with windows2008 NPS. |

**Runtime V1.1.1.12, Loader 0.1.1.2**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00241 | ARP: The DUT doesn't renew ARP entry when receive gratuitous arp. |

**Runtime V1.1.1.10, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00186 | DAI: During display DAI log, the entry will print in different line. |
| 2 | ECS2000-28PP-00198 | RD-MAC-Learning: configure static mac address entries to a trunk,after delete the trunk these entries still exist |
| 3 | ECS2000-28PP-00199 | RD-MAC-Learning: configure static mac address entries to a vlan,after delete the vlan these entries still exist |
| 4 | ECS2000-28PP-00217 | PoE: CLI display incorrect power inline status. |

**Runtime V1.1.1.7, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00162 | DHCP-Relay: DUT should not configure own IP and subnet address as relay server. |
| 2 | ECS2000-28PP-00178 | NTP: The ntp client of DUT will getting the ntp information after 1024 secs when the DUT reboot. |
| 3 | ECS2000-28PP-00184 | STP: The range of pathcost method is incorrect. |

**Runtime V1.1.1.6, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00116 | DHCP Snooping: This DHCP snooping limit cannot work, DUT return error message. |
| 2 | ECS2000-28PP-00157 | DAI: Configure DAI rate-limit to none, the rate of ARP message still be limited. |

**Runtime V1.1.1.5, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00089 | IPv6\_HTTP: Can not login management page via link-local address of the DUT. |
| 2 | ECS2000-28PP-00103 | ImageMgmt: Can't download the image when the DUT has full load traffic. |
| 3 | ECS2000-28PP-00113 | PortSecurity: The CPU Utilization displays 100% when the port has configure the port security setting. |
| 4 | ECS2000-28PP-00119 | MAC-Filter: The MAC-Filter doesn't work which has no "network-access mode mac-authentication" command on per-port. |

**Runtime V1.1.1.2, Loader 0.1.0.0**

|  |  |  |
| --- | --- | --- |
|  | EPR | Headline |
| 1 | ECS2000-28PP-00100 | ImageMgmt: During download the opcode which DUT will reboot by another session. |
| 2 | ECS2000-28PP-00101 | IGMP-SNP: Multicast data flood after group timeout. |

**Diag change log**

|  |  |  |
| --- | --- | --- |
|  | version | Change log |
| 1 | V0.0.1.6 | 1.Fix extloopback.test on 10P  2.Fix msi\_poe get error message with first operation。 |
| 2 | V0.0.1.5 | 1.Fix bug caused by diag 0.0.1.4 display fix  led.test:  RTK.0> LED default  register set 0xa000  2. Fix i2c write error message  swutil smi set reg 4 0x1 0xFF  smi set reg 4 0x1 0xFF  Error (0xffffffff): General Error  3. fix gpio18 init value, which will cause soft-reboot can not enter runtime OS.  4.fix gpio17 init direction as "in" |
| 3 | V0.0.1.4 | Fix display of command "swutil port dump port 0" |
| 4 | V0.0.1.36(testing) | 1. remove msi\_poe.new (test finished)  2. cancel 100ms wait between UART communication to accelerate FW download speed |
| 5 | V0.0.1.3 | 28PP Support board id = 8 (8218B->8218D) |

**Known Bugs and Issues:**

Any other problems than those listed above should be reported to our Technical Support Staff.

**Known RESTRICITIONS AND Limitations:**

|  |  |
| --- | --- |
| 1 | L2 table (8K entries) share for L2 unicast, L2 multicast, IPv4 multicast, IPv6 multicast, Routing. |
| 2 | For all Basic Switching Unit-Test items of the half duplex, the counter of fragments would increase the same number/speed as the counter, collisions on IXIA.  It is confirmed by Realtek Josh. It is chip normal behaviour which follow the standard.  RTK use the “Collision based backpressure” of flow control(backpressure) on half mode. It will send the jam pattern packet to do the flow control. |
| 3 | Due to chip limitation, do not support Port-based QoS. |
| 4 | Due to chip limitation, not support global ACL (As before said "VLAN ACL") |
| 5 | Due to chip limitation, not allow configure IP/IPv6 pattern on MAC ACL. |
| 6 | Due to chip limitation(chip did not have addition table which internal priority to Queue for CPU), do not support command “qos map phb-queue”. |
| 7 | We had double confirm with REALTEK, and the chip  1. doesn't support color  2. burst size only support global setting (Only two configuration)  so it only could use for police flow rate-limite,  Add new CLI command on "police-map class" mode  **[no] police rate** *rate-kbps* |
| 8 | Due to chip limitation, there are 7 counters not be supported: (ECS2000-28PP-00051)  Error Output  Unknown Protocols Input  QLen Output  Alignment Errors  SQE Test Errors  Internal Mac Reveive Errors  Carrier Sense Errors  Due to chip limitation, The Discard input(IF\_IN\_DISCARDS\_INDEX) is not support in the RealTek 838x / 839x chip family, however, the SDK would return RT\_ERR\_OK with such case.( ECS2000-28PP-00466) |
| 9 | The cabel diag function can detect maximum to 100 meters, the error is 12~15 meters. |
| 10 | Due to chip limitation, do not support per-port jumbo frame. Only support per-system jumbo frame. |
| 11 | Due to chip limitation(rule's remark action only can remark cos or dscp), voice vlan function can not support remarking dscp priority. |
| 12 | Due to chip and h/w board’s design limitation, while SFP transceiver plug in, the cpu need take more time to init it. It will lead system response slow. |
| 13 | Due to chip limitation, can not support “False Carrier Sense Counter” on MAU MIB. |
| 14 | Chip can not provide the collision mac-address. |
| 15 | Due to chip limitation, cannot support change the priority of multicast packet. |
| 16 | Due to chip limitation, the reason of trap to cpu of protocol packet like bpdu/lacp/lldp/dot1x are all the same, all these packets will go throw the queue 5. |
| 17 | Due to many functions need rule table to implement. IPv4 std/extend ACL use the same h/w rule slice. So IPv4 std and IPv4 extend ACL can not enable at the same time. |
| 18 | Due to many functions need rule table to implement. IPv6 std/extend ACL use the same h/w rule slice. So IPv6 std and IPv6 extend ACL can not enable at the same time. |
| 19 | Due to chip limitation, only support BPDU bypass VLAN check, LACP bypass VLAN check, LLDP bypass VLAN check. OK |
| 20 | Due to chip limitation. MAC-base VLAN can't work with IPSG. [ECS2000-28PP-00321] |
| 21 | PHY internal loopback test can not test the port which did not have PHY. Like port 9, 10 at 10 port device. |
| 22 | Due to chip limitation, when port is link up at 10 Mbps, Cable Diag is not supported. |
| 23 | Chip limitation: If a packet is mirrored to mirroring port due to one port’s rx and the other port’s tx, only 1 packet, the copy of rx, will be copied to mirroring port. [ECS4100-52T-00046] |
| 24 | Chip limitation: Cable diagnostics can detect cable length up to 100 meters with an inaccuracy around 15 meters. |
| 25 | Chip limitation: When a port is linkup at 10 Mbps speed, cable diagnostics is not supported. [ECS2110-26T-00055] |
| 26 | Chip limitation: 8x Storm Control UC / MC / BC maximum values: 262142 (0x3ffff-1) |
| 27 | Due to chip limitation, there is only 1 copy, which is from the port with smallest port id, for mirroring non-unicast in egress dirextion(tx). [ECS2100-10P-ACN-00022] |
| 28 | Due to Jquery software limitation. The web browser need IE 9+, Chrome 54+, Firefox 52+ or Opera 41+. [ECS2000-28PP-00706] |
| 29 | Due to Openssh software limitation. SSH only support 6 encryption algorithms default: chacha20-poly1305@openssh.com 、aes128-ctr 、aes192-ctr、aes256-ctr、aes128-gcm@openssh.com 、[aes256-gcm@openssh.com](mailto:aes256-gcm@openssh.com). [ECS2100EC-138/121] |

**Compliance support:**

|  |  |
| --- | --- |
| **Compliance Level** | **Compliant** |
|  |  |

Known Anomalies: None.

**IEEE Standards Support:**

|  |  |
| --- | --- |
| **Standard** | **Title** |
| IEEE 802.1D | Transparent Bridging Specifications (ISO/IEC 10038) |
| IEEE 802.1p | Traffic Class Expediting and Dynamic Multicast Filtering |
| IEEE 802.1Q | Virtual Bridged Local Area Networks |
| IEEE 802.1w | Rapid Spanning Tree |
| IEEE 802.2 | Local Area Networks, Logical Link Control (LLC) |
| IEEE 802.3 | CSMA/CD 9 (ISO/IEC 8802-3) |
| IEEE 802.3I | 10Base-T (ISO/IEC 8802-3, clause 14) |
| IEEE 802.3u | 100Base-TX (ISO/IEC 8802-3, clause 25) |
| IEEE 802.3x | Flow Control |
| IEEE 802.3z | 1000Base-SX, 1000Base-LX |
| IEEE 802.3ab | 1000Base-TX |
| IEEE 802.3ac | VLAN Tag |
| IEEE 802.3ad | Link Aggregation |
| IEEE 802.1X | Port-based Network Access Control |

**IETF Standards MIB Support:**

|  |  |  |
| --- | --- | --- |
| **RFC No.** | Title | **Groups Supported** |
| 1907 | SNMPv2-MIB (MIB II) | - system group ( 1-9)  - snmp group (1-6, 8-22, 24-32) |
| 2011 | IP-MIB (MIB-II) | - ip group (1-20, 22-23) - icmp group (1-26) |
| 2012 | TCP-MIB (MIB-II) | - tcp group (1-15)(tcpConnTable only support read.) |
| 2013 | UDP-MIB (MIB-II) | - udp group (1-5) |
| IEEE  802.1X MIB | IEEE8021-PAE-MIB | - dot1xPaeSystem (1-2)  - dot1xPaeAuthenticator (1-3)(not support per-port timer setting) |
| 1493 | Bridge MIB | - dot1dBase group (1-4) - dot1dStp group (1-15) - dot1dTp group (1-4) - dot1dStatic group (1) |
| 2863 | Interfaces Evolution MIB (IF-MIB) | - interface group (1-2) (ifadminStatus not support set to 3(testing))  - ifXTable group (1) - ifStackTable group (1)(support  read-only) |
| 2819 | RMON MIB | - statistics group (1) - history group (1-2) - alarm group (1) - event group (1-2) |
| 2618 | RADIUS MIB | - radiusAuthClientMIB (1) |
| 2665 | Etherlike MIB | - dot3StatsTable group (1-19) |
| 2737 | Entity MIB | * entityPhysical group (1-16)   (support read-only) |
| 2674 | P-bridge | - dot1dExtBase group (1-4) - dot1dPriority group (1,3)  - dot1dGarp group (1) |
| 2674 | Q-bridge | - dot1qBase group (1-5) - dot1qTp group (1-2) - dot1qStatic group(1) - dot1qVlan (1-5) (9-10) |
| V-Bridge MIB | V-Bridge MIB | - dot1vProtocol group |
| 3636 | MAU MIB | * dot3IfMauBasicGroup * dot3IfMauAutoNegGroup |

|  |  |  |
| --- | --- | --- |
| 1612 | DNS Reslover MIB | * dnsServConfig * dnsServCounter * dnsServCounterAuthAns * dnsServCounterAuthNoNames * dnsServCounterAuthNoDataResps * dnsServCounterNonAuthDatas * dnsServCounterNonAuthNoDatas * dnsServCounterReferrals * dnsServCounterErrors * dnsServCounterRelNames * dnsServCounterReqRefusals * dnsServCounterReqUnparses * dnsServCounterOtherErrors * dnsServOptCounter * dnsResMIBObjects * dnsResConfig * dnsResCounter * dnsResCache * dnsResCacheStatus * dnsResCacheMaxTTL * dnsResCacheGoodCaches * dnsResCacheBadCaches * dnsResOptCounter |
| 3411 | SNMP FrameWork | * snmpFrameworkMIBObjects |
| 3412 | SNMP MPD MIB | * snmpMPDMIBObjects |
| 3413 | SNMP Target MIB | * snmpTargetObjects |
| 3413 | SNMP Notify MIB | * SnmpNotifyObjects * snmpNotifyTable * usmMIBObjects |
| 3415 | SNMP View-Based ACM MIB | * vacmMIBObjects * Private MIB * switchMgt * portMgt * trunkMgt * lacpMgt * staMgt * tftpMgt * restartMgt * mirrorMgt * igmpSnoopMgt * ipMgt * bcastStormMgt * vlanMgt * priorityMgt * trapDestMgt * qosMgt * securityMgt * sysLogMgt * lineMgt |

**ECS2100 Private Enterprise MIB Support:**

|  |  |
| --- | --- |
| **Title** | Version |
| ECS2100-Series.mib | 201903120000Z |

**SNMP Trap Support:**

|  |  |
| --- | --- |
| **RFC No.** | **Title** |
| RFC 1215 | ColdStart (v1) warmStart (v1) linkDown (v1) linkUp (v1) authenticationFailure (v1) |
| RFC 1907 | coldStart (v2c) warmStart (v2c) authenticationFailure (v2c) |
| RFC 2863 | linkDown (v2c) linkUp (v2c) |
| RFC 1493 | newRoot (v1) topologyChange (v1) |
| RFC 1757 | risingAlarm (v1)  fallingAlarm (v1) |
| RFC 2819 | risingAlarm (v2c) fallingAlarm (v2c) |

**Customer Support:**

By Phone:

By Email:

By Web:

By Fax: