Access Switch ECS4100-52T/ECS4100-26TX/ECS4100-28T/ECS4100-12T/ECS4100-28P/ECS4100-52P/ECS4100-12PH/ECS4100-28TC/ECS4100-12Tv2

***Phase 2 Firmware Version 1.2.72.203***

**INTRODUCTION:**

ECS4100-52T is a Gigabit Ethernet L3-Lite switch featuring 48 10/100/1000 ports, and 4 Gigabit Ethernet SFP uplink ports.

ECS4100-26TX is a Gigabit Ethernet L3-Lite switch featuring 24 10/100/1000 ports, and 2 10Gigabit Ethernet SFP+ uplink ports.

ECS4100-28T is a Gigabit Ethernet L3-Lite switch featuring 24 10/100/1000 ports, and 4 Gigabit Ethernet SFP uplink ports.

ECS4100-12T/12Tv2 is a Gigabit Ethernet L3-Lite switch featuring 8 10/100/1000 ports, 2 Gigabit Copper/SFP combo ports, and 2 Gigabit Ethernet SFP uplink ports.

ECS4100-12PH is a Gigabit Ethernet L3-Lite PoE switch featuring 8 10/100/1000 PoE ports, 2 Gigabit Copper/SFP combo ports, and 2 Gigabit Ethernet SFP uplink ports.

ECS4100-28TC/28TC-F is a Gigabit Ethernet L3-Lite switch featuring 24 10/100/1000 ports, and 4 Gigabit Copper/SFP combo ports.

|  |
| --- |
| **It is recommended that one thoroughly review this release notes prior to the installation or upgrade of this product.** |

**Firmware Specification:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Status** | **Version No.** | **Type** | **Release Date** |
| EIT/NTC Test Version | 1.2.73.203 | Git Master (2020/09/02 1PM) | 2020/09/02 |
| EIT/NTC Test Version | 1.2.72.203 | Git Master (2020/08/25 3PM) | 2020/08/25 |
| TS Test Version | 1.2.44.201 | Git Master (2020/03/30 3PM) | 2020/03/30 |
| TS Test Version | 1.2.43.201 | Git Master (2020/03/26 9AM) | 2020/03/26 |
| EIT/TS Test Version | 1.2.42.201 | Git Master (2020/03/23 10AM) | 2020/03/23 |
| EIT/TS Test Version | 1.2.41.201 | Git Master (2020/02/28 4PM) | 2020/03/02 |
| EIT/TS Test Version | 1.2.40.194 | Git Master (2019/12/2 2PM) | 2019/12/2 |
| TS Test Version | 1.2.39.193 | Git Master (2019/09/24 3PM) | 2019/09/27 |
| TS Test Version | 1.2.38.193 | Git Master (2019/08/22 9AM) | 2019/08/22 |
| TS Test Version | 1.2.37.191 | Git Master (2019/03/21 5PM) | 2019/03/26 |
| NTC/TS Test Version | 1.2.36.191 | Git Master (2019/01/30 5PM) | 2019/01/31 |
| NTC/TS Test Version | 1.2.35.191 | Git Master (2019/01/04 3PM) | 2019/01/07 |
| NTC/TS Test Version | 1.2.34.184 | Git Master (2018/12/12 4PM) | 2018/12/13 |
| TS Test Version | 1.2.33.184 | Git Master (2018/11/09 8PM) | 2018/11/15 |
| NTC/TS Test Version | 1.2.32.184 | Git Master (2018/10/18 8PM) | 2018/10/19 |
| TS Test Version | 1.2.31.184 | Git Master (2018/10/05 3PM) | 2018/10/05 |
| NTC/TS Test Version | 1.2.30.183 | CC: EC\_VOB main (2018/09/12 1PM) | 2018/09/12 |
| Cancelled | 1.2.29.183 | CC: EC\_VOB main (2018/08/23 5PM) | 2018/08/24 |
| Cancelled | 1.2.28.183 | CC: EC\_VOB main (2018/08/20 10AM) | 2018/08/20 |
| NTC Test Version | 1.2.27.183 | CC: EC\_VOB main (2018/07/24 2PM) | 2018/07/24 |
| NTC Test Version | 1.2.26.182 | CC: EC\_VOB main (2018/06/29 4PM) | 2018/06/29 |
| Cancelled | 1.2.25.182 | CC: EC\_VOB main (2018/06/19 4PM) | 2018/06/20 |
| NTC Test Version | 1.2.24.182 | CC: EC\_VOB main (2018/05/18 11AM) | 2018/05/18 |
| NTC Test Version | 1.2.23.182 | CC: EC\_VOB main (2018/05/15 6PM) | 2018/05/15 |
| NTC Test Version | 1.2.22.182 | CC: EC\_VOB main (2018/05/02 5PM) | 2018/05/02 |
| NTC Test Version | 1.2.21.182 | CC: EC\_VOB main (2018/04/24 4PM) | 2018/04/24 |
| NTC Test Version | 1.2.20.182 | CC: EC\_VOB main (2018/04/20 11AM) | 2018/04/20 |
| NTC Test Version | 1.2.19.182 | CC: EC\_VOB main (2018/04/17 2PM) | 2018/04/17 |
| RD Test Version | 1.2.18.182 | CC: EC\_VOB main (2018/04/03 12PM) | 2018/04/03 |
| NTC Test Version | 1.2.17.18112PH specific | CC: EC\_VOB main (2018/03/30 10AM) | 2018/03/30 |
| NTC Test Version | 1.2.17.181 | CC: EC\_VOB main (2018/03/19 8PM) | 2018/03/20 |
| NTC Test Version | 1.2.16.181 | CC: EC\_VOB main (2018/03/05 12PM) | 2018/03/05 |
| NTC Test Version | 1.2.15.181 | CC: EC\_VOB main (2018/01/15 5PM) | 2018/01/16 |
| TS Test Version | 1.2.14.181 | CC: EC\_VOB main (2018/01/04 9AM) | 2018/01/04 |
| EIT Test Version | 1.2.13.174 | CC: EC\_VOB main (2017/12/11 12PM) | 2017/12/11 |
| EIT Test Version | 1.2.12.174 | CC: EC\_VOB main (2017/11/6 9AM) | 2017/11/6 |
| Cancelled | 1.2.11.174 | CC: EC\_VOB main (2017/11/2 9AM) | 2017/11/2 |
| NTC Test Version | 1.2.10.174 | CC: EC\_VOB main (2017/10/26 1PM) | 2017/10/26 |
| NTC Test Version | 1.2.9.173 | CC: EC\_VOB main (2017/09/21 1PM) | 2017/09/21 |
| NTC Test Version | 1.2.7.173 | CC: EC\_VOB main (2017/09/15 9AM) | 2017/09/15 |
| NTC Test Version | 1.2.6.173 | CC: EC\_VOB main (2017/08/22 9AM) | 2017/08/22 |
| NTC Test Version | 1.2.5.173 | CC: EC\_VOB main (2017/08/16 9AM) | 2017/08/16 |
| NTC Test Version | 1.2.4.173 | Based on V1.2.3.173 + ECS4100-52T-00103 only | 2017/07/12 |
| NTC Test Version | 1.2.3.173 | CC: EC\_VOB main (2017/07/07 9AM) | 2017/07/07 |
| NTC Test Version | 1.2.2.172 | CC: EC\_VOB main (2017/06/05 10PM) | 2017/06/06 |
| EIT Test Version | 1.2.1.172 | CC: EC\_VOB main (2017/05/23 1PM) | 2017/05/23 |
| TS Patch Version~~NTC Test Candidate~~ | 1.2.0.172 | CC: EC\_VOB main (2017/04/20 6PM) | 2017/04/21 |
| Customer Test Version | 1.03.02.171 | CC: EC\_VOB main (2017/03/02 4PM) | 2017/03/02 |
| TS Patch Version(Cancelled) | 1.1.11.171 | CC: EC\_VOB main (2017/01/13 5PM) | 2017/01/16 |
| NTC Test Version(Formal Release /MP) | 1.1.8.164 | CC: EC\_VOB main (2016/11/24 4PM) | 2016/11/24 |
| RD Test Version(Customer Sample) | 1.1.4.164 | CC: EC\_VOB main (2016/10/21 12PM) | 2016/10/21 |
| NTC Test Version | 1.1.3.164 | CC: EC\_VOB main (2016/10/17 9PM) | 2016/10/18 |
| RD Test Version(Customer Sample) | 1.1.2.1641.1.1.164 | CC: EC\_VOB main (2016/10/11 11AM) | 2016/10/132016/10/11 |
| RD Test Version(Customer Sample) | 1.1.0.163 | CC: EC\_VOB main (2016/9/29 9PM) | 2016/9/30 |
| NTC Test Version | 0.0.3.0 | CC: EC\_VOB main (2016/9/14 12PM) | 2016/9/19 |
| NTC Test Version | 0.0.2.5 | CC: EC\_VOB main (2016/8/11 9PM) | 2016/8/12 |
| NTC Test Version | 0.0.2.3 | CC: EC\_VOB main (2016/7/19 8PM) | 2016/7/20 |
| NTC Test Version | 0.0.1.1 | CC: EC\_VOB main (2016/5/6 5PM) | 2016/5/6 |

**LOADER:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Status** | **Version No.** | **Type** | **Release Date** |
| Testing Version | 1.0.2.2 | - | 2018/08/15 |
| Testing Version | 1.0.2.1 | - | 2018/07/24 |
| Testing Version | 1.0.2.0 | - | 2018/07/02 |
| Testing Version | 1.0.1.9 | - | 2018/05/14 |
| Testing Version | 1.0.1.8 | - | 2018/04/03 |
| Testing Version | 1.0.1.7 | - | 2018/02/12 |
| Testing Version | 1.0.1.6 | - | 2017/12/18 |
| Testing Version | 1.0.1.4 | - | 2017/11/8 |
| Testing Version | 1.0.1.1 | - | 2017/04/21 |
| Testing Version | 1.0.0.5 | - | 2015/11/09 |
| Testing Version | 1.0.0.4 | - | 2015/10/17 |
| Deposed | 1.0.0.3 | - | 2015/9/19 |
| Testing Version | 1.0.0.2 | - | 2015/8/18 |
| Testing Version | 1.0.0.1 | - | 2015/7/20 |
| Testing Version | 1.0.0.0 | - | 2015/6/23 |
| Testing Version | 0.0.1.0 | - | 2015/3/14 |

**HARDware compatibility:**

ALL

**BootPROM compatibility:**

ALL

**Network Management Software Support:**

|  |  |  |
| --- | --- | --- |
| **NMS Platform** | **Version No.** | **Module No.** |
| TBD |   |   |

If you install this image, you may not have control of all of the latest features of this product until the next version(s) of network management software. Please review the software release notes for your specific network management platform for details.

**SUPPORTED FUNCTIONALITY:**

Please see the ECS4100\_ECS2110\_Phase2\_FeatureList\_20180418.xlsx

**Installation and Configuration Notes:**

In general, the ECS4100 **Switch** will be shipped to you pre-configured with this version of firmware. If you would like to upgrade an existing ECS4100 **Switch,** please follow the TFTP download instructions that are included with your firmware image upgrade kit.

**Known Bugs and Issues:**

|  |  |  |
| --- | --- | --- |
|  | ECS4100-52T-00026ECS2110-26T-00155 | ImageMgmt: Got result "Image checksum error" when copy ftp file by FileZilla V0.9.56 beta (Not-Reproducible) |
|  | ECS4100-52T-00029ECS2110-26T-00200 | Nessus\_Scan: Nessus Scan found some security issues. (Under investigation) |
|  | ECS4100-52T-00031ECS2110-26T-00208 | System: CPU is closed to 100% when 6 HTTPS sessions are connected and stayed on Dashboard. (Under investigation) |
|  | ECS4100-52T-00032ECS2110-26T-00210 | WebMgmt: There are some vulnerability issues.(SSL: 2 Critical, 1 High, ....) (Under investigation) |

**Firmware Changes and Enhancements:**

The following Known Issues have been fixed in this release of firmware.

**loader code modifications:**

**Loader V1.0.2.2**

|  |  |  |
| --- | --- | --- |
|  | EPR N/A | (12Tv2) While Loader V1.0.2.1 is booting with SFP module insertion to port 11/12, the Port LED will be turned On then Off quickly. |

**Loader V1.0.2.1**

|  |  |  |
| --- | --- | --- |
|  | ECS4100-52T-00436 | (12Tv2) Support for board re-layout (new BID=17) |

**Loader V1.0.2.0**

|  |  |  |
| --- | --- | --- |
|  | ECS4100-52T-00421 | [Enhance] Bootloader automatically boots the second one when the startup runtime is corrupted. |
|  | ECS4100-52T-00429 | (Enhancement) Support 28TC-F (BID = 16)for Fan speed control and system reboot with Reset button |

**Loader V1.0.1.9**

|  |  |  |
| --- | --- | --- |
|  | EPR N/A | Fixed some mfg issues, reported by TE & PPE |

**Loader V1.0.1.8**

|  |  |  |
| --- | --- | --- |
|  | ECS4100-52T-00369 | (Enhancement) Support 28TC-ITUS (BID = 15) |
|  | EPR N/A | Init to make (DIAG LED – Green Blinking) and (PWD LED - Green Solid) |

**Loader V1.0.1.7**

|  |  |  |
| --- | --- | --- |
|  | ECS4100-52T-00325 | (Enhancement) Support 12T-ITUS (BID = 14) |

**Loader V1.0.1.6**

|  |  |  |
| --- | --- | --- |
|  | ECS4100-52T-00308 | (Updated) Support 28TC, 28T-ITUS, 28P-ITUS (BID = 11, 12, 13) |

**Loader V1.0.1.4**

|  |  |  |
| --- | --- | --- |
|  | EPR N/A | Support disable fan when booting in 12PH. |
|  | EPR N/A | Support bid 11, 12, 13 |
|  | EPR N/A | The default boot argument mem change to 240M and add quiet. |

**Loader V1.0.1.1**

|  |  |  |
| --- | --- | --- |
|  | ECS4100-52T-00144,145 | Supports new boards for 12T, 28P, 52P (BID = 9, 6, 8, respectively) |

**Loader V1.0.0.5**

|  |  |  |
| --- | --- | --- |
|  | EPR N/A | 10G Port LEDs (#25,#26) are not lighting on external\_loopback\_test /Diag. |

**Loader V1.0.0.4**

|  |  |  |
| --- | --- | --- |
|  | EPR N/A | a. Get DRAM clock back to 300 MHz (V1.0.0.2 MEM:300MHz stable, V1.0.0.3 MEM:400MHz risky)b. Add BID=4 (fan-less 52T), doing exactly same HW init as BID=0 (fan-ful 52T)c. Do not display Realtek Chip# on U-Boot messages |

**Loader V1.0.0.3**

|  |  |  |
| --- | --- | --- |
|  | EPR N/A | [Enhance] Update bootloader’s backdoor password (default) and enable password |
|  | ECS4100-52T-00037 | [Enhance] Support new board - ECS4100-28T: 24\*GbE + 4\*SFP(GbE) |

**Loader V1.0.0.2**

|  |  |  |
| --- | --- | --- |
|  | EPR N/A | (Diag) external\_loopback\_test fails (SFP port linkdown) after internal\_loopback\_test is executed. |

**Loader V1.0.0.1**

|  |  |  |
| --- | --- | --- |
|  | ECS2110-26T-00196 | [Enhance] Support for new sku ECS2110-26T-ME, additional DC power & 6KV surge protection (New BID=2 for 26T-ME) |

**Loader V1.0.0.0 / V0.0.3.4**

|  |  |  |
| --- | --- | --- |
|  | EPR N/A | a. [Enhance] Reduce DRAM operational clock, 400 -> 300 MHz (V0.0.3.4+)b. [Bug] Reverse Port LED lighting - green for 10/100M link, amber for 1000M link (V1.0.0.0+) |

**runtime code modifications:**

**(ECS4100) Runtime V1.2.73.203, Loader V1.0.2.2**

**ECS4100\_V1.2.73.203.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.73.203.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100EC-81 | SNMP: only three snmp community is allowed | EIT |
|  | ECS4100EC-82 | SNMP: snmp-server user add failed when add two private snmp user | EIT |
|  | ES4100EC-93 | Delete exclude-vlan setting;system crashed and show exception. | RD |
|  | ECS4100EC-86 | save config stuck for tens minutes and then reboot auto when save config the second time | EIT |
|  | ECS4100EC-83 | DUT stuck after delete/recreate ip interface and then show ip interface | EIT |
|  | ECS4100EC-88 | RADIUS-Acct:The DUT would hang when process of radius accounting | EIT |

**(ECS4100) Runtime V1.2.72.203, Loader V1.0.2.2**

**ECS4100\_V1.2.72.203.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.72.203.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100EC-78 | DUT console lock and auto reboot after 10 minutes while change management vlan | NTC |
|  | ECS2100EC-14 | update new license for ECS2110 and update cloud mgmt file all module | RD |
|  | ECS4100EC-77 | partner switch cannot detect link change when shutdown/no shutdown 12T in short time and show kernel version erorr | Customer |
|  | ECS4100EC-53 | [Enhancement]Radsec function for TLS over TCP | RD |
|  | ECS4100EC-73 | SW Watchdog Timeout due to thread GVRP\_GROUP(Porting from ECS4100EC-63 to ECS4100\_master | Customer |
|  | ECS4100EC-70 | ERPS delete L3 table code case build error for ECS4100\_master | RD |
|  | ECS4100EC-69 | dying-gasp can not work exclude vlan 1 for ECS4100\_master | TS |
|  | ECS4100EC-18 | [MSTP] configure mstp cause console print error message. | TS |
|  |  | [Enhance]support old and new license. | RD |
|  | ECS4100-52T-00655 | Add "burst-size" cmd for ecs4100\_12ph. | Customer |
|  | ECS4100EC-2 | Add IgniteNet cloud management daemon (mgmtd) on 10 selected models:ECS4100-12T, ECS4100-28T, ECS4100-28P, ECS2100-10P, ECS2100-28PP, ECS2100-28P, ECS2100-10T, ECS2100-28T, ECS4100-12PH, ECS2100-52T. To be consistent with current EdgeCore switches line, the Cloud management will be disabled by default. Customers would enable Cloud themselves. Requires increased BIX file upload buffer (i.e. intermediate firmware for upgrade to Cloud managed one). It was also decided to merge Called-Station-Id commit into this very ticket. | RD |
|  | ECS4100EC-3 | IP Source Guard is filtering PPPoE | Customer |
|  | ECS4100-52T-00677 | Configure logging command failed in provisioning | Customer |

**(ECS4100) Runtime V1.2.44.201, Loader V1.0.2.2**

**ECS4100\_V1.2.44.201.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.44.201.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00655 | open "set burst size" for all board type. | TS |

**(ECS4100) Runtime V1.2.43.201, Loader V1.0.2.2**

**ECS4100\_V1.2.43.201.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.43.201.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00655 | open "set burst size" for all board type. | TS |

**(ECS4100) Runtime V1.2.42.201, Loader V1.0.2.2**

**ECS4100\_V1.2.42.201.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.42.201.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100EC-4 | ERPS will have the loop when interface shutdown/no shutdown in short time. | TS |

**(ECS4100) Runtime V1.2.41.201, Loader V1.0.2.2**

**ECS4100\_V1.2.41.201.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.41.201.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00655 | Policy-map ingress rate-limiting is not accurate, open "burst size" for user configuration to improve rate-limiting. | TS |
|  | ECS4100-52T-00678 | Linux Kernel version display problem with "show version" command. | TS |

**(ECS4100) Runtime V1.2.40.194, Loader V1.0.2.2**

**ECS4100\_V1.2.40.194.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.40.194.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00649 | [NTP server] When the switch reboot and check configuration provision will occur "Fail to set NTP server xxxxx” | TS |
|  | ECS4100-52T-00660 | [IGMP] When the first IGMP query is received, manually remove the IGMP VLAN on the port will trigger an exception. | Customer |
|  | ECS4100-52T-00661 | [Enhancement] Support DHCPSNP filter-only mode | Customer |
|  | ECS4100-52T-00662 | [MVR] The multicast group will not receive multicast data after the expiry time. | Customer |
|  | ECS4100-52T-00663 | show erps vlan-group cause HW watchdog reboot | Customer |
|  | ECS2000-28PP-01047 | HTTP-Download Config and get old config | Customer |

**(ECS4100) Runtime V1.2.39.193, Loader V1.0.2.2**

**ECS4100\_V1.2.39.193.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.39.193.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00658 | [SNMP] SNMP get "diffServPolicyMapName" OID will display does not currently exist. | Customer |
|  | ECS4100-52T-00659 | [ACL] ACL does not filter DHCP packet. | Customer |

**(ECS4100) Runtime V1.2.38.193, Loader V1.0.2.2**

**ECS4100\_V1.2.38.193.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.38.193.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00044 | [Enhance] MVR source port mode, IGMPSNP router port mode - always forward (w/o packet drop) | RD |
|  | ECS4100-52T-00585 | "authentication login tacacs local" does not turn to local account after the tacacs-server setting is removed. (occurs in V1.2.34.184 ~ .37.191) | TS |
|  | ECS4100-52T-00601ECS4100-52T-00616 | ConfigFileMgmt: Got "Unclassified error" while exec "copy sftp file" (file type: 2. opcode) \* SFTP server: Xlight 3.9.0SFTP: Cannot download opcode into DUT, neither IPv4 nor IPv6; but works to download config. | NTC |
|  | ECS4100-52T-00620 | RADIUS: NAS-Port attribute is not carried in Accounting-Request packet, but carried in Access-Request packet. | Customer |
|  | ECS4100-52T-00640 | [Enhance] AAA TACACS: No system-auto privilege authorization following login authentication. | RD |
|  | ECS4100-52T-00641 | ACL's 64th rule does not take effect after it is binding to a port. | Customer |
|  | ECS4100-52T-00643 | [Enhance] ERPS multiple instances - Web support  | RD |
|  | ECS4100-52T-00645 | Enabled both VLAN Trunking and Ingress Filtering, DAI trusted port does not forward unknown-VLAN ARP packets. | RD |
|  | ECS4100-52T-00650 | When the 1st trunk member (active & least port#) is gone, re-learning MAC addresses on the next trunk member causes system reboot (Warning: System reboot by HW Watchdog due to SW Watchdog hang.). | Customer |
|  | ECS4100-52T-00653 | IPSG drops the traffic even though the entries are valid. | Customer |

**(ECS4100) Runtime V1.2.37.191, Loader V1.0.2.2**

**ECS4100\_V1.2.37.191.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.37.191.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00617 | ZTPv6: DUT cannot get bootfile when DHCPv6 server’s lease timer is less than 5 seconds. | NTC |
|  | ECS4100-52T-00623 | Enabled VLAN trunking, DAI is not forwarding unknown VLAN ARP packets. | Customer |
|  | ECS4100-52T-00627 | Enabled VLAN trunking, unknown VLAN MAC addresses are not learned. | Customer |
|  | ECS4100-52T-00628 | DHCP Relay: DHCP packets are always sent to the relay server configured at last. | Customer |
|  | ECS4100-52T-00630 | 1X EAPOL Pass Through is not reset to the default status (Disabled) after "dot1x default" is configured | NTC |
|  | ECS4100-52T-00631 | When the switch responds SNMP replies, it uses one of the egress port’s IP addresses as the source IP, instead of that address on SNMP requests. | Customer |
|  | ECS4100-52T-00633 | DAI does not normally drop ARP packets over IPSG SIP mode. | Customer |
|  | ECS4100-52T-00634 | [Enhance] 12PH supports 60W UPoE (802.3bt compliant) - Phase1Two enhanced items also apply to 802.3at PoE...1. Power Management mode is changed from Pre-Allocated to Dynamic Allocated.2. SNMP reads the 5 error counters of pethPsePortTable in RFC3621 POWER-ETHERNET-MIB - pethPsePort<xxx>Counter := {MPSAbsent(8) | InvalidSignature(11) | PowerDenied(12) | OverLoad(13) | Short(14)} | RD |
|  | ECS4100-52T-00637 | SNMP fails to get lldpXdot1RemoteData(1.0.8802.1.1.2.1.5.32962.1.3) after 249+ days | Customer |
|  | ECS4100-52T-00639 | VLAN-Trunking port will receive packets carrying existent VLANs, which are created after that port is VLAN-Trunking enabled. | NTC |
|  | ECS4100-52T-00252 | 3at PoE Class value (maximum: 4) is incorrectly displayed in 5 on the CLI. | TS |

**(ECS4100) Runtime V1.2.36.191, Loader V1.0.2.2**

**ECS4100\_V1.2.36.191.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.36.191.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00615 | MIB: fileCopyServerInetAddressType description misses the ‘ipv6(2)’ type.*=> Modified MIB file only (LAST-UPDATED "201903080000Z")* | TS |
|  | ECS4100-52T-00638 | ERPS Trap OID is inconsistent between MIB definition and actual packet's.*=> Modified MIB file only (LAST-UPDATED "201903080000Z")* | Customer |
|  |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00600 | TWAMP: Server Start Time in Server Start packet would change when SNTP time is set. | NTC |
|  | ECS4100-52T-00614 | SNMP: DAI mode cannot be changed via SNMP daiVlanArpAclStatus. | Customer |
|  | ECS4100-52T-00618 | SW\_WDT will be triggered (SNMP\_TD task exception) when SNMP retrieves ARP ACL name having 18 and more chars. | TS |
|  | ECS4100-52T-00621 | [Enhance] Trap appends with hostname in var-bind list | Customer |
|  | ECS4100-52T-00622 | [Enhance] DyingGasp trap supports SNMPv3 | Customer |
|  | ECS4100-52T-00629 | [Enhance] Support CLI ‘Discard Input’ (namely SNMP ifInDiscards /IF-MIB) | Customer |
| Test Build V1.01.24.191 |
|  | ECS4100-52T-00588 | Invalid SSHv2 key type (DSA) can be copied to DUT. | NTC |
|  | ECS4100-52T-00602 | ERPS: After shutdown and no shutdown this trunk member ports, DUT cannot forward some VLAN-group data correctly. | NTC |
|  | ECS4100-52T-00603 | ERPS: After we reload this DUT, it cannot forward some VLAN-group data correctly. | NTC |
|  | ECS4100-52T-00610 | [Enhance] HW reworks *(+ dual-power PSU)* to monitor power source *{AC220V | DC12V}* via Reset button contacts *{Released | Pressed}*. SW adds a MIB object to read its state. | Customer |
|  | ECS4100-52T-00611 | 802.1X: Both system-auth-control and eapol-pass-through can be enabled. *(negative, as described in the design spec)* | RD |
|  | ECS4100-52T-00612 | DHCPv6 SNP blocks reply messages from DHCPv6 server when both client and server locate on trust ports. *(No such issue in DHCP SNP)* | Customer |
|  | ECS4100-52T-00613 | ERPS: Mismatched error messages between Device CLI and Cmd Spec while configuring over the maximum # of vlan groups and rings | NTC |

**(ECS4100) Runtime V1.2.35.191, Loader V1.0.2.2**

**ECS4100\_V1.2.35.191.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.35.191.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00416 | [Enhance] DHCP Relay Option 82 status per interface – can be enabled/disabled per-Ethernet & per-VLAN. | Customer |
|  | ECS4100-52T-00541 | [Enhancement] Support to download exception\_log and watchdog\_log. | RD |
|  | ECS4100-52T-00578 | [Enhance] (12Tv2) SW supports notification of thermal temperature rising/falling. HW adds thermal sensor. | RD |
|  | ECS4100-52T-00580 | Support to enable SSH at default | Customer |
|  | ECS4100-52T-00584 | [MVR] the value of Query interval should not be able to set less than the Query max-resp-time. | TS |
|  | ECS4100-52T-00589 | [MVR] proxy-switching should not send back the "leave packet" to the MVR source port which is the last member port. | TS |
|  | ECS4100-52T-00590 | SNMP coldstart/warmstart traps carry invalid IPv6 Loopback address (::1) in the Source IP address. | TS |
|  | ECS4100-52T-00591 | ERPS Open Ring does not flush FDB after the WTR timer is expired. | TS |
|  | ECS4100-52T-00596 | ERPS: DUT cannot forward all VLAN-group data as eanbled ERPS. | NTC |
|  | ECS4100-52T-00609 | Fails to add/delete static mac address via SNMP, however, works well via CLI. *(Occurs in V1.2.31.184~1.2.34.184)* | Customer |

**(ECS4100) Runtime V1.2.34.184, Loader V1.0.2.2**

**ECS4100\_V1.2.34.184.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.34.184.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00514 | [Enhance] ERPS multiple instances. *UI includes CLI and SNMP.* | Customer |
|  | ECS4100-52T-00515 | [Enhance] TWAMP server/reflector plus IPv6 support. *UI includes CLI ~~and SNMP~~.* | Customer |
|  | ECS4100-52T-00574 | ECS4100-series drops the last one of fragmented UDP packets when DHCP snooping is enabled. | Customer |
|  | ECS4100-52T-00577 | Throughput slower than service-policy flow rate after reboot for a while (actually after ARP rate-limit is set and ARP packets are injected) | Customer |
|  | ECS4100-52T-00579 | [MVR] Receiver port stops receiving G-Query packets after it leaves some IP multicast group. | TS |
|  | ECS4100-52T-00581 | Auto Upgrade does not work with DHCP IP. | TS |
|  | ECS2000-28PP-00895 | Use vlan 4094, can’t autoupgrade -- Monitoring | TS |
|  | ECS4100-52T-00586 | Authorization level is incorrect without "authorization exec" setting | TS |
|  | ECS4100-52T-00569 | [Enhance] TACACS+ authorization is already supported. Shall grant the administrator privilege by 'enable' method. | RD |
|  | ECS4100-52T-00563 | [Enhance] XFER copy status messages sharing with CLI and WEB. | RD |
|  | ECS4100-52T-00575 | Modify the locations of spanning-tree commands in CLI running-config. | RD |
|  | ECS4100-52T-00582 | access to wrong array index for swctrl\_station\_move\_trap\_per\_port | RD |
|  | ECS2000-28PP-00874 | If vlan interface enables dhcp and v6 autoconfig, auto upgrade could not find new image | Customer |
| Test Build V1.11.26.184 / 12Tv2 Specific Patch V1.2.30.183\_N1127 |
|  | ECS4100-52T-00551 | [Enhance] SSH supports CTR cipher - upgrade to OpenSSHv7.8p1. *UI includes CLI, SNMP, and WEB.* | Customer |
|  | ECS4100-52T-00564 | The SFTP feature does not work with IPv6 | Customer |
|  | ECS4100-52T-00572 | ECS4100-series SSH key exchange protocol is obsolete | TS |
|  | ECS4100-52T-00559 | [Enhance] TACACS IPv6 support. *UI includes CLI, SNMP, and WEB.* | Customer |
|  | ECS4100-52T-00567 | [Enhance] MVR proxy-switching adds leave-proxy for MVR source port at dynamic mode. | Customer |
|  | ECS4100-52T-00568 | [Enhance] Configurable mgmt. IPv6 address with prefix length up to 126. | Customer |
|  | ECS4100-52T-00576 | [MVR] switch will not forward multicast data from source port to other source port after configured 'Always Forward' mode. | TS |
|  | ECS2000-28PP-00941 | plug in any device will learn on voice vlan and will not age out | Customer |
|  | ECS2000-28PP-00971 | Vlan IP is delivering by DHCP. Execute "ip dhcp dynamic-provision",No reaction for a while and the device will reboot by WDT | TS |
|  | ECS2000-28PP-00984 | Console will freeze while executing "copy startup-config (w/ ‘lldp med-location civic-addr‘ settings) to running-config". | TS |
|  | ECS2000-28PP-00989 | IGMPSNP: Statically registered group cannot be saved successfully. | NTC |

**(ECS4100) Runtime V1.2.33.184, Loader V1.0.2.2**

**ECS4100\_V1.2.33.184.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.33.184.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00540 | If dynamic-provision configuration include dynamic-provision setting again, it will let the function to loop | TS |
|  | ECS4100-52T-00553 | ERPS WTR timer should support range 1 - 12 minutes | TS |
|  | ECS4100-52T-00562 | The STP loopback detection fails after port shutdown / no shutdown | Customer |
|  | ECS4100-52T-00565 | Switch doesn't support this command "mvr source-port-mode forward" | TS |
|  | ECS4100-52T-00566 | (ECS4100-12PH) switch fail to deliver power due to PoE MCU configuration data is damaged | RD |
|  | ECS4100-52T-00571 | [Enhancement] SW WatchDog monitor GVRP\_GROUP | RD |
|  | ECS4100-52T-00573 | [Enhance] Kernel immediately dumps the exception messages on the console. | RD |
|  | ~~ECS2000-28PP-00945~~ | ~~Customized(Non-Std) LLDP broadcast packets (DA: FFFFFFFFFFFF & EtherType: 88CC) cannot be flooding to other ports~~ *~~-> ECS2100 only~~* | ~~Customer~~ |
|  | ECS2000-28PP-00969 | Upgrade from v1.2.2.20 to v1.2.2.21, Enable IP dhcp dynamic-provision (ZTP funciton). It fails to download config file. | TS |
|  | ECS2000-28PP-00980 | Switch will warm-start when repeatedly retrieve/release DHCP IP (lease time: 60s) | Customer |
| V1.2.32.184 |
|  | ECS4100-52T-00570 | MVR didn't work when you disable "mvr proxy-switching". | Customer |

**(ECS4100) Runtime V1.2.32.184, Loader V1.0.2.2**

**ECS4100\_V1.2.32.184.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.32.184.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00468extension | NOTIFICATION-TYPE: sFlowEnableTrap/sFlowDisableTrap are added. However, OBJECTS: trapVarOwnerName is missed (no definition). | RD |
|  | ECS4100-52T-00544 | ZTPv6: When we configure mutiple IPV6 interface, DUT fail to get this bootfile. | NTC |
|  | ECS4100-52T-00546 | ZTP - It's failed to request configuration file. (due to link-local IP address) | TS |
|  | ECS4100-52T-00548 | DHCPv6: After change IPV6 with dhcp mode from AutoConfig, DUT cannot get DHCP ip address. | NTC |
|  | ECS4100-52T-00560 | MAC ACL for PPPoE Session EtherType 0x8864 ("permit any any ethertype 8864”) does not work | Customer |
|  | ECS2000-28PP-00939 | ip phone cannot join back to voice vlan when ip changed | Customer |
|  | ECS2000-28PP-00941 | plug in any device will learn on voice vlan and will not age out | Customer |
|  | ECS2000-28PP-00956 | When enabled IGMP snooping plus querier, the console will hang after setting the VLAN suspended after 5 minutes | Customer |

**(ECS4100) Runtime V1.2.31.184, Loader V1.0.2.2**

**ECS4100\_V1.2.31.184.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.31.184.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00497 | "show mac-address-table a?" display incomplete | TS |
|  | ECS4100-52T-00499 | [Enhance] CLI: XML command without action shall not be convert to a completed command | RD |
|  | ECS4100-52T-00500 | CLI: XML convert to CLI command tree, same prefix parameter will wrong on enter [TAB]/[?] | RD |
|  | ECS4100-52T-00521 | ZTPv6: Repetitions of restarting IPv6 DHCP client (100 times); CLI halts and then system reboots. | NTC |
|  | ES4528BH2-HPoE-0815-EC-00753, 795, 797 | ZTPv6: After DUT fail to get bootfile, CLI show exception.DHCPv6: After restart DHCPv6 client on DUT continuously, system halts and dumps exception.ZTPv6: After restart this ZTPv6 for 10 times, DUT failed to get IPV6 address. | NTCNTCNTC |
|  | ECS4100-52T-00531 | IPv6AddrConfig: IPv6 neighbor list is empty after save and reboot when set ipv6 link local address. | NTC |
|  | ECS4100-52T-00533 | IPv6-MLD-SNP-0180: Port 2 receive 2 times of done report packets when disable ipv6 mld snooping | NTC |
|  | NA | MVR leave packet is not forwarded to source port. | RD |
|  | ECS4100-52T-00535 | [Enhance] Re-design Rx Loss Interrupt task procedure | RD |
|  | ECS4100-52T-00538 | Wrong behavior after plugging in the unknown transceiver, e.g. checksum error | TS |
|  | ECS4100-52T-00552 | NTP: support to add or delete NTP IPv4/IPv6/hostname servers in SNMP private MIB | RD |
|  | ECS4100-52T-00554 | The ERPS convergence time more than 600ms, shall be less than 50ms | TS |
|  | ECS4100-52T-00558 | (MSTP\_issue)MST configuration of spanning-tree is deleted by device after reboot in 1.2.28.183 | TS |
|  | ECS2000-28PP-00878 | snmpwalk .1.3.6.1.2.1.4.22 (ipNetToMediaTable) then error is displayed (Error: OID not increasing: ...) | Customer |
|  | ECS2000-28PP-00950 | NTP server cannot be deleted if set in WEB, however, CLI works well. | Customer |

**(ECS4100) Runtime V1.2.30.183, Loader V1.0.2.2**

**ECS4100\_V1.2.30.183\_N1011.bix is a specific patch for 12Tv2**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00535 | [Enhance] Re-design Rx Loss Interrupt task procedure | RD |
|  | ECS4100-52T-00554 | The ERPS convergence time more than 600ms, shall be less than 50ms | TS |

**(ECS4100) Runtime V1.2.30.183, Loader V1.0.2.2**

**ECS4100\_V1.2.30.183.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

**ECS4100-12PH\_V1.2.30.183.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00434 | [Enhancement] Support sticky mac (SNMP/MIB) | Customer |
|  | ECS4100-52T-00498 | PortSecurity, aging-time expired & max-mac-count reached, learned/secured MAC addresses do not disappear when intrusion traffic is large enough. | Customer |
|  | ECS4100-52T-00510 | ImageDownload: Response "Unsupported version number. Not updated.", but announce "Success" | NTC |
|  | ECS4100-52T-00511 | When the switch acts as DHCP server, the inccoming DHCP Discover packet will cause memory leakage. | Customer |
|  | ECS4100-52T-00513 | [Enhancement] sflow enabled/disabled syslog for jio | TS |
|  | ECS4100-52T-00517 | (Critical) ECS4100 series - Copper part of Combo Copper/Fiber port can't link up*=> Occurs in V1.2.29.183 only* | TS |
|  | ECS4100-52T-00518ES4528BH2-HPoE-0815-EC-00768 | The switch does not request IPv6 address(DHCP Mode) after rebooting.After the switch performs ZTP for IPv6 to get/apply the remote configuration file, the remote "ipv6 address dhcp" does not take effect. | TSTS |
|  | ECS4100-52T-00520ES4528BH2-HPoE-0815-EC-00771 | ZTPv6: DUT failed to get bootfile after reload this DUT.DUT is unable restart ipv6 dynamic provision process after it's failed to get config from TFTP server | NTCTS |
|  | ~~ECS4100-52T-00521~~ES4528BH2-HPoE-0815-EC-00773 | ~~ZTPv6: Repetitions of restarting IPv6 DHCP client (100 times); CLI halts and then system reboots.~~the switch does not request ipv6 address after configure ipv6 address DHCP | ~~NTC~~TS |
|  | ECS4100-52T-00523 | IGMPSNP: While auto test is running, the DUT will hang with the error message "Fail to allocate buffer from pool". | NTC |
|  | ECS4100-52T-00525ES4528BH2-...-EC-00769 | Can't get the maximum management ip if the vlan interface gets ipv6 interface by autoconfig. | TS |
|  | ECS4100-52T-00526ES4528BH2-...-EC-00772 | The IPv6 information is incorrect at "show run interface vlan id 1" output. However, correct at “show run”. | TS |
|  | ECS4100-52T-00527ES4528BH2-...-EC-00775 | “show ipv6 interface “ displays "AUTOCONFIG" even it is DHCP mode. | TS |
|  | ECS4100-52T-00529 | [Enhance] Recover is\_rx\_los\_implemented checking for SFP transceivers | RD |
|  | ECS4100-52T-00534 | NTP: new show commands to display more detailed information from NTP daemon *+1) show ntp status* *+2) show ntp peer-status [{ip-address | host-name}]* *+3) show ntp statistics peer {ip-address | host-name}* | RD |
|  | ECS2000-28PP-00877 | One of vlans request ip, it will let other vlan request at the same time. | TS |
|  | ECS2000-28PP-00898 | In the source guard function with DHCP snooping linkage, part of the source IP address assigned by DHCP becomes Block | Customer |
|  | ECS2000-28PP-00907 | The lifetime of the IPv6 address shows wrong | Customer |
|  | ECS2000-28PP-00908 | suspended vlan sends out dhcp discover packet | Customer |
|  | ECS2000-28PP-00913 | [MLDSNP] when added a static mrouter port that the switch will not sent out the report by proxy-reporting. | Customer |
|  | ECS2000-28PP-00914 | [IGMPSNP] "dynamic" mrouter-forward-mode will forward multicast traffic to the another mrouter port directly. | TS |
|  | ECS2000-28PP-00919 | [MLDSNP] switch will removed the MLD entry when it received another MLD Query(lower IP address). | Customer |
|  | ECS2000-28PP-00922 | [MLDSNP] After switch received the MLDv1 Query then it will start to send abnormal MLD Query | Customer |
| V1.2.28.183 |
|  | ECS4100-52T-00484 | number of igmpsnp and mldsnp groups is incorrect | TS |
|  | ECS4100-52T-00494 | After calendar is set to some specific time (system bootup time, actually), the system time does not sync up with NTP server anymore. | TS |

**(ECS4100) Runtime V1.2.29.183, Loader V1.0.2.2**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00097 | Support IPv6 static route | Customer |
|  | ECS4100-52T-00442ECS4100-52T-00489 | DHCPv6 options and ZTP for IPv6DUID Type 2 (DUID-EN) for DHCPv6 client | CustomerCustomer |
|  | ECS4100-52T-00465 | Reachability to Multiple TACACS server | Customer |
|  | ECS4100-52T-00466 | Time-Range configuration could not be deleted. | TS |
|  | ECS4100-52T-00490extension | [Enance] Configurable IPv4 /31 subnet for Mgmt IP. However, not allowed to configure IPv6 address with prefix length over 64. | Customer |
|  | ECS4100-52T-00492 | [Enhance] Gets port status to link-down on GPON module insertion, which causes link-up first. | RD |
|  | ECS4100-52T-00503 | NTP: The DUT doesn't send the NTP client packets when enable authenticate and save/reboot. | NTC |
|  | ECS4100-52T-00505 | TACACS: global secret key overwrites all servers' secret keys, no matter iif single or multiple (V1.2.29.183+) TACACS servers are supported | EIT |
|  | ECS4100-52T-00506 | ZTP can’t autorun. (necessary to press any key to trigger the process) | TS |
|  | ECS4100-52T-00508ECS4100-52T-00509 | port security traffic blockport security can't learn mac when sticky mac + network-access aging*=> Occurs in V1.2.28.183 only* | TSTS |
|  | ECS2000-28PP-00878 | snmpwalk .1.3.6.1.2.1.4.22 (ipNetToMediaTable) then error is displayed (Error: OID not increasing: ...) | Customer |
|  | ECS2000-28PP-00902 | After enable the proxy-reporting of IGMP/MLD,the general query didn't flood to all of ports | Customer |
|  | ECS2000-28PP-00904 | When the "mrouter-forward-mode" is dynamic, the client bellowing static mrouter port isn't in group table | Customer |
|  | ECS2000-28PP-00912ECS2000-28PP-00911ECS2000-28PP-00894 | MAC ACL counter does not work when it is bound to time-rangeMAC ACL(3rules) with time-range & counter, but counter can’t workMAC ACL with time-range(2rules) could not work well for counter setting | CustomerCustomerCustomer |
| V1.2.23.182 |
|  | ECS2000-28PP-00866 | switch send out untagged report when enabled MLD snooping | Customer |

**(ECS4100) Runtime V1.2.28.183, Loader V1.0.2.2**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ~~ECS4100-52T-00097~~ | ~~Support IPv6 static route~~ | ~~Customer~~ |
|  | ECS4100-52T-00429 | (28TC-F) Support for Fan speed control ~~and system reboot w/ Reset button~~ (new BID=16) | RD |
|  | ECS4100-52T-00256 | [Enhance] ACL supports to filter MAC and IPv4 fields in an ACE (at TCAM Mixed-MAC-IPv4 mode).*=> targets for PPPoE Sesstion packet (EtherType 0x8864) carrying IPv4 header* | Customer |
|  | ECS4100-52T-00412 | DDM: Set media-type to "spf-forced 100fx", but link status and threshold is still1000 sfp. | NTC |
|  | ECS4100-52T-00434 | [Enhancement] Support sticky mac (CLI & Web) | Customer |
|  | ECS4100-52T-00435 | [Enhancement] Extend the characters of remote-id and circuit-id for DHCPSNP option82 and PPPoEIA | Customer |
|  | ECS4100-52T-00439 | [Enhance] LLDP IPv6 Support (LLDP Management-IP-Address TLV for IPv4/v6) | Customer |
|  | ECS4100-52T-00456Simba-Common-00263 | when IPACL entry is full and bind to a port, that port can't show hardware counter by WebUIWebUI display white screen when apply ACL counter more than 10 ACE | TSCustomer |
|  | ECS4100-52T-00457 | When TACACS server key gets more than 48 chars, switch will be warm-started by SW watchdog. | TS |
|  | ECS4100-52T-00458 | IPv6 ACL can't work well for the source-port destination-port filter | TS |
|  | ECS4100-52T-00460,476,477 | We receive snmp inform and show run, then freeze | TS |
|  | ECS4100-52T-00461 | When we want to set "clock timezone-predefined" by telnet, then switch crash. | TS |
|  | ECS4100-52T-00463 | [enhance] TransceiverAbsentTrap & TransceiverPresentTrap for Jio | RD |
|  | ECS4100-52T-00464 | ERPS trap enhancement for Jio | RD |
|  | ECS4100-52T-00467 | Can't trigger the swSmtpConnFailure trap. | TS |
|  | ECS4100-52T-00468 | [Enhancement] sflow enabled/disabled trap for jio | RD |
|  | ECS4100-52T-00469ECS4100-52T-00470ECS4100-52T-00471 | NTP: The DUT will crash when enable ntp client with authenticate and save/reboot.NTP: The DUT will crash when enable ntp client and set the NTP server after save/reboot.Get error message when we configure ntp server and client | NTCNTCTS |
|  | ECS4100-52T-00472 | NTPv4 have long latency issue | RD |
|  | ECS4100-52T-00474 | [12Tv2] : insert 100sfp into port11&12 and change media-type will cause link down. | NTC |
|  | ECS4100-52T-00478 | NTP: Need to remove the polling time information on NTP version 4. | NTC |
|  | ECS4100-52T-00479 | (12Tv2) Support to switch Port 11/12 SFP interface between SERDES and SGMII modes (on RTK shell). | RD |
|  | ECS4100-52T-00481 | [12Tv2] Source GPON transceiver (SPS-34-24T-HP-TDFO-RR) EEPROM info. partially missing or overlapped with other SFP | RD |
|  | ECS4100-52T-00482 | Avoid new HW board from being downloaded old runtime image, in which the new BID is not available. | RD |
|  | ECS4100-52T-00483 | clear ip igmp snooping groups dynamic does not delete all multicast groups | TS |
|  | ECS4100-52T-00485 | clear ipv6 mld snooping groups dynamic does not delete all multicast groups | TS |
|  | ECS4100-52T-00486 | maximum groups of mld snooping should be 256 | TS |
|  | ECS4100-52T-00487 | "ipv6 mld snooping unknown-multicast mode flood " malfunction | TS |
|  | ECS4100-52T-00488 | Debug message "Find new version" is printed while copying runtime image with newer version. | RD |
|  | ECS4100-52T-00490 | [Enance] Configurable IPv4 /31 and IPv6 /127 subnets for Mgmt IP addresses | Customer |
|  | ECS4100-52T-00491 | ECS4100-12Tv2 can't be rebooted on Linux shell*=> CPLD code upgrade to ‘VER0102180801’* | TS |
|  | ECS4100-52T-00493 | Can set the to history command to port-channel , but we can't remove it via port-channel interface. | Customer |
|  | ECS4100-52T-00501 | IPv6-AddrConfig-0670: No static neighbors exist in ipv6 neighbour table after adding 10 static ones | EIT |
|  | ~~ECS4100-52T-00502~~ | ~~A tacacs-authenticated user gets the privilege level no matter if 'authorization exec' is enabled.~~ | ~~Customer~~ |
|  | ECS2000-28PP-00890 | WebGUI: ACE entry for Hardware Counter does not have the ‘CoS’ information. | Customer |
|  | ECS2000-28PP-00892 | Static Mac-address-table entry won't work on lacp interface after reboot | Customer |
|  | ECS2000-28PP-00903 | If the IGMP entries is full, only one client can join to multicast stream well. | Customer |

**(ECS4100) Runtime V1.2.27.183, Loader V1.0.2.1**

**ECS4100\_V1.2.27.183.bix is for 52T/26TX/28T/12T/28P/52P/28TC/12Tv2**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00124 | MVR: MVR VLAN can overlapped on each domain. | NTC |
|  | ECS4100-52T-00309 | Too lot ARP request make ping switch packet loss | TS |
|  | ECS4100-52T-00397 | SW Enhance NTPv4 | Customer |
|  | ECS4100-52T-00427 | failed to bind egress ACL when apply output service-policy first | Customer |
|  | ECS4100-52T-00428 | DHCP snooping max-number no log | TS |
|  | ECS4100-52T-00436ECS4100-52T-00454ECS4100-52T-00462 | (12Tv2) Support for board re-layout (new BID=17)[12Tv2] Support CPLD UART functions for ext. GPIO control & SFP DDM read.[12Tv2] Display CPLD Version at CLI "show version" output. | RDRDRD |
|  | ECS4100-52T-00437 | [ITUS] If a config file is more than 100K, "dir" displays the extra leading separator ',' in "Size (bytes)". | Customer |
|  | ECS4100-52T-00438(#355 ext) | [ITUS] Remove Pool No. 11 ‘D6S D6E’ from “show access-list tcam-utilization” output as specified "tcam allocation extend-mac-vlan“. | Customer |
|  | ECS4100-52T-00440 | JumboFrame: The DUT will an exception occurs when enable jumbo frame and send the maximum packet size. | NTC |
|  | ECS4100-52T-00452 | Missing 'sftp' option for "copy running-config" & "copy startup-config" command | RD |
|  | ECS4100-52T-00455 | [WEB] There is no place to configure ERPS VLAN-inclusion or exclusion. | RD |
|  | ECS4100-52T-00459 | [enhance] Add smart pair Web page | RD |
| Test Build V1.07.19.183 (Code base V1.2.24.182, instead of V1.2.26.182) |
|  | ECS4100-52T-00451 | STP state will flapping (non-fwd/fwd) when switch received the SyncE packet. | Customer |
| V1.2.16.181 |
|  | ECS4100-52T-00335 | MVR status is at inactive, even if Receiver and Source ports are link up. | TS |

**(ECS4100) Runtime V1.2.26.182, Loader V1.0.2.0**

**ECS4100\_V1.2.26.182.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.26.182.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00075 | QinQ: We cannot enable/disable to drop this "matched service-vlan untagg/all" packets from WEB and MIB. | NTC |
|  | ECS4100-52T-00382 | [Enhance] Support Active/Standby static LAG - Smart Pair | RD |
|  | ECS4100-52T-00403ECS4100-52T-00404 | SmartPair: The time of Rx Lose is over then 50 ms that is not match customer requirement.SmartPair: wait-to-restore delay is over then 30 secs when inject packets with VLAN 4094 tag. | NTCNTC |
|  | ECS4100-52T-00421 | [Enhance] Bootloader automatically boots the second one when the startup runtime is corrupted.*=> “Startup runtime is corrupted.", Syslog message recorded at runtime* | RD |
|  | ECS4100-52T-00429 | (28TC-F) Support for ~~Fan speed control~~ ~~and~~ system reboot w/ Reset button (new BID=16) | RD |
|  | ECS4100-52T-00430 | [WEB] Administration > ERPS, Configure Details page may be blank. | RD |
|  | ECS4100-52T-00431 | To apply an incremental patch "patch018" of "00004313-SDK\_V2.1.4.53590\_Patch" for SGMII setting | RD |
|  | ECS4100-52T-00432 | Cannot modify user's privilege and create/delete user via SNMP userAuthTable. | Customer |

**(ECS4100) Runtime V1.2.25.182, Loader V1.0.0.5 / V1.0.1.9**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00058 | 802.1X-DACL: The ACL rule can not binding on the port when re-create the ACL rule. | NTC |
|  | ECS4100-52T-00074 | WEB: We cannot set VLAN-translation ingress/egress setting individually. | NTC |
|  | ECS4100-52T-00143 | DiffServ[MIB]The description of diffServClassMapAttachCtlElementIndex contains error words | NTC |
|  | ECS4100-52T-00237 | DHCP Server: We cannot modify any setting of existing pool from WEB. | NTC |
|  | ECS4100-52T-00344ECS4100-52T-00386ECS4100-52T-00391 | 802.1ag-CFM-1260 1270: DUT shall send out 100 tagged LTR from DUTPA when LTM with destination is Down-ME 1 CFM: DUT should not reply tagged LTR as it is untagged VLAN member.CFM: When MEP/MIP is untagged VLAN member, it should not send out tagged LTM/LTR frames. | EITNTCNTC |
|  | ECS4100-52T-00359 | Upload wrong format license file make switch stuck. | TS |
|  | ~~ECS4100-52T-00382~~ | ~~[Enhance] Support Active/Standby static LAG - Smart Pair~~ | ~~RD~~ |
|  | ~~ECS4100-52T-00403~~~~ECS4100-52T-00404~~ | ~~SmartPair: The time of Rx Lose is over then 50 ms that is not match customer requirement.~~~~SmartPair: wait-to-restore delay is over then 30 secs when inject packets with VLAN 4094 tag.~~ | ~~NTC~~~~NTC~~ |
|  | ECS4100-52T-00383 | [Enhance] Support ERPS for open ring & VLAN excluded/included on ring port | RD |
|  | ECS4100-52T-00413 | After sw\_wdt process is killed on Kernel shell and system is restarted, the syslog message is incorrect for ‘warmStart’, should be ‘coldStart’. | RD |
|  | ECS4100-52T-00414 | [Enhance] sFlow with no time limit | RD |
|  | ECS4100-52T-00415 | SNMP: We can configure redistribute OSPF/BGP by ripRedistributeEntry. | NTC |
|  | ECS4100-52T-00417 | LACP: In "show running", we should remove partner mode setting if we didn't write this config | Customer |
|  | ECS4100-52T-00418 | Switch does not forward the ICMP packet (DA=224.0.0.5) when IGMPSNP/MVR is enabled. | Customer |
|  | ECS4100-52T-00419 | after reboot will fail to config remote-id and circuit-id of option82 and PPPoEIA with space in string | Customer |
|  | ECS4100-52T-00420 | PortSecurity: The DUT cannot send the port security trap when the packet size is over then 1600. | NTC |
|  | ECS4100-52T-00422 | [Enhancement]Force port link-down be detected if rx los interrupt is detected | RD |
|  | ECS4100-52T-00423 | After reboot LAG not calculate on MSTP | TS |
|  | ECS4100-52T-00424 | ECS4100 port security does not learn MAC address which ethertype of pkt is 0x9000 | TS |
|  | ECS4100-52T-00426 | removes selective qinq match cause exception | RD |
|  | ECS2000-28PP-00869 | After having bound mac acl and time range to port, no command to remove time range rule. | Customer |
|  | ECS2000-28PP-00870 | When ACL is bound to port with counter and then it is updated, the ACL counter does not function. | Customer |
|  | Simba-Common-00133 | SNTP: Timezone is EU, summer time doesn't end at the last sunday of October every year | NTC |
|  | Simba-Common-00221 | TACACS+Acct-0080:Interim value and Accounting Stop value not find in Accounting log | EIT |
|  | Simba-Common-00222 | Fail to telnet EC switch(ECS4120) from Cisco device | Customer |
| V1.2.19.182 |
|  | ECS4100-52T-00315 | WebHelp: Lost baudrate 57600 on WebHelp. | NTC |
|  | ECS4100-52T-00316 | WebHelp: "Sets the IPv4 address for up to three time servers." shall be removed from NTP. | NTC |
|  | ECS4100-52T-00320 | WebHelp: Please remove "(Range: 25-28)" from "Interface > Port > Transceiver" because no all SFP ports No. are "25-28". | NTC |
| V1.2.13.174 |
|  | ECS4100-52T-00257ECS4100-52T-00254 | Enlarge the IGMP packet's limitation on CPU.Enhance dev\_nicdrv for IGMP performance (burst with 256 igmp packets) | CustomerRD |
| V1.2.3.173 |
|  | ECS4100-52T-00166 | IPv6-SNMP-0050,0060:set ipv6 address and ping from pc failed | EIT |

**(ECS4100) Runtime V1.2.24.182, Loader V1.0.0.5 / V1.0.1.9**

**ECS4100\_V1.2.24.182.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.24.182.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00383 | REMOVED - [Enhance] Support ERPS for open ring & VLAN excluded/included on ring port | RD |
|  | ECS4100-52T-00382 | REMOVED - [Enhance] Support Active/Standby static LAG - Smart Pair | RD |

**(ECS4100) Runtime V1.2.23.182, Loader V1.0.0.5 / V1.0.1.9**

**ECS4100\_V1.2.23.182.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.23.182.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00176 | system name was changed when configure interface vlan ip address | Customer |
|  | ECS4100-52T-00185 | RIP: There is no ripMgt in private MIB. | NTC |
|  | ECS4100-52T-00258 | [Enhance] support ATC. | Customer |
|  | ECS4100-52T-00306 | RSTP path cost will be fixed when static port-channel link up/down | TS |
|  | ECS4100-52T-00310 | LLDP web:LLDP remote port/trunk "port id" information display in web is not correct | EIT |
|  | ECS4100-52T-00355,406 | Add a TCAM allocate increase mac-based-vlan entries to 256. | TS |
|  | ECS4100-52T-00361 | CLI: DEV\_SWDRV\_GetPortFlowCtrl(): Line = 6868 , error\_id=5 | NTC |
|  | ECS4100-52T-00387ECS4100-52T-00345 | CFM: DUT should not learn aged LTR to linktrace cache.802.1ag-CFM-1290: LTR recorded in linktrace-cache table when Inject 100 aged LTR from DUTPA | NTCEIT |
|  | ECS4100-52T-00388ECS4100-52T-00395ECS4100-52T-00341 | CFM: The transmission interval of LBM and DMM is incorrect.CFM: DUT cannot send out correct LBM packet count.802.1ag-CFM-0210: DUT only send out 40 LBM packets when transmit LBM with count 100 | NTCNTCEIT |
|  | ECS4100-52T-00394 | If using Console login failed, the syslog could not send the syslog trap. | TS |
|  | ECS4100-52T-00396 | ZTP function, switch will freeze during configuration provision.*(occurs in v1.2.16.181~v1.2.22.182)* | TS |
|  | ECS4100-52T-00398 | Log message in "show log flash" is cleared in case unplug power cord | Customer |
|  | ECS4100-52T-00399 | 1QVLAN: DUT does not reject to delete the native VLAN by WEB, it cause PC cannot ping to DUT. | NTC |
|  | ECS4100-52T-00401 | switch send out untagged report when enabled MLD snooping | TS |
|  | ECS4100-52T-00147ECS4100-52T-00402 | [enhance] critical section of SW watchdog[enhance] improve behavior of DEV\_NICDRV\_GATEWAY\_SendPacketByPortList | RDRD |
|  | ECS4100-52T-00407ECS4100-52T-00408 | The BPDU sending time is not stable.Sending the BUDU time will have delay when client to join or leave the multicast group. | CustomerCustomer |
|  | ECS4100-52T-00409 | CFM: When MEP receive some error CCM frames, the error/RX CCM count is incorrect. | NTC |
|  | ECS2000-28PP-00863 | OSPF can specify to delete route information via WebUI | Customer |
|  | ECS2000-28PP-00864 | LA instantaneous interruption occurred when copy running-config to startup-config | Customer |
| V1.2.19.182 |
|  | ECS4100-52T-00167 | port security : the switch learning mac adresses and discards the first packets. | Customer |
| V1.2.10.174 |
|  | ECS4100-52T-00196 | CFM: DUT should reject to set this same MEP\_ID with remote MEP. | NTC |
|  | ECS4100-52T-00242 | CFM: DUT does not reject to set remote MEP as local MEP in same domain. | NTC |
| V1.2.7.173 |
|  | ECS4100-52T-00164,214, 366ECS4100-52T-00169,238 | RMON2: Can not set/get RMON2-MIB ‘trapDestTable’ objects (trapDestOwner, trapDestStatus, ...)*=> Removed trapDestTable (1.3.6.1.2.1.16.19.13) because deprecated years ago.* | EITNTC |
| V1.2.5.173 |
|  | ECS4100-52T-00182 | Web:RIP: DUT doesn't support OSPF, but can configure RIP redistribute as OSPF on Web page for DUT. | EIT |
|  | ECS4100-52T-00183 | Web:RIP: Information about sending RIP version and Receiving RIP version from Web page is not same as that from CLI. | EIT |
|  | ECS4100-52T-00161,189  | Web-1QVLAN-0020:delete all vlan didnot successfully | EIT |
| V1.2.3.173 |
|  | ECS4100-52T-00134 | LLDP-MED: capabilities TLV transmission shall be enabled first and disabled last relative to other MED TLVs | RD |
| V1.2.2.172 |
|  | ECS4100-52T-00158 | PPPoE-IA-0090:DUT not add new circuit id and remote id | EIT |
| V1.2.0.172 |
|  | ECS4100-52T-00116,117 | [Enhancement] Support IPv6 ND snooping function, incl. SNMP/MIB | Customer |

**(ECS4100) Runtime V1.2.22.182, Loader V1.0.0.5 / V1.0.1.8**

**ECS4100\_V1.2.22.182.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.22.182.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00383 | [Enhance] Support ERPS for open ring & VLAN excluded/included on ring port | RD |
|  | ECS4100-52T-00382 | [Enhance] Support Active/Standby static LAG - Smart Pair | RD |
|  | ECS4100-52T-00377 | Private MIB misses the var-bind defintions of thermal temperature rising/falling traps. | RD |
|  | ECS4100-52T-00367 | PoE help Web page is copy from ECS2100-series | TS |
|  | ECS4100-52T-00275 | L2Switch: Threshold is only 100Mbps when media-type is changed from 100fx to 1000sfp. | NTC |
|  | ECS4100-52T-00199 | IPv4-RemotePing-0260: DUT not drop icmp type 13 packets | EIT |
|  | ECS4100-52T-00034 | IPv6-MLD-SNP: Well-known packets can not be flooded when input unknown multicast data first. | NTC |
| V1.2.5.173 |
|  | ECS4100-52T-00165 | DHCPSnoping-0370:"Fail to find egress port, drop" were not record on Log Information. | EIT |
|  | ECS4100-52T-00170 | DHCP-SNP: When DUT detect this even "Failed to classify DHCP packet", it display incorrect log. | NTC |

**(ECS4100) Runtime V1.2.21.182, Loader V1.0.0.5 / V1.0.1.8**

**ECS4100\_V1.2.21.182.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.21.182.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| V1.04.30.182 |
|  | ECS4100-52T-00373 | STP Alternate port does not discard VLAN tagged BPDU packets | Customer |
|  | ECS4100-52T-00190 | Stacking:can ping to client's gateway but cannot ping to client | TS |
| V1.2.19.182 |
|  | ECS2000-28PP-00842 | After delete vlan on Web, ip address loss on this vlan | TS |
| V1.2.16.181 |
|  | ECS4100-52T-00246 | Correct the PoE budget of 28P and 52P | RD |
|  | ECS4100-52T-00281 | [ECS4100-28P]PoE: When PD request total mainpower over 310W, PSE will cut the power off. | NTC |

**(ECS4100) Runtime V1.2.20.182, Loader V1.0.0.5 / V1.0.1.8**

**ECS4100\_V1.2.20.182.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.20.182.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00376 | [Enhance] ERPS core incorporates with SFP RX\_LOS interrupt support. | RD |
| V1.2.19.182 |
|  | ECS4100-52T-00167 | port security : the switch learning mac adresses and discards the first packets. | Customer |
| V1.2.16.181 |
|  | ECS4100-52T-00274 | PoE: There is no PoE help web page. | NTC |
| V1.2.15.181 |
|  | ECS4100-52T-00302 | Enhancement:If project support MSTP, setting chip as MSTP mode in initial phase. | RD |
| V1.2.14.181 |
|  | ECS4100-52T-00236ECS4100-52T-00262 | CustomerInfo: User can not login the DUT by https session.HTTPS: Can not establish HTTPS connection. | NTCNTC |
| V1.2.13.174 |
|  | ECS4100-52T-00267 | MAC-thrashing: When the action mode is change to Port-disable from stop-learning, this Mac-thrashing cannot work normally. | NTC |
|  | ECS4100-52T-00356 | 50 mac-address remained in mac table even if clear all mac table. | TS |
| V1.2.7.173 |
|  | ECS4100-52T-00197 | [IGMP filter] the multicast traffic does not match rule, but it still will be forwarded. | Customer |
|  | ECS4100-52T-00203 | Static port-channel cause loopback detection enable global failed | TS |
| V1.2.3.173 |
|  | ECS4100-52T-00141 | snmpEngineTime didn't reset the value even switch reboot | Customer |

**(ECS4100) Runtime V1.2.19.182, Loader V1.0.0.5 / V1.0.1.8**

**ECS4100\_V1.2.19.182.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.19.182.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00369 | (28TC-ITUS) Turn to use ECS4100-28TC as Vnet4524G (new BID=15) | RD |
|  | ECS4100-52T-00374 | [Enhance] Unify DIAG LED lighting - Green blinking /Loader(init) then Green solid /Runtime(system-boot-up). | RD |
|  | ECS4100-52T-00375 | [Enhance] Unify PWR LED lighting - Green solid from Loader(init) till Runtime(system-boot-up). | RD |
|  | ECS4100-52T-00354 | After disable then enable vlan on Web, vlan interface link down | TS |
|  | ECS4100-52T-00307 | [enhance] support simple chinese web page, web help page. | RD |
|  | ECS2000-28PP-00847 | RIP: After disable/enable vlan, the statistic value always display 750251720 on "show ip protocol rip" | TS |
|  | ECS2100-10P-ACN-00117 | assign ip to management vlan via SNMP failed | Customer |
|  | ES4528BH2-HPoE-0815-EC-00611 | [enhance] Use HW watchdog to monitor SW watchdog (When SW watchdog hangs, HW watchdog will restart the device intead.) | RD |

**(ECS4100) Runtime V1.2.18.182, Loader V1.0.0.5 / V1.0.1.7**

**ECS4100\_V1.2.18.182.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-28T-38IK-00001 | [enhancement] remove cli "show license file" command | Customer |
|  | ECS4100-52T-00371 | [Enhance] Unify Port LED lighting - <Link> LD port-disable: Green<0.5s>Amber; <PoE> Powering: Amber | Customer |

**(ECS4100) Runtime V1.2.17.181, Loader V1.0.1.7**

**ECS4100-12PH\_V1.2.17.181.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00368 | (12PH) PoE fails to power inrush while system booting from Loader V1.0.1.7 | RD |

**(ECS4100) Runtime V1.2.17.181, Loader V1.0.0.5 / V1.0.1.7**

**ECS4100\_V1.2.17.181.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.17.181.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00274 | PoE: There is no PoE help web page. | NTC |
|  | ECS4100-52T-00358 | LED: 10G ports of ECS4100-26TX are always off.\* Updated PS2 & Added PS5 for “PORT LED DEFINITIONS” on last page. | NTC |
|  | ECS4100-52T-00362 | FAN: The speed of FAN No. 1-3 will not raise even the temperature is up to 99. | NTC |
|  | ECS4100-52T-00363 | Default configure each interface will be set to "ethernet cfm port-enable" | TS |
|  | ECS4100-52T-00364 | [Enhancement] Revise ‘insmod module ...’ messages of ‘running rc’ while system booting. | RD |
| Test Build V1.03.14.181 |
|  | ECS4100-52T-00360 | MVR/IGMPSNP function to cause memory leak. | Customer |

**(ECS4100) Runtime V1.2.16.181, Loader V1.0.0.5 / V1.0.1.7**

**ECS4100\_V1.2.16.181.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.16.181.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00326 | (28P-ITUS) Add CLI command to switch Port LED lighting according to {Link/ACT | PoE} modeConsole(config)#led-port-mode {poe | link-activity}\* Refers to the updated “PORT LED DEFINITIONS” on the last page. | RD |
|  | ECS4100-52T-00333 | New Fans in ECS4100-28P sound strange, 52P as well. | TS |
|  | ECS4100-52T-00334 | L2SW: Led of ports No. 49-52 (ECS4100-52P) is always lit off. | RD |
|  | ECS4100-52T-00340 | DHCP snooping trigger the switch reboot by itself. | TS |
|  | ECS4100-52T-00348 | SYSLOG-0040 0220 :Dut auto reboot after join port to vlan 2-4094 when testing syslog. | EIT |
|  | ECS4100-52T-00353 | After reboot static MAC of LAG disappear | TS |
|  | ECS4100-52T-00025ECS2110-26T-00145 | DHCPV6 Relay: DUT suould support to configure DHCPV6 Relay setting through WEB. | NTC |
| Test Build V1.02.14.181 |
|  | ECS4100-52T-00300 | (28P-ITUS) PoE status is enabled at default instead | RD |
|  | ECS4100-52T-00324Simba-Common-00234 | SNMPWALK but get error about sysResourceMgt | TS |
|  | ECS4100-52T-00325 | (12T-ITUS) Support for reset button (new BID=14) | RD |
|  | ECS4100-52T-00329ECS4100-52T-00294 | MVR function trigger the exception.MVR: MVR-0210 will cause console stop response | TSEIT |
|  | ECS4100-52T-00330 | Missing 'ftp' option for "copy running-config" and "copy startup-config" commands | TS |
|  | ECS4100-52T-00331 | switch ping response time will be higher when DDM SFP insert | Customer |
|  | ECS4100-52T-00332 | Write "reload in" command in configure file make switch stuck. | TS |
|  | ECS4100-52T-00336 | [Enhancement]SFP EEPROM/DDM/Measured info no clear after SFP removed. | RD |
|  | ECS4100-52T-00337 | [Enhancement] support dot1x eapol-pass-through | TS |
|  | Simba-Common-00228 | sflow sample packet doesn't include IPv4 information. | RD |
|  | Simba-Common-00232 | [Enhancement] Support read Total/Dynamic/Static mac count by SNMP | Customer |
|  | Simba-Common-00235 | switch forward all LLDP packets when dot1q enabled globally | Customer |

**(ECS4100) Runtime V1.2.15.181, Loader V1.0.0.5 / V1.0.1.6**

**ECS4100\_V1.2.15.181.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**ECS4100-12PH\_V1.2.15.181.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00194 | lost "ip arp inspection trust" setting on port-channel after reboot | Customer |
|  | ECS4100-52T-00195 | vlan translation does not work when enable dot1q-tunnel system.*(#138 workaround is disabled, however, #94 workaround is enabled.)* | TS |
|  | ECS4100-52T-00263 | [ECS4100-12PH]when thermal sensor exceeds 85 degrees, write information to syslog and specific file | RD |
|  | ECS4100-52T-00271 | Europe summer time end date is incorrect *(further revised to Westerm Europe, DST: Mar, last Sun, 01:00:00 ~ Oct, last Sun, 01:00:00)* | Customer |
|  | ECS4100-52T-00280 | MAC ACL cannot deny ethertype 8902(CFM)*(CFM status at default… global: disabled, port: enabled)* | TS |
|  | ECS4100-52T-00302 | Enhancement:If project support MSTP, setting chip as MSTP mode in initial phase. | RD |
|  | ECS4100-52T-00305 | L2SW: Led of ports No. 25-28 (ECS4100-28P) is always lit off. | NTC |
|  | ECS4100-52T-00312 | (12PH) support to force fan operational in full speed | RD |
|  | ECS4100-52T-00313 | (28TC) WebGUI soft panel is not correct. | RD |
|  | ECS4100-52T-00323 | (52P) runtime revision to match HW R0B design change for fan speed*(control: PWM 2,3,4 -> 1,2,4; reading: tach 2,3,4 -> 1,2,4)* | RD |
| V1.2.3.173 |
|  | ECS4100-52T-00175 | After reload , CPU Utilization incorrect bigger than 800M | TS |

**(ECS4100) Runtime V1.2.14.181, Loader V1.0.0.5 / V1.0.1.6**

**ECS4100\_V1.2.14.181.bix is for 52T/26TX/28T/12T/28P/52P/28TC**

**~~ECS4100-12PH\_V1.2.14.181.bix is for 12PH~~**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ~~ECS4100-52T-00176~~ | ~~system name was changed when configure interface vlan ip address~~ | ~~Customer~~ |
|  | ECS4100-52T-00262 | HTTPS: Can not establish HTTPS connection. | NTC |
|  | ~~ECS4100-52T-00263~~ | ~~[ECS4100-12PH]when thermal sensor exceeds 85 degrees, write information to syslog and specific file~~ | ~~RD~~ |
|  | ECS4100-52T-00264 | display fan speed on CLI | RD |
|  | ECS4100-52T-00282 | [enhance] when loopback detection detected, port led light yellow(green+amber). (copper port only) (28T-ITUS, 28P-ITUS only)) | RD |
|  | ECS4100-52T-00284 | [Enhancement]Porting for board id 11/12/13(combo port/stktplg board) | RD |
|  | ECS4100-52T-00285 | [Enhancement]Porting for board id 11/12/13(rx los enhancement) | RD |
|  | ECS4100-52T-00295 | Failed to set the TACACS+ server for aaa accounting dot1x. | RD |
|  | ECS4100-52T-00296 | (28TC) Support for bi-color LED | RD |
|  | ECS4100-52T-00297ECS4100-52T-00308 | (28TC) Support for thermal temperature[Enhancement]porting thermal, fan, watchdog for bid 11,12,13 | RDRD |
|  | ECS4100-52T-00298 | (28P-ITUS) Light Port LED in yellow (green+amber) when PoE is enabled and power is delivering. | RD |
|  | ECS4100-52T-00299 | (28T/28P-ITUS) Support for reset button | RD |
|  | ECS4100-52T-00300 | (28P-ITUS) PoE is disabled at default | RD |
|  | ECS4100-52T-00311 | Ip address and ip default-gateway can't accept 169.254.0.0/16 | RD |
|  | ECS2000-28PP-00736 | Conflict of diffserv and routing | Customer |
|  | ECS2000-28PP-00768 | Web: Administration > Time Range, the help page is not accessible when the Help(?) icon is pressed | TS |
|  | ES4528BH2-HPoE-0815-EC-00545 | switch could still learn the mac-address which belong none-vlan member even if enable the ingress filtering. | TS |
| V1.2.13.174 |
|  | ECS4100-52T-00253 | [Enhancement]Let RTK SDK RX thread be realtime with high priority | RD |
|  | ECS4100-52T-00254 | [Enhancement]Enhancement dev\_nicdrv for IGMP performance(handle a burst with 256 igmp packet) | RD |
| V1.2.7.173 |
|  | ECS4100-52T-00201 | Link state of LACP trunk member port changes between up and down repeatedly | Customer |
| V1.2.6.173 |
|  | ECS4100-52T-00193 | switch can't display output policy-map | TS |
| V1.1.11.171 |
|  | ECS4100-52T-00155(Same as #00093) | LBD: Log message is incorrect when the loopback-detection occurs and than the port numbers are over than 10. | NTC |

**(ECS4100) Runtime V1.2.13.174, Loader V1.0.0.5 / V1.0.1.4**

**ECS4100\_V1.2.13.174.bix is for 52T/26TX/28T/12T/28P/52P**

**ECS4100-12PH\_V1.2.13.174.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00167 | port security : the switch learning mac adresses and discards the first packets. | Customer |
|  | ECS4100-52T-00226 | Boot up log not sync when log ram & log flash are history 7 | TS |
|  | ECS4100-52T-00232ECS4100-52T-00260ECS4100-52T-00265 | MAC-Thrashing : the function is failed after port detection happened with the action is stop-learningMAC-thrashing: The "stop-learning" action mode cannot work repeatedly.MAC-thrashing: When the action mode is change to Link-down from stop-learning, this Mac-thrashing cannot work normally. | EITNTCNTC |
|  | ECS4100-52T-00249 | Syslog: no coldStart log after device cold start. | RD |
|  | ECS4100-52T-00251 | [ECS4100-12PH] fan status display wrong | TS |
|  | ECS4100-52T-00255 | Increas mac-based vlan entries to max 128 | TS |
|  | ECS4100-52T-00259 | mac-thrashing: When the mac-thrashing is "On", this Port should not learn MAC address. | NTC |
|  | ECS4100-52T-00261 | CustomerInfo: Display of the System OID on CLI and WebUI is wrong. (12PH only) | NTC |
|  | ECS4100-52T-00269 | [RX Los Interrupt handling]Add Rx los interrupt handling to notify core layer for specific board(12ph) | RD |
|  | ECS4100-52T-00270 | L2SW: (ECS4100-12PH) Port 9&10 it lit up amber when connected to test center via 10/100Mbps. | NTC |
|  | ECS4100-52T-00271 | Europe summer time end date is incorrect *(updated to Turkey, DST: Mar, last Sun, 03:00:00 ~ Oct, last Sun, 04:00:00)* | Customer |
|  | ECS4100-52T-00273 | PoE: The CLI help for power allocation is incorrect. | NTC |
|  | ECS4100-52T-00278 | LLDP: There is no command to enable LLDP PoE TLV. | NTC |
|  | ECS4100-52T-00279 | The switch needs to send SNMP TRAP if the contacts of reset button are closed. | RD |
|  | ECS4100-52T-00280 | MAC ACL cannot deny ethertype 8902(CFM) | TS |
|  | Simba-Common-00219 | RARP ethertype ix 0x8035, but the code is defined as 0x0835 in lan.c | RD |
|  | ECS2000-28PP-00757 | stop routing after flush mac-address table two times | TS |

**(ECS4100) Runtime V1.2.12.174, Loader 1.0.0.5 / 1.0.1.1**

**ECS4100\_V1.2.12.174.bix is for 52T/26TX/28T/12T/28P/52P**

**ECS4100-12PH\_V1.2.12.174.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| 1 | ECS4100-52T-00231 | [enhance] support 12PH LED, FAN, Thermal (fix 9~12 port led) | RD |
| 2 | ECS4100-52T-00241 | [RTK patch] rtk\_l2\_addrEntry\_get() support to get CAM entry | RD |
| 3 | ECS4100-52T-00243 | CPU utilization rising to 16% in idel issue for new board ECS4100-12PH(board id 10) | RD |

**(ECS4100) Runtime V1.2.11.174, Loader 1.0.0.5 / 1.0.1.1**

**ECS4100\_V1.2.11.174.bix is for 52T/26TX/28T/12T/28P/52P**

**ECS4100-12PH\_V1.2.11.174.bix is for 12PH**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| 1 | ECS4100-52T-00192 | [enhance] support ECS4100-12PH with BCM PoE chip | RD |
| ~~2~~ | ~~ECS4100-52T-00226~~ | ~~Boot up log not sync when log ram & log flash are history 7~~ | ~~TS~~ |
| 3 | ECS4100-52T-00227 | [RX Los Interrupt handling]Add Rx los interrupt handling to notify core layer for specific board ((1)Support board id 6(ECS4100-28P)) | RD |
| 4 | ECS4100-52T-00230 | create an ECS4100-12PH build environment and code. | RD |
| 5 | ECS4100-52T-00231 | [enhance] support 12PH LED, FAN, Thermal | RD |

**(ECS4100) Runtime V1.2.10.174, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| 1 | ECS4100-52T-00135 | Failed to add static multicast group during config provision | TS |
| 2 | ECS4100-52T-00136 | Src ip of igmp report is always 0.0.0.0. | TS |
| 3 | ECS4100-52T-00184 | [enhance] support VLAN-TRUNKING | RD |
| 4 | ECS4100-52T-00204. | loopback detecion detects traffic loop even port is DOWN | RD |
| 5 | ECS4100-52T-00206. | 802.1ag-CFM-0570:Dut did not send out MEP-Down Trap or record it in log ram after CCM interval time. | RD |
| 6 | ECS4100-52T-00208 | MSTP : DUT can NOT show the port information after saving reload | EIT |
| 7 | ECS4100-52T-00210. | Web:RIP: On Routing Protocol>RIP>Distance>Action:Show page, display RIP distance with error subnet mask. | RD |
| 8 | ECS4100-52T-00211. | Web:RIP: When only create a RIP network per VLAN, can't open Routing Protocol>RIP>Network>Action:Show page. | RD |
| 9 | ECS4100-52T-00215. | IGMPSNP: fail to configure per VLAN settings soon after many VLANs are created | RD |
| 10 | ECS4100-52T-00216 | 802.1ag-CFM-0150:Dut didnot handle well with Remote MEP cross-check | EIT |
| 11 | ECS4100-52T-00217. | PPPoEIA can't work with QinQ tunnel | RD |
| 12 | ECS4100-52T-00220. | ASIC still learns mac address even disable mac learning on the port | RD |
| 13 | ECS4100-52T-00221 | [enhance] support mac thrashing | RD |
| 14 | ECS4100-52T-00222 | When switch enable DHCP Snooping & IP source-guard, DHCP renew cause packet loss(ECS4100-28T) | TS |
| 15 | ECS4100-52T-00228 | OAM should init the semaphore when startup | RD |
| 16 | ECS4100-52T-00229 | Disable LBD trigger a LBD recover log | TS |
| 17 | Simba-Common-00210. | Web:RIP: On Routing Protocol>RIP>Distance>Action:Show page, display RIP distance with error subnet mask. | EIT |
| 18 | Simba-Common-00211. | Web:RIP: When only create a RIP network per VLAN, can't open Routing Protocol>RIP>Network>Action:Show page. | EIT |
| 19 | Simba-Common-00212. | IGMPSNP: fail to configure per VLAN settings soon after many VLANs are created | RD |
| 20 | Simba-Common-00213. | PPPoEIA can't work with QinQ tunnel | Customer |
| 21 | Simba-Common-00216. | OAM should init the semaphore when startup | RD |

**(ECS4100) Runtime V1.2.9.173, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| 1 | ECS4100-52T-00212 | [Enhance][52P] support bi-color for LED on new 52P | RD |

**(ECS4100) Runtime V1.2.8.173, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| 1 | ECS4100-52T-00174 | [Enhance] Dying gasp (Syslog and SNMP trap) | RD |
| 2 | ECS4100-52T-00205. | SNMP: The value of OID "lldpRemManAddrIfId" remove ".0" at the end. | RD |
| 3 | ECS4100-52T-00207 | [Enhance][28P] support bi-color for LED on new 28P | RD |
| 4 | ECS4100-52T-00209 | software watch dog reboot while add vlan in vlan database | RD |
| 5 | ECS4100-52T-00212 | [Enhance][52P] support bi-color for LED on new 52P | RD |
| 6 | ECS4100-52T-00213 | When inster one POE, the PWR led display amber | RD |
| 7 | Simba-Common-00155. | SNMP: The value of OID "lldpRemManAddrIfId" remove ".0" at the end. | RD |

**(ECS4100) Runtime V1.2.7.173, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| 1 | ECS4100-52T-00186 | [Enhance] switching B/W L2 DHCP relay and L3 DHCP relay | RD |
| 2 | Simba-Common-00138. | [Enhance] Modified openSSL/libXML build script to avoid privilege issue | RD |
| 3 | Simba-Common-00145. | NTP: The ntp client of DUT will getting the ntp information after 1024 secs when the DUT reboot. | RD |
| 4 | Simba-Common-00150. | [IGMP filter] the multicast traffic does not match rule, but it still will be forwarded. | RD |
| 5 | Simba-Common-00151. | [S900-S1\_9/E-NEST-056]After execution of copy running-config startup-config, if Startup configuration file name is NULL, no e | RD |
| 6 | Simba-Common-00152. | Link state of LACP trunk member port changes between up and down repeatedly | RD |
| 7 | Simba-Common-00153. | Static port-channel cause loopback detection enable global failed | RD |
| 8 | Simba-Common-00154. | loopback detecion detects traffic loop even port is DOWN | RD |
| 9 | Simba-Common-00156. | IPv6FTP: When DUT upgrade code with interrupt network connection and reconnect. It would cause upload fail. | NTC |

**(ECS4100) Runtime V1.2.6.173, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| 1 | ECS4100-52T-00056 | DHCP Server: We cannot configure this maximum pool name to 32 characters from WEB. | NTC |
| 2 | ECS4100-52T-00188 | Enhancement: support LACP passive mode | RD |
| 3 | Simba-Common-00146. | Web-1QVLAN-0020:delete all vlan didnot successfully | RD |

**(ECS4100) Runtime V1.2.5.173, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
| 1 | ECS4100-52T-00052 | DHCP Server: We cannot enmable/disable DHCP service from WEB. | NTC |
| 2 | ECS4100-52T-00055 | DHCP Server: The lease time of host entry is incorrect. | NTC |
| 3 | ECS4100-52T-00057 | DHCP Server: We cannot configure specifice DHCP option successfully. | NTC |
| 4 | ECS4100-52T-00137 | DHCP-Snooping-0370:There is no information of DHCP drop in flash log when untrust port drop dhcp packets | EIT |
| 5 | ECS4100-52T-00138 | use vlan translation egress rule to modify TPID when QinQ is enabled | RD |
| 6 | ECS4100-52T-00172 | Loop Detection (refer to ES4328QV-FLF-38IK-00004) | RD |
| 7 | ECS4100-52T-00181 | ECS4100-28T/28P add DHCP Server support with 256 hosts | Customer |
| 8 | ECS4100-52T-00179 | watchdog reboot - XFER\_TD & CLI\_GROUP | Customer |
| 9 | ECS4100-52T-00187 | qinq priority mapping problem - inner pri to outer pri | TS |
| 10 | Simba-Common-00141. | Failed to get switchport LACP info. | RD |
| 11 | Simba-Common-00143. | Web:RIP: DUT doesn't support OSPF, but can configure RIP redistribute as OSPF on Web page for DUT. |  |
| 12 | Simba-Common-00144. | Web:RIP: Information about sending RIP version and Receiving RIP version from Web page is not same as that from CLI. |  |

**(ECS4100) Runtime V1.2.4.173, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00103 | RA Snooping Support | Custom |

**(ECS4100) Runtime V1.2.3.173, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00156ES3510-28T-00758 | SNMP\_TD crash | Custom |
|  | ECS4100-52T-00162 | igmpsnooping-1280:Dut didnot handle router port registered well | EIT |
|  | ECS4100-52T-00168ECS2000-28PP-00701 | Inject the LLDP packet, then dashboard and show remote device information will empty. | TS |
|  | ECS4100-52T-00171 | IPv6-AddrConfig: DUT doesn't reply NA when it received NS. | NTC |
|  | ECS4100-52T-00172 | Loop Detection (refer to ES4328QV-FLF-38IK-00004) | RD |
|  | ECS4100-52T-00173 | LLDP: ECS4100-12T doesn't have TIA TR-41 committee-inventory-model name TLV. | NTC |
|  | ECS4100-52T-00177 | free memory decreases every min/hour/day because of DDM SFP\* happens to ECS4100-28T only | Custom |
|  | ECS4100-52T-00178 | [enhance] Change kernel memory allocator from SLOB to SLAB to have better performance | RD |
|  | ECS2100-52T-00075 | [enhance] support RIP | RD |
|  | ES4627MB-FLF-EC-00791 | Revise design of VLAN ingress fitering | Custom |
|  | ECS2000-28PP-00699 | packets send to switch cause routing loop - L3 rule issue | Custom |
|  | ECS2000-28PP-00704 | the switch doesn't remove host route(arp entry) when mac aging out. | TS |

**(ECS4100) Runtime V1.2.2.172, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00152 | lost settings of qos map dscp-queue after switch rebooting. | Custom |
|  | ECS4100-52T-00162 | igmpsnooping-1280:Dut didnot handle router port registered well | EIT |

**(ECS4100) Runtime V1.2.1.172, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-NA | WebGUI soft panel is not available for 28P, 52P, and 12T. | RD |
|  | ECS4100-52T-00151 | ECS4100-26TX uplink port with 10G full duplex drops packet with VLAN tag which packets size 1522 bytes | Custom |
|  | ECS4100-52T-00154ECS2000-28PP-00864 | switch drop OSPF/RIP/VRRP packets when IGMPSNP or MVR is enabled | Custom |
|  | ECS4100-52T-00157 | [Enhance] Support TCAM allocatioon profile | RD |

**(ECS4100) Runtime V1.2.0.172, Loader 1.0.0.5 / 1.0.1.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00076 | QinQ: When we enable/disable to discard all matched default-service traffic, DUT does not drop/forward tagged packets. | NTC |
|  | ECS4100-52T-00094ECS4100-52T-00138 | vlan translation does not work even disable dot1q-tunnel systemuse vlan translation egress rule to modify TPID when QinQ is enabled | CustomRD |
|  | ECS4100-52T-00102 | support DHCPv6 Snooping, Option 18 (INTERFACE\_ID) and 37 (REMOTE\_ID); | Custom |
|  | ECS4100-52T-00103 | Support IPv6 RA Guard | Custom |
|  | ECS4100-52T-00108 | DoS: Use LOIC to attack port 22, CLI has no response and DUT reboot by watchdog. | NTC |
|  | ECS4100-52T-00116 | [Enhancement] Support IPv6 ND snooping function | Custom |
|  | ECS4100-52T-00117 | [Enhancement] Support IPv6 ND snooping setting via SNMP | Custom |
|  | ECS4100-52T-00140 | MSTP: Change the instance priority, the traffic will stop and recover the issue after 6 mins. | NTC |
|  | ECS4100-52T-00142 | [Telnet] After tool "LOIC" TCP:23port attack, modified thread pool for telnetd & tnshd | RD |
|  | ECS4100-52T-00144 | [Enhance] Support 4 new CO boards - ES4328R[-PoE]-CO / ES4552R[-PoE]-CO | RD |
|  | ECS4100-52T-00145 | [Enhance] Support new 12T/PH boards - ECS4100-12T/PH: 8\*GbE + 4\*SFP(GbE) /HPoE | RD |
|  | ECS4100-52T-00146ECS2000-28PP-00691 | ECS4100 high cpu util | Custom |
|  | ECS4100-52T-00148ECS2000-28PP-00690 | massive ip & arp packets may trigger hw watchdog reboot | Custom |
|  | ECS4100-52T-00149ECS2000-28PP-00694 | switch drops packest every 300 seconds because of port ecurity and mac aging time | Custom |

**(ECS4100) Runtime V1.03.02.171, Loader 1.0.0.5**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00084 | [Enhancement] MVR shall recognize IGMP report/leave with PPPoE header. (process unicast SA) | Custom |
|  | ECS4100-52T-00086 | [Enhancement] IGMP-SNP: multicast static-group on uplink per-port per-vlan | Custom |
|  | ECS4100-52T-00094 | vlan translation does not work even disable dot1q-tunnel system | Custom |
|  | ECS4100-52T-00095 | multicast strom control stops working when enabling mvr or igmp snooping | Custom |
|  | ECS4100-52T-00101 | SSH over IPv6 address - does not support record of ipv6 login info in log ram/flash | Custom |
|  | ECS4100-52T-00105 | unified file size unit in byte and add thousands separator | Custom |
|  | ECS4100-52T-00110 | All Link-down receiver port still has G query packet counter increased | RD |
|  | ECS4100-52T-00111(#45 extension) | The MVR VLAN does not removed automatically when I disable“mvr do 1 type receiver” on port 1. | TS |
|  | ECS4100-52T-00115 | DHCP dynamic-provision does not work on the other VLANs except the default VLAN 1. | Custom |
|  | ECS4100-52T-00118 | cable diag does not support the port at 10M Full/Half duplex. | Custom |
|  | ECS4100-52T-00119 | support UDLD | Custom |
|  | ECS4100-52T-00123 | (DCR) Use Egress DiffServ slice to patch the actions on Ingress DiffServ slice (3 slices for IPv6/IPv4/MAC) | RD |
|  | ECS4100-52T-00125 | support remarking ingress diffserv "ip dscp" | Custom |
|  | ECS4100-52T-00127 | Huawei switch S2300 can't recognize ECS4100's LLDP packet with "dot1-tlv protocol identity" | TS |
|  | ECS4100-52T-00128 | enlarge IPSG (ACL mode) per port maximum entry, 5 -> 32 | Custom |
|  | ECS4100-52T-00131 | remove the reset button function code in the software | Custom |

**(ECS4100) Runtime V1.1.11.171, Loader 1.0.0.5**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00021 | TraceRoute: WebUI doesn't support traceroute to hostname. | NTC |
|  | ECS4100-52T-00045 | The MVR VLAN does not removed automatically when I disable “mvr do 1 type receiver” on port 1. | TS |
|  | ECS4100-52T-00073 | VLAN-translation: Falied to save the VLAN-translation trunk setting to configuration file. | NTC |
|  | ECS4100-52T-00080 | RADIUS-Acct: The console and Web of accounting information that is unmatched | NTC |
|  | ECS4100-52T-00082 | PPPoE-IA: PPPoE circuit id format type string is not working. | NTC |
|  | ECS4100-52T-00083 | storm control maximum and minimum threshold is incorrect | Custom |
|  | ECS4100-52T-00084 | [Enhancement] MVR shall recognize IGMP report/leave with PPPoE header. (move cmd) | Custom |
|  | ECS4100-52T-00085 | Spanning-tree: We cannot enable the STP mode from WEB. | NTC |
|  | ECS4100-52T-00086 | [Enhancement] IGMP-SNP: multicast static-group on uplink per-port per-vlan | Custom |
|  | ECS4100-52T-00087 | [Enhancement] IGMP-SNP: immediate-leave per-port | Custom |
|  | ECS4100-52T-00088 | tacacs+-0080:dut crash when admin/admin login dut after tacacs-server key removed | EIT |
|  | ECS4100-52T-00090 | CLI: Please rename "Excutes" to "Executes" about cable-diagnostics. | NTC |
|  | ECS4100-52T-00091 | Support banner information | Custom |
|  | ECS4100-52T-00092 | [Enhancement] initial IP address 192.168.2.10/24 on DHCP mode | Custom |
|  | ECS4100-52T-00093 | loopback detection log messages are incorrect | Custom |
|  | ECS4100-52T-00107 | ECS4100-52T sends LLDP packet with no “port description, system name and system description” field after receiving Huawei’s | Custom |
|  | ECS4100-52T-00109 | Duplicate DHCP discover packet and maximum value of retransmission interval is not right | RD |
|  | ECS2000-28PP-00649 | Voice VLAN: DUT should not display the trunk member port in voice-vlan status list. | NTC |

**(ECS4100) Runtime V1.1.8.164, Loader 1.0.0.5**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00009 | [Enhancement] PPPoE-IA To support Cirquit-Id (hostname/port/vlan), Remote-Id (mac-address CPE). | RD |
|  | ECS4100-52T-00015 | [Enhancement] MVR shall recognize IGMP report/leave with PPPoE header. | RD |
|  | ECS4100-52T-00040 | [Enhance] Support IP Cluster | RD |
|  | ECS4100-52T-00047 | Selective QinQ: Selective QinQ doesn't work, always match the default QinQ rule | NTC |
|  | ECS4100-52T-00048 | MVR: General query can not be forwarded to receiver ports when MVR VLAN was down and up. | NTC |
|  | ECS4100-52T-00053 | ""empty log message in log ram/flash when inject DHCP ACK packet to DHCPSNP trust port | TS |
|  | ECS4100-52T-00059 | [Enhance] 28T reads I2C eeprom-raw-data in order to detect SFP insertion. | RD |
|  | ECS4100-52T-00061 | [ECR] Remove DHCP Server | RD |
|  | ECS4100-52T-00062 | [Enhance] Hide the option for copying sw license file | RD |
|  | ECS4100-52T-00067 | (ECR) MIB: replace 'ecs4100-26tx<xxx>' with 'ecs4100-52t<xxx>' | RD |
|  | ECS4100-52T-00069 | switch with stack can't display config complete via SSH | TS |
|  | ECS4100-52T-00071 | switch still send schedule report to all MVR source port | TS |
|  | ECS2110-52T-00044 | IGMP-SNP: After remove vlan, an exception occurs. | NTC |

**(ECS4100) Runtime V1.1.4.164, Loader 1.0.0.4**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS2100-52T-00033 | MLDSNP: Forwarding rate of some UDP well known packets is very poor. | NTC |
|  | ECS4100-52T-00005 | [Enhancement] Separate ingress and egress direction of VLAN-translation. Need new commands. | Custom |
|  | ECS4100-52T-00050 | [Enhance] Afford CLI commands to select L2 hash method {Algo\_0 | Algo\_1} in RTL839x. | RD |
|  |  | Fan-less 52T is locally patched at BID=0 |  |

**(ECS4100) Runtime V1.1.3.164, Loader 1.0.0.4**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS4100-52T-00010 | [Enhancement] it is about DHCPSNP to support Cirquit-Id (hostname/port/vlan), Remote-Id (mac-address CPE). | Custom |
|  | ECS4100-52T-00041 | [Enhance] Support new 52T for having no fan and thermal. (BID=4) | RD |
|  | ECS4100-52T-00043 | 52T System(Diag) LED stays in amber steady when system is operational normally. | RD |

 **(ECS4100) Runtime V1.1.2.164**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | N/A | Fan-less 52T System(Diag) LED stays in amber steady at runtime. (local patched) | - |

**(ECS4100) Runtime V1.1.1.164**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | N/A | Support fan-less 52T, retained BID=0. (local patched) | - |
|  | ECS2110-26T-00221ECS2100-52T-00031 | CoS: Change cos-queue mapping, the data receive ratio is not changed. | NTC |
|  | ECS2110-26T-00162 | [QinQ]TPID is not modified when traffic comes from normal port to QinQ uplink port | RD |
|  | ECS4100-52T-00006 | [Enhancement] Disable untagged traffic for dot1q mode access port. | Custom |
|  | ECS4100-52T-00013ECS4100-52T-00019 | Running-config shows an incredible static route 224.0.0.0 at default system-boot-up.remove useless command "ip route 224.0.0.0 240.0.0.0 0.0.0.0" on running-config | RDTS |
|  | ECS4100-52T-00016 | spanning-tree blocking port does not discard ipv4 mdns packet | TS |
|  | ECS4100-52T-00037 | 28T Web panel is not available (page not found). | RD |

**(ECS4100) Runtime V1.1.0.163, Loader 1.0.0.3**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS2110-26T-00204 | DQoS: The default priority is not modifying when the port had once the authenticated. | NTC |
|  | ECS2110-26T-00215 | 802.1XDQoS: The DUT will permit the supplicant when the attribute is wrong configure. | NTC |
|  | ECS4100-52T-00003 | [Enhance] Porting the switch protection with software license from AOS | RD |
|  | ECS4100-52T-00004 | [Enhance] IGMP Authentication | RD |
|  | ECS4100-52T-00007 | [Enhancement] Checking of Restricted TCN function | Custom |
|  | ECS4100-52T-00014 | Running-config shows "ip igmp snooping vlan 1" at default system-boot-up. | RD |
|  | ECS4100-52T-00037 | [Enhance] Support new board - ECS4100-28T: 24\*GbE + 4\*SFP(GbE) | RD |
|  | ECS4100-52T-00038 | DHCP Snooping stops forwarding DHCP discover packets if mac-table is full. | TS |

**(ECS2110) Runtime V0.0.3.0, Loader 1.0.0.3**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS2110-26T-00156 | Web: Got "Data is invalid" when another copy ftp is run. | NTC |
|  | ECS2110-26T-00175 | Transceiver: Got debugging message "SFP 2 unknown sfp type:0x2" and got "checksum error" information | NTC |
|  | ECS2110-26T-00206 | Syslog: restartControl by cold start (SNMP) will send warm start trap. | NTC |
|  | ECS2110-26T-00220 | SNMP: We can't get the value of switchMgt on ECS2110-26T-ME. | NTC |
|  | ECS2110-26T-00223 | enabled proxy-switching still reply the IGMP querier when MVR source port receive the join report | TS |
|  | ECS4100-52T-00012ECS4100-52T-00018 | Running-config shows LLDP PoE-specific settings on each port at factory defaults.useless commands "no lldp dot3-tlv poe" "no lldp dot3-tlv poe" in running-config | RDTS |
|  | ECS4100-52T-00017 | loopback detection does not detect traffic loop because of ipv4 mdns packet | TS |

**(ECS2110) Runtime V0.0.2.5, Loader 1.0.0.1**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS2110-26T-00094 | SNMP/MIB and Web miss the "Linux Kernel Version" item. | RD |
|  | ECS2110-26T-00125 | MVR:Groups belong to MVR profile can not be registered on normal port. | NTC |
|  | ECS2110-26T-00131 | MVR: Inactive receiver port would forward data to source port and receiver port. | NTC |
|  | ECS2110-26T-00156 | Web: Got "Data is invalid" when another copy ftp is run. | NTC |
|  | ECS2110-26T-00196 | [Enhance] Support for new sku ECS2110-26T-ME, additional DC power | Custom |
|  | ECS2110-26T-00197 | switch can't dynamic learn mrouter port when enable MVR | TS |
|  | ECS2110-26T-00198 | [Enhance] Add Web help pages (prepared by TW using v0.0.2.0) to CC | RD |
|  | ECS2110-26T-00199 | MVR: Group can not be deleted when registered port received leave report in transparent mode. | NTC |
|  | ECS2110-26T-00201 | TACACS+: The DUT will reboot automatically when user logins the DUT by TACACS account, but the TACACS key is mismatch. | NTC |
|  | ECS2110-26T-00202 | StaticRoute: Source MAC in routing packets is not DUT's MAC address. | NTC |
|  | ECS2110-26T-00203 | EFM-OAM: When we start/stop remote loopback, it can't start again. | NTC |
|  | ECS2110-26T-00205 | There is no WEB help page. | NTC |
|  | ECS2110-26T-00207 | System: DUT cannot forward the IGMP general Querier to host on v0.0.2.3. | NTC |
|  | ECS2110-26T-00209 | WebAuth: When quiet period is set to 30 seconds, it shows "You are allowed to re-login after 0 minutes." | NTC |
|  | ECS2110-26T-00213 | [enhance] support mDNS | RD |

**(ECS2110) Runtime V0.0.2.3, Loader 1.0.0.0**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  | ECS2110-26T-00183 | [enhance] remove phy internal loopback test. | RD |
|  | ECS2110-26T-00186 | [enhance] display total flash size in CLI 'dir' command for EC products. | RD |
|  | ECS2110-26T-00187 | [enhance] MVR redesign in ES3528MV2 Ph5 branch -> EC main | RD |
|  | ECS2110-26T-00193 | [Enhance] Disable those unused 25M output clocks in RTL839x (52T only) | RD |
|  | ECS2110-26T-00195 | [Enhance] Enable BCAM from L2 lookup table | RD |

**(ECS2110) Runtime V0.0.1.1, Loader 0.0.1.0**

|  |  |  |  |
| --- | --- | --- | --- |
|  | EPR | Headline | Role |
|  |  |  |  |

**Known RESTRICITIONS AND Limitations:**

|  |  |
| --- | --- |
| 1 | L2 table (16K entries) share for L2 unicast, L2 multicast, IPv4 multicast, IPv6 multicast, Routing. |
| 2 | For all Basic Switching Unit-Test items of the half duplex, the counter of fragments would increase the same number/speed as the counter, collisions on IXIA.It is confirmed by Realtek Josh. It is chip normal behaviour which follows the standard.RTK use the “Collision based backpressure” of flow control (backpressure) on half mode. It will send the jam pattern packet to do the flow control. |
| 3 | Due to chip limitation, do not support Port-based QoS. |
| 4 | Chip limitation: Not supported for global ACK, which was known as “VLAN ACL” before. |
| 5 | Chip limitation: MAC ACL does not allow for configuring any IP/IPv6 pattern. |
| 6 | Chip limitation: Supports for mapping CoS/DSCP to PHB (or Internal Priority) and then to Queue. But CoS/DSCP-to-PHB mapping also changes a packet's trap-to-cpu queue.Therefore, SW design decides to remove CoS/DSCP-to-PHB mapping, causing straight CoS/DSCP-to-Queue mapping on user configuration. [ECS2000-28PP-00344]Note: The implementation gets to be partially compliant with RFC 2597/2598.Implemented the CLI command: “Console(config-if)#[no] qos map {cos-queue | dscp-queue}”, for ethernet inferface only. |
| 7 | Chip limitation: Ingress/Egress DiffServ poorly supports for SRTCM/TRTCM remarking. 1) Meter burst size is global setting, instead of per-police. => So hard to meet various SRTCM/TRTCM cases. 2) Ingress rule does not support for color action and CoS/DSCP remarking. => Has to additionally use egress rule. 3) Egress ACL action is global for DLF/broadcast/multicast traffic, however, per-port for unicast. => DLF/broadcast/multicast will not be matched with port list. Therefore, SW design decides to only implements flow rate-limiting. [ECS2110-26T-00034]Implemented the CLI command: “Console(config-pmap-c)#[no] police rate *<16-10000000 Kbps>*”.~~Besides, DiffServ ingress policy-map can remark CoS only. If a police is configured to remark DSCP, it shall be rejected while binding to input port. [ECS2110-26T-00034] [Workaround in ECS4100-52T-00123]~~ |
| 8 | Chip limitation: Following counters are not supported. These counters are not visible. [ECS2000-28PP-00051,00466]IF-MIB:Discard Input (ifInDiscards)Unknown Protocols Input (ifInUnknownProtos)Error Output (ifOutErrors) - RTL838x does not support this counter, however, RTL839x does.QLen Output (ifOutQLen)EtherLike-MIB:Alignment Errors (dot3StatsAlignmentErrors)SQE Test Errors (dot3StatsSQETestErrors)Internal Mac Receive Errors (dot3StatsInternalMacReceiveErrors)Carrier Sense Errors (dot3StatsCarrierSenseErrors) |
| 9 | Chip limitation: Cable diagnostics can detect cable length up to 100 meters with an inaccuracy around 15 meters. |
| 10 | Chip limitation: Jumbo frame is supported by system, instead of per port. |
| 11 | Chip limitation: Voice VLAN can not support for remarking DSCP priority (because rule action can not remark CoS and DSCP at the same time). [ECS2000-28PP-00041] |
| 12 | Chip and HW board limitations: When an SFP transceiver is inserted, CPU will take some more time to have it initialized. This will lead to slow system response. |
| 13 | Chip limitation: Not supported for false carrier events ‘rpMauFalseCarriers’ in MAU-MIB. The counter value will always stay in 0. |
| 14 | Chip limitation: The collision mac-address is not affordable. |
| 15 | Chip limitation: Not supported for changing the priority of multicast traffic in IGMPSNP/MVR/MVR6. [ECS2000-28PP-00341, ECS2110-26T-00064,76,129] |
| 16  | Chip limitation: One single reason for trap-to-cpu of protocol packets, like BPDU/LACP/LLDP/dot1X (because all of these packets go through queue #5). |
| 17 | Chip limitation: IPv4 standard ACL and IPv4 extended ACL are implemented using a same rule slice. Their entries share the total 128 rules in the slice. |
| 18 | Chip limitation: IPv6 standard ACL and IPv6 extended ACL are implemented using a same rule slice. Their entries share the total 64 rules in the slice. |
| 19 | Chip limitation: Not supported for GVRP bypass VLAN check in RTL839x, but supported in RTL838x.(Supported for BPDU/LACP/LLDP bypass VLAN check in 8x [ECS2000-28PP-000147]. 9x as well.).Therefore, when a receive port does not join PVID VLAN and its VLAN ingress filter is enabled, GVRP does not work (GVRP packet is dropped by chip). |
| 20 | Chip limitation: MAC-based VLAN can not work with IP Source Guard. [ECS2000-28PP-00321] |
| 21 | Chip limitation: Internal loopback test does not work on 10G SFP+ ports (port# 25,26) in ECS2110-26T device because of no PHY chip there. |
| 22 | Chip limitation: When a port is linkup at 10 Mbps speed, cable diagnostics is not supported. [ECS2110-26T-00055]Btw, cable-diag can only measure cable length on the two conditions: 1. (Link\_Up; Speed\_1000M) and 2. (Link\_Down; link partner inexistent, port admin up).Case\_1) Link\_Up 1.1) Speed\_1000M => can measure cable length 1.2) Speed\_100M => cannot measure cable length 1.3) Speed\_10M => cannot measure cable length (cable-diag is not supported actually)Case\_2) Link\_Down 2.1) link partner existent, port admin up => cannot measure cable length 2.2) link partner existent, port admin down => cannot measure cable length 2.3) link partner inexistent, port admin up => can measure cable length 2.4) link partner inexistent, port admin down => cannot measure cable length |
| 23 | Chip limitation: L2 hashing algorithm (algo\_1) will get to observable collisions when both Source MAC address and VLAN ID are incremental successively.However, when only SA is random (no matter if VID is fixed, incremental, or random), L2 hashing will have very good performance. |
| 24 | Chip limitation: L2 table can contain up to (16K + 64) entries because BCAM (extension table with additional 64 entries) is enabled. [ECS2110-26T-00211, ECS2100-52T-00032] |
| 25 | ECS4100-28T Board limitation:1) Not available for SFP\_Present state (GPIO signal). ~~1-1) SW is not aware of any SFP insertion, and does not read out the EEPROM data. So, not able to afford any SFP information (CLI “show interfaces transceiver”).~~ ~~1-2) When 100M SFP is inserted and connected to link partner, the fiber port will not get to linkup until it is forced to 100FX mode (CLI “media-type sfp-forced 100fx”).~~\* No such issues (1-1, 1-2) in SW V1.1.5.164 and higher.2) System and Port LEDs are single-color and can only be lighting in green (blinking or solid).3) System LED will not be blinking while system is booting.~~4) There is no thermal sensor for system temperature. Fan neither.~~ |
| 26 | Chip limitation: When a packet is mirrored to mirroring port due to one port’s rx and the other port’s tx, only one packet (i.e. the copy of that rx) will be copied to mirroring port. [ECS4100-52T-00046] |
| 27 | Chip limitation: There is only 1 copy, which is from the port with smallest port id, for mirroring non-unicast in egress direction(tx). [ECS2100-10P-ACN-00022] |
| ~~28~~ | ~~Chip limitation: When an input packet's field (e.g. VLAN\_ID) is modified by ingress ACL, egress ACL is not able to match that updated value because it still sees the original packet's value. [ECS4100-52T-00138]~~~~For example,~~ ~~1. port\_1 is configured with ingress VLAN translation 10 -> 100, port\_2 is configured with egress VLAN translation 100 -> 200.~~~~2. Inject tagged packets with VLAN\_ID=10 to port\_1.~~~~3. These packets will not out-go from port\_2 because port\_2 sees VLAN\_ID=10, instead of VLAN\_ID=100.~~ |
| 29 | Chip limitation: For the tagged traffic between QinQ uplink port and normal port, if QinQ TPID is not 0x8100, packet's egress TPID will be incorrect. [ECS4100-52T-00195]PS. #00138 workaround solution is disabled, however, #00094 workaround solution is enabled.For example, QinQ TPID is 9100. When 9100 tagged packet is incoming from QinQ uplink port and outgoing to normal port with tagged member, its TPID remains 9100. (Should be 8100.)And vice versa. Say, 8100 tagged packet, normal port income, QinQ uplink port outgo, TPID remains 100. |
| 30 | ECS4100-28T/28P/28TC Board limitation: There is no GPIO signal available for SFP\_Present state. Therefore, in order for SFP-insertion polling, it takes more CPU resource to read SFP EEPROM data via I2C channel. This may result in higher CPU utilization, as compared with other skus having GPIO signal for SFP\_Present. |
| 31 | Chip limitation: The ARP packet would be still filtered by MAC ACL even the ACE permits the source MAC address. The cause is Realtek chip matches ‘Source MAC’ /ACE with ‘Sender Hardware Address’ /ARP. The two fields of an ARP packet are supposed to be the same. However, they are different for some reason. [ECS4100-52T-00247] |
| 32 | Chip limitation: ATC (Auto Traffic Control) does not support for Unknown Unicast storm control. [ECS4100-52T-00258] |
| 33 | Chip limitation: ACL and DiffServ can be bound to a same egress port. However, it gets higher priority to match ACL. [ECS4100-52T-00427] |
| 34 | Chip limitation: RTL839x does not have the ifInDiscards /IF-MIB register. However, SW works around to provide a substitute ifInDiscards counter, and its valus is a sum of (dot1dTpPortInDiscards, rxMacDiscards) registers. [ECS4100-52T-00629] - dot1dTpPortInDiscards:  count of valid frames received which were discarded (i.e., filtered) by the forwarding process (dropped in ALE) - rxMacDiscards: the number of packets dropped in MAC RX and switch core including bad packets and dropped packet due to lack of resource (dropped before ALE) |
| 35 | SW limitation: When both VLAN Trunking and Ingress Filtering are enabled, the system will drop those to-CPU packets, carrying unknown VLANs (not existent in the system).For example, Enabled both VLAN Trunking and Ingress Filtering, a DAI trusted port does not forward unknown-VLAN ARP packets.Note: First has a port's Lookback Detection disabled, then can have its Ingress Filtering disabled. |
| 36 | Notes for ECS4100-12PH supporting 60W UPoE (802.3bt Type 3 Class 5~6), starting from V1.2.37.191 [ECS4100-52T-00634]1. Broadcom PoE MCU firmware version has to be upgraded to 4.0.0.5 first.2. Any PD shall follow 3bt/at/af specifications of current and voltage ratings. If the ratings are exceeded due to short circuits or voltage transients, PSE ports might be damaged permanently, as per Broadcom PAE advices.3. So far Accton PoE Loader (AnalogDevice LT4321) is tested, and the PDs can be provided power up to 60W. That means no other chip vendor’s 3bt PD solution is guaranteed for 60W.4. When 3 PDs are provided with power 58.x~60.x W each (causing the total power consumption get 175+ W), 12PH PoE powering will become unstable - some PD may lose the power in several(3) minutes. |

**Compliance support:**

|  |  |
| --- | --- |
| **Compliance Level** | **Compliant** |
|  |  |

Known Anomalies: None.

**IEEE Standards Support:**

|  |  |
| --- | --- |
| **Standard** | **Title** |
| IEEE 802.1D | Transparent Bridging Specifications (ISO/IEC 10038) |
| IEEE 802.1p | Traffic Class Expediting and Dynamic Multicast Filtering |
| IEEE 802.1Q | Virtual Bridged Local Area Networks |
| IEEE 802.1w | Rapid Spanning Tree |
| IEEE 802.2  | Local Area Networks, Logical Link Control (LLC) |
| IEEE 802.3  | CSMA/CD 9 (ISO/IEC 8802-3) |
| IEEE 802.3I  | 10Base-T (ISO/IEC 8802-3, clause 14) |
| IEEE 802.3u  | 100Base-TX (ISO/IEC 8802-3, clause 25) |
| IEEE 802.3x | Flow Control |
| IEEE 802.3z | 1000Base-SX, 1000Base-LX |
| IEEE 802.3ab | 1000Base-TX |
| IEEE 802.3ac | VLAN Tag |
| IEEE 802.3ad | Link Aggregation |
| IEEE 802.1X | Port-based Network Access Control |

**IETF Standards MIB Support:**

|  |  |  |
| --- | --- | --- |
| **RFC No.** | Title | **Groups Supported** |
| 1907 | SNMPv2-MIB (MIB II) | - system group ( 1-9)- snmp group (1-6, 8-22, 24-32) |
| 2011 | IP-MIB (MIB-II) | - ip group (1-20, 22-23)- icmp group (1-26) |
| 2012 | TCP-MIB (MIB-II) | - tcp group (1-15)(tcpConnTable only support read.) |
| 2013 | UDP-MIB (MIB-II) | - udp group (1-5) |
| IEEE802.1X MIB | IEEE8021-PAE-MIB | - dot1xPaeSystem (1-2)- dot1xPaeAuthenticator (1-3)(not support per-port timer setting) |
| 1493 | Bridge MIB | - dot1dBase group (1-4)- dot1dStp group (1-15)- dot1dTp group (1-4)- dot1dStatic group (1) |
| 2863 | Interfaces Evolution MIB (IF-MIB) | - interface group (1-2) (ifadminStatus not support set to 3(testing))- ifXTable group (1)- ifStackTable group (1)(support read-only) |
| 2819 |  RMON MIB | - statistics group (1)- history group (1-2)- alarm group (1)- event group (1-2) |
| 2618 | RADIUS MIB | - radiusAuthClientMIB (1) |
| 2665 | Etherlike MIB | - dot3StatsTable group (1-19) |
| 2737 | Entity MIB | * entityPhysical group (1-16)

(support read-only) |
| 2674 | P-bridge | - dot1dExtBase group (1-4)- dot1dPriority group (1,3) - dot1dGarp group (1) |
| 2674 | Q-bridge | - dot1qBase group (1-5)- dot1qTp group (1-2)- dot1qStatic group(1)- dot1qVlan (1-5) (9-10) |
| V-Bridge MIB | V-Bridge MIB | - dot1vProtocol group |
| 3636 | MAU MIB | * dot3IfMauBasicGroup
* dot3IfMauAutoNegGroup
 |

|  |  |  |
| --- | --- | --- |
| 1612 | DNS Reslover MIB | * dnsServConfig
* dnsServCounter
* dnsServCounterAuthAns
* dnsServCounterAuthNoNames
* dnsServCounterAuthNoDataResps
* dnsServCounterNonAuthDatas
* dnsServCounterNonAuthNoDatas
* dnsServCounterReferrals
* dnsServCounterErrors
* dnsServCounterRelNames
* dnsServCounterReqRefusals
* dnsServCounterReqUnparses
* dnsServCounterOtherErrors
* dnsServOptCounter
* dnsResMIBObjects
* dnsResConfig
* dnsResCounter
* dnsResCache
* dnsResCacheStatus
* dnsResCacheMaxTTL
* dnsResCacheGoodCaches
* dnsResCacheBadCaches
* dnsResOptCounter
 |
| 3411 | SNMP FrameWork | * snmpFrameworkMIBObjects
 |
| 3412 | SNMP MPD MIB | * snmpMPDMIBObjects
 |
| 3413 | SNMP Target MIB | * snmpTargetObjects
 |
| 3413 | SNMP Notify MIB | * SnmpNotifyObjects
* snmpNotifyTable
* usmMIBObjects
 |
| 3415 | SNMP View-Based ACM MIB | * vacmMIBObjects
* Private MIB
* switchMgt
* portMgt
* trunkMgt
* lacpMgt
* staMgt
* tftpMgt
* restartMgt
* mirrorMgt
* igmpSnoopMgt
* ipMgt
* bcastStormMgt
* vlanMgt
* priorityMgt
* trapDestMgt
* qosMgt
* securityMgt
* sysLogMgt
* lineMgt
 |

**ECS4100 Private Enterprise MIB Support:**

|  |  |
| --- | --- |
| **Title** | Version |
| ECS4100-Series.mib | 201903080000Z |

**SNMP Trap Support:**

|  |  |
| --- | --- |
| **RFC No.** | **Title** |
| RFC 1215 | ColdStart (v1)warmStart (v1)linkDown (v1)linkUp (v1)authenticationFailure (v1) |
| RFC 1907 | coldStart (v2c)warmStart (v2c)authenticationFailure (v2c) |
| RFC 2863 | linkDown (v2c)linkUp (v2c) |
| RFC 1493 | newRoot (v1)topologyChange (v1) |
| RFC 1757 | risingAlarm (v1)fallingAlarm (v1) |
| RFC 2819 | risingAlarm (v2c)fallingAlarm (v2c) |

**CUSTOMER SUPPORT:**

By Phone:

By Email:

By Web:

 By Fax:

**Port LED Definitions:**

The following Port LED definitions are effective in Runtime V1.2.19.182 and higher.

|  |  |  |  |
| --- | --- | --- | --- |
| Mode\  Port LED  \Sku | Link/Act | PoE | Note |
| 1000 Mbps | 10/100 Mbps | Loopback-Detection |
| Copper | Fiber / Combo |
| ~~ECS4100-28T (12)~~ | ~~Green~~ | ~~Orange~~ | ~~Green<0.5>Orange~~ | ~~Green<0.5>Orange~~ | ~~NA~~ | ~~> Reset button - Yes(12)~~~~> LED - Bi-color~~ |
| ECS4100-28P (13,6) | Green | Orange | Green<0.5>Orange | Green<0.5>Orange | Orange | > Reset button - Yes(13), No(6)> LED - Bi-color |
| ECS4100-12T (14,9) | Green | Orange | Green<0.5>Orange | Green<0.5>Orange | NA | > Reset button - Yes(14), No(9)> LED - Bi-color |
| ECS4100-12PH (10) | Green | Orange | Green<0.5>Orange | Green<0.5>Orange | Orange | > Reset button - No> LED - Bi-color |
| ECS4100-52T (4) | Green | Orange | Green<0.5>Orange | Green<0.5>Orange | NA | > Reset button - No> LED - Bi-color |
| ECS4100-52P (8) | Green | Orange | Green<0.5>Orange | Green<0.5>Orange | Orange | > Reset button - No> LED - Bi-color |
| ECS4100-26TX (1,2) | Green | Orange | Green<0.5>Orange | Green<0.5>Orange | NA | > Reset button - No> LED - Bi-color |
| ECS4100-28TC (15,11) | Green | Orange | Green<0.5>Orange | Green<0.5>Orange | NA | > Reset button - Yes(15), No(11)> LED - Bi-color |
| ECS4100-28T (3) | Green | Green | Green | Green | NA | > Reset button - No> LED - Single-color |

PS1. The value(s) within parentheses are the associating Board ID(s).

PS2. The Port LED light of a looped port on loopback-detection only applies to the port-disabled mode (disabled port’s Tx/Rx traffic).

PS3. Green<0.5>Orange means for alternately Green/Orange flashing in 0.5sec period, say |<- Green,0.5s ->|<- Orange,0.5s ->|<- Green,0.5s ->|<- Orange,0.5s ->|...|<- Green,0.5s ->|<- Orange,0.5s ->|.

PS4. At PoE mode Port LED light will not be blinking - either solid (powering) or off (not powering).

PS5. For ECS4100-26TX (1,2), when 10G SFP Port 25/26 get to linkup at 10G speed, the Port LED is also lighting in Green (same as 1000M).

**Device Name v.s. 1st Firmware Version:**

Below given is the ECS4100 Device Name and the 1st Runtime Version, which is operational in that device.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Device | BID | 1st Runtime Ver | 1st Loader Ver | Note |
| 12Tv2 | 17 | 1.2.27.183 | 1.0.2.2 | 12T board relayout, ext.GPIO -> CPLD |
| 28TC-F | 16 | 1.2.26.182 | 1.0.2.0 |  |
| 28TC-ITUS | 15 | 1.2.19.182 | 1.0.1.8 |  |
| 12T-ITUS | 14 | 1.2.16.181 | 1.0.1.7 |  |
| 28P-ITUS | 13 | 1.2.16.181 | 1.0.1.6 |  |
| 28T-ITUS | 12 | 1.2.16.181 | 1.0.1.6 | Replaced with 28TC-ITUS |
| 28TC | 11 | 1.2.16.181 | 1.0.1.6 |  |
| 12PH | 10 | 1.2.13.174 | 1.0.1.1 |  |
| 12T | 9 | 1.2.2.172 | 1.0.1.1 |  |
| 52P | 8 | 1.2.2.172 | 1.0.1.1 |  |
| 52T | 7 | NA |  | Deposed |
| 28P | 6 | 1.2.2.172 | 1.0.1.1 |  |
| 28T | 5 | NA |  | Deposed |
| 52T | 4 | 1.1.8.164 | 1.0.0.5 |  |
| 28T | 3 | 1.1.8.164 | 1.0.0.5 |  |
| 26TX-ME | 2 | 1.1.8.164 | 1.0.0.5 |  |
| 26TX | 1 | 1.1.8.164 | 1.0.0.5 |  |
| 52T | 0 | 1.1.8.164 | 1.0.0.5 |  |